LCOV - code coverage report
Current view: | top level - physics/cam - wv_sat_methods.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 103 | 169 | 60.9 %
Date: | 2024-12-17 17:57:11 |  | Functions: | 18 | 28 | 64.3 %

Function Name | Hit count
__wv_sat_methods_MOD_bolton_svp_water | 0
__wv_sat_methods_MOD_bolton_svp_water_vect | 0
__wv_sat_methods_MOD_goffgratch_svp_ice | 4650767015
__wv_sat_methods_MOD_goffgratch_svp_ice_vect | 384207408
__wv_sat_methods_MOD_goffgratch_svp_water | 33670967524
__wv_sat_methods_MOD_goffgratch_svp_water_vect | 1143687168
__wv_sat_methods_MOD_murphykoop_svp_ice | 0
__wv_sat_methods_MOD_murphykoop_svp_ice_vect | 0
__wv_sat_methods_MOD_murphykoop_svp_water | 0
__wv_sat_methods_MOD_murphykoop_svp_water_vect | 0
__wv_sat_methods_MOD_wv_sat_get_scheme_idx | 1536
__wv_sat_methods_MOD_wv_sat_methods_init | 1536
__wv_sat_methods_MOD_wv_sat_qsat_ice | 0
__wv_sat_methods_MOD_wv_sat_qsat_ice_vect | 8935056
__wv_sat_methods_MOD_wv_sat_qsat_trans | 0
__wv_sat_methods_MOD_wv_sat_qsat_water | 29020232765
__wv_sat_methods_MOD_wv_sat_qsat_water_vect | 768414816
__wv_sat_methods_MOD_wv_sat_reset_default | 0
__wv_sat_methods_MOD_wv_sat_set_default | 1536
__wv_sat_methods_MOD_wv_sat_svp_ice | 4650767015
__wv_sat_methods_MOD_wv_sat_svp_ice_vect | 384207408
__wv_sat_methods_MOD_wv_sat_svp_to_qsat | 29532646494
__wv_sat_methods_MOD_wv_sat_svp_to_qsat_vect | 1195182936
__wv_sat_methods_MOD_wv_sat_svp_trans | 385536
__wv_sat_methods_MOD_wv_sat_svp_trans_vect | 0
__wv_sat_methods_MOD_wv_sat_svp_water | 33670967524
__wv_sat_methods_MOD_wv_sat_svp_water_vect | 1143687168
__wv_sat_methods_MOD_wv_sat_valid_idx | 1536

Generated by: LCOV version 1.14