LCOV - code coverage report
Current view: | top level - physics/cam - radiation_data.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 38 | 576 | 6.6 %
Date: | 2024-12-17 17:57:11 |  | Functions: | 4 | 11 | 36.4 %

              Line data    Source code
           1             : !================================================================================================
           2             : ! output/input data necessary to drive radiation offline
           3             : ! Francis Vitt -- Created 15 Dec 2009
           4             : !================================================================================================
           5             : module radiation_data
           6             :
           7             :   use shr_kind_mod,     only: r8=>shr_kind_r8
           8             :   use ppgrid,           only : pcols, pver, pverp, begchunk, endchunk
           9             :   use cam_history,      only: addfld, add_default, horiz_only, outfld
          10             :   use rad_constituents, only: rad_cnst_get_info, rad_cnst_get_gas, rad_cnst_get_aer_mmr
          11             :   use radconstants,     only: nradgas, gaslist
          12             :   use cam_history_support, only: fieldname_len, fillvalue
          13             :   use spmd_utils,       only: masterproc
          14             :   use cam_abortutils,   only: endrun
          15             :
          16             :   use drv_input_data,only: drv_input_data_t
          17             :   use drv_input_data,only: drv_input_data_get, drv_input_2d_t, drv_input_3d_t, drv_input_4d_t, drv_input_2di_t
          18             :   use physics_types, only: physics_state
          19             :   use physics_buffer,only: physics_buffer_desc, pbuf_get_chunk
          20             :
          21             :   implicit none
          22             :   private
          23             :
          24             :   public :: rad_data_readnl
          25             :   public :: rad_data_register
          26             :   public :: rad_data_init
          27             :   public :: rad_data_write
          28             :   public :: rad_data_read
          29             :   public :: rad_data_enable
          30             :
          31             :   integer :: volcgeom_ifld, volcgeom1_ifld, volcgeom2_ifld, volcgeom3_ifld
          32             :   integer :: cld_ifld,rel_ifld,rei_ifld
          33             :   integer :: dei_ifld,mu_ifld,lambdac_ifld,iciwp_ifld,iclwp_ifld
          34             :   integer :: des_ifld,icswp_ifld,cldfsnow_ifld
          35             :   integer :: cldemis_ifld, cldtau_ifld, cicewp_ifld, cliqwp_ifld, nmxrgn_ifld, pmxrgn_ifld
          36             :   integer :: qrs_ifld, qrl_ifld
          37             :   integer :: dgnumwet_ifld, qaerwat_ifld
          38             :
          39             :   character(len=fieldname_len), parameter :: &
          40             :        lndfrc_fldn    = 'rad_lndfrc      ' , &
          41             :        icefrc_fldn    = 'rad_icefrc      ' , &
          42             :        snowh_fldn     = 'rad_snowh       ' , &
          43             :        asdir_fldn     = 'rad_asdir       ' , &
          44             :        asdif_fldn     = 'rad_asdif       ' , &
          45             :        aldir_fldn     = 'rad_aldir       ' , &
          46             :        aldif_fldn     = 'rad_aldif       ' , &
          47             :        coszen_fldn    = 'rad_coszen      ' , &
          48             :        asdir_pos_fldn = 'rad_asdir_pos   ' , &
          49             :        asdif_pos_fldn = 'rad_asdif_pos   ' , &
          50             :        aldir_pos_fldn = 'rad_aldir_pos   ' , &
          51             :        aldif_pos_fldn = 'rad_aldif_pos   ' , &
          52             :        lwup_fldn      = 'rad_lwup        ' , &
          53             :        ts_fldn        = 'rad_ts          ' , &
          54             :        temp_fldn      = 'rad_temp        ' , &
          55             :        pdel_fldn      = 'rad_pdel        ' , &
          56             :        pdeldry_fldn   = 'rad_pdeldry     ' , &
          57             :        pmid_fldn      = 'rad_pmid        ' , &
          58             :        watice_fldn    = 'rad_watice      ' , &
          59             :        watliq_fldn    = 'rad_watliq      ' , &
          60             :        watvap_fldn    = 'rad_watvap      ' , &
          61             :        zint_fldn      = 'rad_zint        ' , &
          62             :        pint_fldn      = 'rad_pint        ' , &
          63             :        cld_fldn       = 'rad_cld         ' , &
          64             :        cldemis_fldn   = 'rad_cldemis     ' , &
          65             :        cldtau_fldn    = 'rad_cldtau      ' , &
          66             :        cicewp_fldn    = 'rad_cicewp      ' , &
          67             :        cliqwp_fldn    = 'rad_cliqwp      ' , &
          68             :        nmxrgn_fldn    = 'rad_nmxrgn      ' , &
          69             :        pmxrgn_fldn    = 'rad_pmxrgn      ' , &
          70             :        cldfsnow_fldn  = 'rad_cldfsnow    ' , &
          71             :        rel_fldn       = 'rad_rel         ' , &
          72             :        rei_fldn       = 'rad_rei         ' , &
          73             :        dei_fldn       = 'rad_dei         ' , &
          74             :        des_fldn       = 'rad_des         ' , &
          75             :        mu_fldn        = 'rad_mu          ' , &
          76             :        lambdac_fldn   = 'rad_lambdac     ' , &
          77             :        iciwp_fldn     = 'rad_iciwp       ' , &
          78             :        iclwp_fldn     = 'rad_iclwp       ' , &
          79             :        icswp_fldn     = 'rad_icswp       ' , &
          80             :        qrs_fldn       = 'rad_qrs         ' , &
          81             :        qrl_fldn       = 'rad_qrl         ' , &
          82             :        volcgeom_fldn  = 'rad_volc_geom   ' , &
          83             :        volcgeom1_fldn = 'rad_volc_geom1  ' , &
          84             :        volcgeom2_fldn = 'rad_volc_geom2  ' , &
          85             :        volcgeom3_fldn = 'rad_volc_geom3  '
          86             :
          87             :   ! for modal aerosols
          88             :   character(len=fieldname_len), allocatable :: dgnumwet_fldn(:)
          89             :   character(len=fieldname_len), allocatable :: qaerwat_fldn(:)
          90             :   integer :: nmodes=0
          91             :
          92             :   ! rad constituents mixing ratios
          93             :   integer :: ngas, naer=0
          94             :   character(len=64), allocatable :: gasnames(:)
          95             :   character(len=64), allocatable :: aernames(:)
          96             :
          97             :   ! control options
          98             :   logical          :: rad_data_output = .false.
          99             :   integer          :: rad_data_histfile_num = 2
         100             :   character(len=1) :: rad_data_avgflag = 'I'
         101             :
         102             :   ! MG microphys check
         103             :   logical :: mg_microphys
         104             :
         105             :   logical :: fixed_dyn_heating = .false.
         106             :
         107             :   ! for fixed dynamical heating ...
         108             :   logical :: do_fdh = .false.
         109             :
         110             :   integer :: tcorr_idx = -1
         111             :   integer :: qrsin_idx = -1
         112             :   integer :: qrlin_idx = -1
         113             :   integer :: tropp_idx = -1
         114             :
         115             :   logical :: enabled = .false.
         116             :   logical :: gmean_3modes = .false.
         117             :
         118             : contains
         119             :
         120             :
         121             : !================================================================================================
         122             : !================================================================================================
         123        1536 :   subroutine rad_data_register
         124             :     use physics_buffer,  only: pbuf_add_field, dtype_r8
         125             :
         126        1536 :     if ( do_fdh ) then
         127           0 :       call pbuf_add_field('tcorr', 'global',  dtype_r8, (/pcols,pver/), tcorr_idx)
         128           0 :       call pbuf_add_field('qrsin', 'physpkg', dtype_r8, (/pcols,pver/), qrsin_idx)
         129           0 :       call pbuf_add_field('qrlin', 'physpkg', dtype_r8, (/pcols,pver/), qrlin_idx)
         130           0 :       call pbuf_add_field('tropp', 'physpkg', dtype_r8, (/pcols/),      tropp_idx)
         131             :     end if
         132             :
         133        1536 :   end subroutine rad_data_register
         134             :
         135             : !================================================================================================
         136             : !================================================================================================
         137        1536 :   subroutine rad_data_readnl(nlfile)
         138             :
         139             :     ! Read rad_data_nl namelist group.  Parse input.
         140             :
         141        1536 :     use namelist_utils,  only: find_group_name
         142             :     use units,           only: getunit, freeunit
         143             :     use mpishorthand
         144             :
         145             :     character(len=*), intent(in) :: nlfile  ! filepath for file containing namelist input
         146             :     logical :: rad_data_fdh = .false.
         147             :
         148             :     ! Local variables
         149             :     integer :: unitn, ierr, i
         150             :     character(len=*), parameter :: subname = 'rad_data_readnl'
         151             :
         152             :     namelist /rad_data_nl/ rad_data_output, rad_data_histfile_num, rad_data_avgflag, rad_data_fdh
         153             :
         154             :     !-----------------------------------------------------------------------------
         155             :
         156        1536 :     if (masterproc) then
         157           2 :        unitn = getunit()
         158           2 :        open( unitn, file=trim(nlfile), status='old' )
         159           2 :        call find_group_name(unitn, 'rad_data_nl', status=ierr)
         160           2 :        if (ierr == 0) then
         161           0 :           read(unitn, rad_data_nl, iostat=ierr)
         162           0 :           if (ierr /= 0) then
         163           0 :              call endrun(subname // ':: ERROR reading namelist')
         164             :           end if
         165             :        end if
         166           2 :        close(unitn)
         167           2 :        call freeunit(unitn)
         168             :     end if
         169             :
         170             : #ifdef SPMD
         171             :     ! Broadcast namelist variables
         172        1536 :     call mpibcast (rad_data_output,       1,   mpilog ,  0, mpicom)
         173        1536 :     call mpibcast (rad_data_fdh,          1,   mpilog ,  0, mpicom)
         174        1536 :     call mpibcast (rad_data_histfile_num, 1,   mpiint ,  0, mpicom)
         175        1536 :     call mpibcast (rad_data_avgflag,      1,   mpichar , 0, mpicom)
         176             : #endif
         177        1536 :     do_fdh = rad_data_fdh
         178        1536 :     enabled = rad_data_output
         179             :
         180        1536 :   end subroutine rad_data_readnl
         181             :
         182             :   !================================================================================================
         183             :   !================================================================================================
         184           0 :   subroutine rad_data_enable()
         185           0 :     enabled = .true.
         186           0 :   end subroutine rad_data_enable
         187             :
         188             :   !================================================================================================
         189             :   !================================================================================================
         190        1536 :   subroutine rad_data_init( pbuf2d )
         191             :     use phys_control,     only: phys_getopts
         192             :     use physics_buffer, only: pbuf_get_index
         193             :     use physics_buffer, only: pbuf_set_field
         194             :     implicit none
         195             :
         196             :     ! args
         197             :     type(physics_buffer_desc), pointer :: pbuf2d(:,:)
         198             :
         199             :     ! local vars
         200             :     integer :: i, err
         201             :     integer :: m,l, nspec
         202             :     character(len=64) :: name
         203             :     character(len=32) :: aername =  ' '
         204             :     character(len=128):: long_name
         205             :     character(len=64) :: long_name_description
         206             :     character(len=16)  :: microp_scheme  ! microphysics scheme
         207             :     character(len=16)  :: rad_scheme
         208             :
         209        1536 :     if (.not.enabled) return
         210             :
         211           0 :     call phys_getopts(microp_scheme_out=microp_scheme, radiation_scheme_out=rad_scheme)
         212           0 :     mg_microphys =  (trim(microp_scheme) == 'MG')
         213             :
         214           0 :     volcgeom_ifld = pbuf_get_index('VOLC_RAD_GEOM',errcode=err) ! might need 3 more for 3-mode inputs
         215           0 :     volcgeom1_ifld = pbuf_get_index('VOLC_RAD_GEOM1',errcode=err) ! might need 3 more for 3-mode inputs
         216           0 :     volcgeom2_ifld = pbuf_get_index('VOLC_RAD_GEOM2',errcode=err) ! might need 3 more for 3-mode inputs
         217           0 :     volcgeom3_ifld = pbuf_get_index('VOLC_RAD_GEOM3',errcode=err) ! might need 3 more for 3-mode inputs
         218             :
         219           0 :     gmean_3modes = volcgeom1_ifld > 0 .and. volcgeom2_ifld > 0 .and. volcgeom3_ifld > 0 .and. volcgeom_ifld < 1
         220             :
         221           0 :     if (volcgeom_ifld > 0) then
         222           0 :        call addfld(volcgeom_fldn, (/ 'lev' /), 'I','m', 'combined volcanic aerosol geometric-mode radius' )
         223             :     endif
         224           0 :     if (gmean_3modes) then
         225           0 :        call addfld(volcgeom1_fldn, (/ 'lev' /), 'I','m', 'mode 1 volcanic aerosol geometric-mode radius' )
         226           0 :        call addfld(volcgeom2_fldn, (/ 'lev' /), 'I','m', 'mode 2 volcanic aerosol geometric-mode radius' )
         227           0 :        call addfld(volcgeom3_fldn, (/ 'lev' /), 'I','m', 'mode 3 volcanic aerosol geometric-mode radius' )
         228             :     endif
         229             :
         230           0 :     cld_ifld    = pbuf_get_index('CLD')
         231           0 :     rel_ifld    = pbuf_get_index('REL')
         232           0 :     rei_ifld    = pbuf_get_index('REI')
         233           0 :     qrs_ifld    = pbuf_get_index('QRS')
         234           0 :     qrl_ifld    = pbuf_get_index('QRL')
         235           0 :     if (mg_microphys) then
         236           0 :        dei_ifld      = pbuf_get_index('DEI')
         237           0 :        des_ifld      = pbuf_get_index('DES')
         238           0 :        mu_ifld       = pbuf_get_index('MU')
         239           0 :        lambdac_ifld  = pbuf_get_index('LAMBDAC')
         240           0 :        iciwp_ifld    = pbuf_get_index('ICIWP')
         241           0 :        iclwp_ifld    = pbuf_get_index('ICLWP')
         242           0 :        icswp_ifld    = pbuf_get_index('ICSWP')
         243           0 :        cldfsnow_ifld = pbuf_get_index('CLDFSNOW')
         244             :     else
         245           0 :        cldemis_ifld= pbuf_get_index('CLDEMIS')
         246           0 :        cldtau_ifld = pbuf_get_index('CLDTAU')
         247           0 :        cicewp_ifld = pbuf_get_index('CICEWP')
         248           0 :        cliqwp_ifld = pbuf_get_index('CLIQWP')
         249           0 :        nmxrgn_ifld = pbuf_get_index('NMXRGN')
         250           0 :        pmxrgn_ifld = pbuf_get_index('PMXRGN')
         251             :     endif
         252             :
         253           0 :     if ( do_fdh ) then
         254           0 :        call addfld('rad_TROP_P', horiz_only,  'A','Pa','Pressure at which tropopause is defined for radiation' )
         255           0 :        call addfld('rad_TCORR',  (/ 'lev' /), 'I','K', 'Fixed dynamical heating temperature correction ' )
         256           0 :        call pbuf_set_field(pbuf2d, tcorr_idx, 0.0_r8)
         257           0 :        call pbuf_set_field(pbuf2d, qrsin_idx, 0.0_r8)
         258           0 :        call pbuf_set_field(pbuf2d, qrlin_idx, 0.0_r8)
         259           0 :        call pbuf_set_field(pbuf2d, tropp_idx, -1.0_r8)
         260             :     endif
         261             :
         262           0 :     call rad_cnst_get_info(0, ngas=ngas, naero=naer, nmodes=nmodes)
         263             :
         264             :     ! The code to output the gases assumes that the rad_constituents module has
         265             :     ! ordered them in the same way that they are ordered in the "gaslist" array
         266             :     ! in module radconstants, and that there are nradgas of them.  This ordering
         267             :     ! is performed in the internal init_lists routine in rad_constituents.
         268           0 :     if (ngas /= nradgas) then
         269           0 :        call endrun('rad_data_init: ERROR: ngas /= nradgas')
         270             :     end if
         271             :
         272           0 :     allocate( gasnames(ngas) )
         273           0 :     call rad_cnst_get_info(0, gasnames=gasnames)
         274             :
         275           0 :     if (naer > 0) then
         276           0 :        allocate( aernames(naer) )
         277           0 :        call rad_cnst_get_info(0, aernames=aernames)
         278             :     endif
         279             :
         280           0 :     if (nmodes>0) then
         281           0 :        allocate(dgnumwet_fldn(nmodes),qaerwat_fldn(nmodes))
         282           0 :        dgnumwet_ifld = pbuf_get_index('DGNUMWET')
         283           0 :        qaerwat_ifld  = pbuf_get_index('QAERWAT')
         284           0 :        do m = 1, nmodes
         285           0 :           write(dgnumwet_fldn(m), 1001 ) m
         286           0 :           write(qaerwat_fldn(m), 1003 ) m
         287             :        enddo
         288             :     endif
         289             :
         290           0 :     if (.not.rad_data_output) return
         291             :
         292             :     call addfld (lndfrc_fldn,    horiz_only,   rad_data_avgflag, 'fraction', &
         293           0 :          'radiation input: land fraction')
         294             :     call addfld (icefrc_fldn,    horiz_only,   rad_data_avgflag, 'fraction', &
         295           0 :          'radiation input: ice fraction')
         296             :     call addfld (snowh_fldn,     horiz_only,   rad_data_avgflag, 'm',        &
         297           0 :          'radiation input: water equivalent snow depth')
         298             :     call addfld (asdir_fldn,     horiz_only,   rad_data_avgflag, '1',        &
         299           0 :          'radiation input: s     hort wave direct albedo',                    flag_xyfill=.true.)
         300             :     call addfld (asdif_fldn,     horiz_only,   rad_data_avgflag, '1',        &
         301           0 :          'radiation input: s     hort wave difuse albedo',                    flag_xyfill=.true.)
         302             :     call addfld (aldir_fldn,     horiz_only,   rad_data_avgflag, '1',        &
         303           0 :          'radiation input: long wave direct albedo',                          flag_xyfill=.true.)
         304             :     call addfld (aldif_fldn,     horiz_only,   rad_data_avgflag, '1',        &
         305           0 :          'radiation input: long wave difuse albedo',                          flag_xyfill=.true.)
         306             :
         307             :     call addfld (coszen_fldn,    horiz_only,   rad_data_avgflag, '1',        &
         308           0 :          'radiation input: cosine solar zenith when positive',                flag_xyfill=.true.)
         309             :     call addfld (asdir_pos_fldn, horiz_only,   rad_data_avgflag, '1',        &
         310           0 :          'radiation input: s     hort wave direct albedo weighted by coszen', flag_xyfill=.true.)
         311             :     call addfld (asdif_pos_fldn, horiz_only,   rad_data_avgflag, '1',        &
         312           0 :          'radiation input: s     hort wave difuse albedo weighted by coszen', flag_xyfill=.true.)
         313             :     call addfld (aldir_pos_fldn, horiz_only,   rad_data_avgflag, '1',        &
         314           0 :          'radiation input: long wave direct albedo weighted by coszen',       flag_xyfill=.true.)
         315             :     call addfld (aldif_pos_fldn, horiz_only,   rad_data_avgflag, '1',        &
         316           0 :          'radiation input: long wave difuse albedo weighted by coszen',       flag_xyfill=.true.)
         317             :
         318             :     call addfld (lwup_fldn,      horiz_only,   rad_data_avgflag, 'W/m2',     &
         319           0 :          'radiation input: long wave up radiation flux ')
         320             :     call addfld (ts_fldn,        horiz_only,   rad_data_avgflag, 'K',        &
         321           0 :          'radiation input: surface temperature')
         322             :
         323             :     call addfld (temp_fldn,      (/ 'lev' /),  rad_data_avgflag, 'K',        &
         324           0 :          'radiation input: midpoint temperature')
         325             :     call addfld (pdel_fldn,      (/ 'lev' /),  rad_data_avgflag, 'Pa',       &
         326           0 :          'radiation input: pressure layer thickness')
         327             :     call addfld (pdeldry_fldn,   (/ 'lev' /),  rad_data_avgflag,'Pa',        &
         328           0 :          'radiation input: dry pressure layer thickness')
         329             :     call addfld (pmid_fldn,      (/ 'lev' /),  rad_data_avgflag, 'Pa',       &
         330           0 :          'radiation input: midpoint pressure')
         331             :     call addfld (watice_fldn,    (/ 'lev' /),  rad_data_avgflag, 'kg/kg',    &
         332           0 :          'radiation input: cloud ice')
         333             :     call addfld (watliq_fldn,    (/ 'lev' /),  rad_data_avgflag, 'kg/kg',    &
         334           0 :          'radiation input: cloud liquid water')
         335             :     call addfld (watvap_fldn,    (/ 'lev' /),  rad_data_avgflag, 'kg/kg',    &
         336           0 :          'radiation input: water vapor')
         337             :
         338             :     call addfld (zint_fldn,      (/ 'ilev' /), rad_data_avgflag, 'km',       &
         339           0 :          'radiation input: interface height')
         340             :     call addfld (pint_fldn,      (/ 'ilev' /), rad_data_avgflag, 'Pa',       &
         341           0 :          'radiation input: interface pressure')
         342             :
         343             :     call addfld (cld_fldn,       (/ 'lev' /),  rad_data_avgflag, 'fraction', &
         344           0 :          'radiation input: cloud fraction')
         345             :     call addfld (rel_fldn,       (/ 'lev' /),  rad_data_avgflag, 'micron',   &
         346           0 :          'radiation input: effective liquid drop radius')
         347             :     call addfld (rei_fldn,       (/ 'lev' /),  rad_data_avgflag, 'micron',   &
         348           0 :          'radiation input: effective ice partical radius')
         349             :     call addfld (qrs_fldn,       (/ 'lev' /),  rad_data_avgflag, 'J/s/kg',   &
         350           0 :          'radiation input: solar heating rate')
         351             :     call addfld (qrl_fldn,       (/ 'lev' /),  rad_data_avgflag, 'J/s/kg',   &
         352           0 :          'radiation input: longwave heating rate')
         353             :
         354           0 :     if (mg_microphys) then
         355             :        call addfld (dei_fldn,      (/ 'lev' /), rad_data_avgflag, 'micron',   &
         356           0 :             'radiation input: effective ice partical diameter')
         357             :        call addfld (des_fldn,      (/ 'lev' /), rad_data_avgflag, 'micron',   &
         358           0 :             'radiation input: effective snow partical diameter')
         359             :        call addfld (mu_fldn,       (/ 'lev' /), rad_data_avgflag, ' ',        &
         360           0 :             'radiation input: ice gamma parameter for optics (radiation)')
         361             :        call addfld (lambdac_fldn,  (/ 'lev' /), rad_data_avgflag,' ',         &
         362           0 :             'radiation input: slope of droplet distribution for optics (radiation)')
         363             :        call addfld (iciwp_fldn,    (/ 'lev' /), rad_data_avgflag, 'kg/m2',    &
         364           0 :             'radiation input: In-cloud ice water path')
         365             :        call addfld (iclwp_fldn,    (/ 'lev' /), rad_data_avgflag, 'kg/m2',    &
         366           0 :             'radiation input: In-cloud liquid water path')
         367             :        call addfld (icswp_fldn,    (/ 'lev' /), rad_data_avgflag, 'kg/m2',    &
         368           0 :             'radiation input: In-cloud snow water path')
         369             :        call addfld (cldfsnow_fldn, (/ 'lev' /), rad_data_avgflag, 'fraction', &
         370           0 :             'radiation input: cloud liquid drops + snow')
         371             :     else
         372             :
         373             :       call addfld (nmxrgn_fldn,    horiz_only,   rad_data_avgflag, ' ',       &
         374           0 :          'radiation input: ')
         375             :       call addfld (pmxrgn_fldn,    (/ 'ilev' /), rad_data_avgflag, 'Pa',      &
         376           0 :          'radiation input: ')
         377             :       call addfld (cldemis_fldn,   (/ 'lev' /), rad_data_avgflag, ' ',        &
         378           0 :          'radiation input: cloud property ')
         379             :       call addfld (cldtau_fldn,    (/ 'lev' /), rad_data_avgflag, ' ',        &
         380           0 :          'radiation input: cloud property ')
         381             :       call addfld (cicewp_fldn,    (/ 'lev' /), rad_data_avgflag, ' ',        &
         382           0 :          'radiation input: cloud property ')
         383             :       call addfld (cliqwp_fldn,    (/ 'lev' /), rad_data_avgflag, ' ',        &
         384           0 :          'radiation input: cloud property ')
         385             :     endif
         386             :
         387           0 :     call add_default (lndfrc_fldn,    rad_data_histfile_num, ' ')
         388           0 :     call add_default (icefrc_fldn,    rad_data_histfile_num, ' ')
         389           0 :     call add_default (snowh_fldn,     rad_data_histfile_num, ' ')
         390           0 :     call add_default (asdir_fldn,     rad_data_histfile_num, ' ')
         391           0 :     call add_default (asdif_fldn,     rad_data_histfile_num, ' ')
         392           0 :     call add_default (aldir_fldn,     rad_data_histfile_num, ' ')
         393           0 :     call add_default (aldif_fldn,     rad_data_histfile_num, ' ')
         394             :
         395           0 :     call add_default (coszen_fldn,    rad_data_histfile_num, ' ')
         396           0 :     call add_default (asdir_pos_fldn, rad_data_histfile_num, ' ')
         397           0 :     call add_default (asdif_pos_fldn, rad_data_histfile_num, ' ')
         398           0 :     call add_default (aldir_pos_fldn, rad_data_histfile_num, ' ')
         399           0 :     call add_default (aldif_pos_fldn, rad_data_histfile_num, ' ')
         400             :
         401           0 :     call add_default (lwup_fldn,      rad_data_histfile_num, ' ')
         402           0 :     call add_default (ts_fldn,        rad_data_histfile_num, ' ')
         403           0 :     call add_default (temp_fldn,      rad_data_histfile_num, ' ')
         404           0 :     call add_default (pdel_fldn,      rad_data_histfile_num, ' ')
         405           0 :     call add_default (pdeldry_fldn,   rad_data_histfile_num, ' ')
         406           0 :     call add_default (pmid_fldn,      rad_data_histfile_num, ' ')
         407           0 :     call add_default (watice_fldn,    rad_data_histfile_num, ' ')
         408           0 :     call add_default (watliq_fldn,    rad_data_histfile_num, ' ')
         409           0 :     call add_default (watvap_fldn,    rad_data_histfile_num, ' ')
         410           0 :     call add_default (zint_fldn,      rad_data_histfile_num, ' ')
         411           0 :     call add_default (pint_fldn,      rad_data_histfile_num, ' ')
         412             :
         413           0 :     call add_default (cld_fldn,       rad_data_histfile_num, ' ')
         414           0 :     call add_default (rel_fldn,       rad_data_histfile_num, ' ')
         415           0 :     call add_default (rei_fldn,       rad_data_histfile_num, ' ')
         416           0 :     call add_default (qrs_fldn,       rad_data_histfile_num, ' ')
         417           0 :     call add_default (qrl_fldn,       rad_data_histfile_num, ' ')
         418             :
         419           0 :     if (mg_microphys) then
         420           0 :        call add_default (dei_fldn,       rad_data_histfile_num, ' ')
         421           0 :        call add_default (des_fldn,       rad_data_histfile_num, ' ')
         422           0 :        call add_default (mu_fldn,        rad_data_histfile_num, ' ')
         423           0 :        call add_default (lambdac_fldn,   rad_data_histfile_num, ' ')
         424           0 :        call add_default (iciwp_fldn,     rad_data_histfile_num, ' ')
         425           0 :        call add_default (iclwp_fldn,     rad_data_histfile_num, ' ')
         426           0 :        call add_default (icswp_fldn,     rad_data_histfile_num, ' ')
         427           0 :        call add_default (cldfsnow_fldn,  rad_data_histfile_num, ' ')
         428             :     else
         429           0 :        call add_default (cldemis_fldn,   rad_data_histfile_num, ' ')
         430           0 :        call add_default (cldtau_fldn,    rad_data_histfile_num, ' ')
         431           0 :        call add_default (cicewp_fldn,    rad_data_histfile_num, ' ')
         432           0 :        call add_default (cliqwp_fldn,    rad_data_histfile_num, ' ')
         433           0 :        call add_default (nmxrgn_fldn,    rad_data_histfile_num, ' ')
         434           0 :        call add_default (pmxrgn_fldn,    rad_data_histfile_num, ' ')
         435             :     endif
         436             :
         437             :     ! stratospheric aersols geometric mean radius
         438           0 :     if (volcgeom_ifld > 0) then
         439           0 :        call add_default (volcgeom_fldn, rad_data_histfile_num, ' ')
         440             :     endif
         441           0 :     if (gmean_3modes) then
         442           0 :        call add_default (volcgeom1_fldn, rad_data_histfile_num, ' ')
         443           0 :        call add_default (volcgeom2_fldn, rad_data_histfile_num, ' ')
         444           0 :        call add_default (volcgeom3_fldn, rad_data_histfile_num, ' ')
         445             :     endif
         446             :
         447             :     ! rad constituents
         448             :
         449           0 :     long_name_description = ' mass mixing ratio used in rad climate calculation'
         450             :
         451           0 :     do i = 1, ngas
         452           0 :        long_name = trim(gasnames(i))//trim(long_name_description)
         453           0 :        name = 'rad_'//gasnames(i)
         454           0 :        call addfld(trim(name), (/ 'lev' /), rad_data_avgflag, 'kg/kg', trim(long_name))
         455           0 :        call add_default (trim(name), rad_data_histfile_num, ' ')
         456             :     end do
         457             :
         458           0 :     if (naer > 0) then
         459             :
         460           0 :        do i = 1, naer
         461           0 :           long_name = trim(aernames(i))//trim(long_name_description)
         462           0 :           name = 'rad_'//aernames(i)
         463           0 :           call addfld(trim(name), (/ 'lev' /), rad_data_avgflag, 'kg/kg', trim(long_name))
         464           0 :           call add_default (trim(name), rad_data_histfile_num, ' ')
         465             :        end do
         466             :     endif
         467           0 :     if (nmodes>0) then
         468             :
         469             :        ! for modal aerosol model
         470           0 :        do m = 1, nmodes
         471           0 :           write(long_name, 1002) m
         472           0 :           call addfld ( dgnumwet_fldn(m), (/ 'lev' /), rad_data_avgflag, '', trim(long_name) )
         473           0 :           call add_default (dgnumwet_fldn(m), rad_data_histfile_num, ' ')
         474             :
         475           0 :           write(long_name, 1004) m
         476           0 :           call addfld ( qaerwat_fldn(m),  (/ 'lev' /), rad_data_avgflag, '', trim(long_name) )
         477           0 :           call add_default (qaerwat_fldn(m), rad_data_histfile_num, ' ')
         478             :
         479             :           ! get mode info
         480           0 :           call rad_cnst_get_info(0, m, nspec=nspec)
         481             :           ! aerosol species loop
         482           0 :           do l = 1, nspec
         483           0 :              call rad_cnst_get_info(0,m,l, spec_name=aername)
         484           0 :              name = 'rad_'//trim(aername)
         485           0 :              call addfld(trim(name),      (/ 'lev' /), rad_data_avgflag, 'kg/kg', trim(long_name))
         486           0 :              call add_default (trim(name), rad_data_histfile_num, ' ')
         487             :           end do
         488             :        end do
         489             :     endif
         490             :
         491             :  1001 format ( 'rad_dgnumwet_', I1 )
         492             :  1002 format ( 'radiation input: DGNUMWET for mode ', I1 )
         493             :  1003 format ( 'rad_qaerwat_', I1 )
         494             :  1004 format ( 'radiation input: QAERWAT for mode ', I1 )
         495             :
         496        1536 :   end subroutine rad_data_init
         497             :
         498             :   !================================================================================================
         499             :   !================================================================================================
         500     1492272 :   subroutine rad_data_write(  pbuf, state, cam_in, coszen )
         501             :
         502        1536 :     use physics_types,    only: physics_state
         503             :     use camsrfexch,       only: cam_in_t
         504             :     use constituents,     only: cnst_get_ind
         505             :     use physics_buffer,   only: pbuf_get_field, pbuf_old_tim_idx
         506             :     use drv_input_data,   only: drv_input_data_freq
         507             :     use physconst,        only: cpair
         508             :
         509             :     implicit none
         510             :     type(physics_buffer_desc), pointer :: pbuf(:)
         511             :
         512             :     type(physics_state), intent(in), target :: state
         513             :     type(cam_in_t),      intent(in) :: cam_in
         514             :     real(r8),            intent(in) :: coszen(pcols)
         515             :
         516             :     ! Local variables
         517             :     integer :: i, k
         518             :     integer :: m,l, nspec
         519             :     character(len=32) :: name, aername
         520     1492272 :     real(r8), pointer :: mmr(:,:)
         521             :
         522             :     integer :: lchnk, itim_old, ifld
         523             :     integer :: ixcldice              ! cloud ice water index
         524             :     integer :: ixcldliq              ! cloud liquid water index
         525             :     integer :: icol
         526             :     integer :: ncol
         527             :
         528             :     ! surface albedoes weighted by (positive cosine zenith angle)
         529             :     real(r8):: coszrs_pos(pcols)    ! = max(coszrs,0)
         530             :     real(r8):: asdir_pos (pcols)    !
         531             :     real(r8):: asdif_pos (pcols)    !
         532             :     real(r8):: aldir_pos (pcols)    !
         533             :     real(r8):: aldif_pos (pcols)    !
         534             :
         535     1492272 :     real(r8), pointer, dimension(:,:)  :: ptr
         536     1492272 :     integer , pointer, dimension(:)    :: iptr1d
         537             :     real(r8),          dimension(pcols) :: rptr1d
         538             :
         539             :     ! for Fixed Dynamical Heating
         540     1492272 :     real(r8), pointer, dimension(:,:) :: tcorr
         541     1492272 :     real(r8), pointer, dimension(:,:) :: qrsin
         542     1492272 :     real(r8), pointer, dimension(:,:) :: qrlin
         543     1492272 :     real(r8), pointer, dimension(:)   :: tropp
         544     1492272 :     real(r8), pointer, dimension(:,:) :: qrs
         545     1492272 :     real(r8), pointer, dimension(:,:) :: qrl
         546     1492272 :     real(r8), pointer, dimension(:,:,:) :: dgnumwet_ptr
         547     1492272 :     real(r8), pointer, dimension(:,:,:) :: qaerwat_ptr
         548             :
         549     1492272 :     if (.not.enabled) return
         550           0 :     call pbuf_get_field(pbuf, qrs_ifld, qrs )
         551           0 :     call pbuf_get_field(pbuf, qrl_ifld, qrl )
         552             :
         553           0 :     lchnk = state%lchnk
         554           0 :     ncol = state%ncol
         555             :
         556             :    ! store temperature correction above tropopause in pbuf for Fixed Dynamical Heating
         557           0 :     if(do_fdh) then
         558             :
         559           0 :        call pbuf_get_field(pbuf, tcorr_idx, tcorr)
         560           0 :        call pbuf_get_field(pbuf, qrsin_idx, qrsin)
         561           0 :        call pbuf_get_field(pbuf, qrlin_idx, qrlin)
         562           0 :        call pbuf_get_field(pbuf, tropp_idx, tropp)
         563           0 :        do k = 1, pver
         564           0 :           do i = 1, ncol
         565           0 :              if ( state%pmid(i,k) < tropp(i)) then
         566           0 :                 tcorr(i,k) = tcorr(i,k) + drv_input_data_freq*(qrs(i,k) - qrsin(i,k) + qrl(i,k) - qrlin(i,k)) /cpair
         567             :              endif
         568             :           enddo
         569             :        enddo
         570             :
         571           0 :        call outfld('rad_TROP_P', tropp(:ncol), ncol, lchnk)
         572           0 :        call outfld('rad_TCORR', tcorr(:ncol,:), ncol, lchnk)
         573             :
         574             :     end if
         575             :
         576           0 :     if (.not.rad_data_output) return
         577             :
         578           0 :     call outfld(qrs_fldn, qrs, pcols, lchnk )
         579           0 :     call outfld(qrl_fldn, qrl, pcols, lchnk )
         580             :
         581             :     ! get index of (liquid+ice) cloud water
         582           0 :     call cnst_get_ind('CLDICE', ixcldice)
         583           0 :     call cnst_get_ind('CLDLIQ', ixcldliq)
         584             :
         585           0 :     do icol = 1, ncol
         586           0 :        coszrs_pos(icol)  = max(coszen(icol),0._r8)
         587             :     enddo
         588           0 :     asdir_pos(:ncol)  = cam_in%asdir(:ncol) * coszrs_pos(:ncol)
         589           0 :     asdif_pos(:ncol)  = cam_in%asdif(:ncol) * coszrs_pos(:ncol)
         590           0 :     aldir_pos(:ncol)  = cam_in%aldir(:ncol) * coszrs_pos(:ncol)
         591           0 :     aldif_pos(:ncol)  = cam_in%aldif(:ncol) * coszrs_pos(:ncol)
         592             :
         593           0 :     call outfld(lndfrc_fldn, cam_in%landfrac,  pcols, lchnk)
         594           0 :     call outfld(icefrc_fldn, cam_in%icefrac,   pcols, lchnk)
         595           0 :     call outfld(snowh_fldn,  cam_in%snowhland, pcols, lchnk)
         596           0 :     call outfld(temp_fldn,   state%t,               pcols, lchnk   )
         597           0 :     call outfld(pdel_fldn,   state%pdel,            pcols, lchnk   )
         598           0 :     call outfld(pdeldry_fldn,state%pdeldry,         pcols, lchnk   )
         599           0 :     call outfld(watice_fldn, state%q(:,:,ixcldice), pcols, lchnk   )
         600           0 :     call outfld(watliq_fldn, state%q(:,:,ixcldliq), pcols, lchnk   )
         601           0 :     call outfld(watvap_fldn, state%q(:,:,1),        pcols, lchnk   )
         602           0 :     call outfld(zint_fldn,   state%zi,              pcols, lchnk   )
         603           0 :     call outfld(pint_fldn,   state%pint,            pcols, lchnk   )
         604           0 :     call outfld(pmid_fldn,   state%pmid,            pcols, lchnk   )
         605             :
         606           0 :     call outfld(asdir_fldn, cam_in%asdir, pcols, lchnk   )
         607           0 :     call outfld(asdif_fldn, cam_in%asdif, pcols, lchnk   )
         608           0 :     call outfld(aldir_fldn, cam_in%aldir, pcols, lchnk   )
         609           0 :     call outfld(aldif_fldn, cam_in%aldif, pcols, lchnk   )
         610             :
         611           0 :     call outfld(coszen_fldn, coszrs_pos, pcols, lchnk   )
         612           0 :     call outfld(asdir_pos_fldn, asdir_pos, pcols, lchnk   )
         613           0 :     call outfld(asdif_pos_fldn, asdif_pos, pcols, lchnk   )
         614           0 :     call outfld(aldir_pos_fldn, aldir_pos, pcols, lchnk   )
         615           0 :     call outfld(aldif_pos_fldn, aldif_pos, pcols, lchnk   )
         616             :
         617           0 :     call outfld(lwup_fldn,  cam_in%lwup,  pcols, lchnk   )
         618           0 :     call outfld(ts_fldn,    cam_in%ts,    pcols, lchnk   )
         619             :
         620           0 :     itim_old = pbuf_old_tim_idx()
         621             :
         622           0 :     call pbuf_get_field(pbuf, cld_ifld,    ptr, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
         623           0 :     call outfld(cld_fldn,    ptr, pcols, lchnk )
         624             :
         625           0 :     call pbuf_get_field(pbuf, rel_ifld,    ptr )
         626           0 :     call outfld(rel_fldn,    ptr, pcols, lchnk )
         627             :
         628           0 :     call pbuf_get_field(pbuf, rei_ifld,    ptr )
         629           0 :     call outfld(rei_fldn,    ptr, pcols, lchnk )
         630             :
         631           0 :     if (mg_microphys) then
         632             :
         633           0 :        call pbuf_get_field(pbuf,  dei_ifld, ptr     )
         634           0 :        call outfld(dei_fldn,      ptr, pcols, lchnk   )
         635             :
         636           0 :        call pbuf_get_field(pbuf,  des_ifld, ptr     )
         637           0 :        call outfld(des_fldn,      ptr, pcols, lchnk   )
         638             :
         639           0 :        call pbuf_get_field(pbuf,  mu_ifld, ptr      )
         640           0 :        call outfld(mu_fldn,       ptr, pcols, lchnk   )
         641             :
         642           0 :        call pbuf_get_field(pbuf,  lambdac_ifld, ptr )
         643           0 :        call outfld(lambdac_fldn,  ptr, pcols, lchnk   )
         644             :
         645           0 :        call pbuf_get_field(pbuf,  iciwp_ifld, ptr   )
         646           0 :        call outfld(iciwp_fldn,    ptr, pcols, lchnk   )
         647             :
         648           0 :        call pbuf_get_field(pbuf,  iclwp_ifld, ptr   )
         649           0 :        call outfld(iclwp_fldn,    ptr, pcols, lchnk   )
         650             :
         651           0 :        call pbuf_get_field(pbuf,  icswp_ifld, ptr   )
         652           0 :        call outfld(icswp_fldn,    ptr, pcols, lchnk   )
         653             :
         654           0 :        call pbuf_get_field(pbuf,  cldfsnow_ifld, ptr, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
         655           0 :        call outfld(cldfsnow_fldn, ptr, pcols, lchnk   )
         656             :
         657             :     else
         658             :
         659           0 :        call pbuf_get_field(pbuf, cldemis_ifld,    ptr )
         660           0 :        call outfld(cldemis_fldn,   ptr, pcols, lchnk )
         661             :
         662           0 :        call pbuf_get_field(pbuf, cldtau_ifld,    ptr )
         663           0 :        call outfld(cldtau_fldn,    ptr, pcols, lchnk )
         664             :
         665           0 :        call pbuf_get_field(pbuf, cicewp_ifld,    ptr )
         666           0 :        call outfld(cicewp_fldn,    ptr, pcols, lchnk )
         667             :
         668           0 :        call pbuf_get_field(pbuf, cliqwp_ifld,    ptr )
         669           0 :        call outfld(cliqwp_fldn,    ptr, pcols, lchnk )
         670             :
         671           0 :        call pbuf_get_field(pbuf, nmxrgn_ifld,    iptr1d )
         672           0 :        rptr1d = dble(iptr1d)
         673           0 :        call outfld(nmxrgn_fldn,    rptr1d, pcols, lchnk )
         674             :
         675           0 :        call pbuf_get_field(pbuf, pmxrgn_ifld,    ptr )
         676           0 :        call outfld(pmxrgn_fldn,    ptr, pcols, lchnk )
         677             :
         678             :     endif
         679             :
         680             :     ! output mixing ratio of rad constituents
         681             :
         682           0 :     do i = 1, ngas
         683           0 :        name = 'rad_'//gasnames(i)
         684           0 :        call rad_cnst_get_gas(0, gaslist(i), state, pbuf, mmr)
         685           0 :        call outfld(trim(name), mmr, pcols, lchnk)
         686             :     end do
         687             :
         688           0 :     if ( naer>0 ) then
         689             :        ! bulk aerosol model
         690           0 :        do i = 1, naer
         691           0 :           name = 'rad_'//aernames(i)
         692           0 :           call rad_cnst_get_aer_mmr(0, i, state, pbuf, mmr)
         693           0 :           call outfld(trim(name), mmr, pcols, lchnk)
         694             :        end do
         695             :     endif
         696           0 :     if (nmodes>0) then
         697             :
         698           0 :        call pbuf_get_field(pbuf, dgnumwet_ifld, dgnumwet_ptr)
         699           0 :        call pbuf_get_field(pbuf, qaerwat_ifld, qaerwat_ptr)
         700             :
         701             :        ! for modal aerosol model
         702           0 :        do m = 1, nmodes
         703           0 :           ptr => dgnumwet_ptr(:,:,m)
         704           0 :           call outfld( dgnumwet_fldn(m), ptr, pcols, lchnk )
         705           0 :           ptr => qaerwat_ptr(:,:,m)
         706           0 :           call outfld( qaerwat_fldn(m),  ptr, pcols, lchnk )
         707             :
         708             :           ! get mode info
         709           0 :           call rad_cnst_get_info(0, m, nspec=nspec)
         710             :           ! aerosol species loop
         711           0 :           do l = 1, nspec
         712           0 :              call rad_cnst_get_info(0,m,l, spec_name=aername)
         713           0 :              call rad_cnst_get_aer_mmr(0, m, l, 'a', state, pbuf, mmr)
         714           0 :              name = 'rad_'//aername
         715           0 :              call outfld(trim(name), mmr, pcols, lchnk)
         716             :           enddo
         717             :        enddo
         718             :     endif
         719             :
         720             :     ! stratospheric aersols geometric mean radius
         721           0 :     if (volcgeom_ifld > 0) then
         722           0 :        call pbuf_get_field(pbuf, volcgeom_ifld, ptr)
         723           0 :        call outfld(volcgeom_fldn, ptr, pcols, lchnk)
         724             :     endif
         725           0 :     if (gmean_3modes) then
         726           0 :        call pbuf_get_field(pbuf, volcgeom1_ifld, ptr)
         727           0 :        call outfld(volcgeom1_fldn, ptr, pcols, lchnk)
         728           0 :        call pbuf_get_field(pbuf, volcgeom2_ifld, ptr)
         729           0 :        call outfld(volcgeom2_fldn, ptr, pcols, lchnk)
         730           0 :        call pbuf_get_field(pbuf, volcgeom3_ifld, ptr)
         731           0 :        call outfld(volcgeom3_fldn, ptr, pcols, lchnk)
         732             :     endif
         733             :
         734     1492272 :   end subroutine rad_data_write
         735             :
         736             : !=================================================================================
         737             : !=================================================================================
         738           0 :   subroutine rad_data_read(indata, phys_state, pbuf2d, cam_in, recno )
         739             :
         740     1492272 :     use camsrfexch,       only: cam_in_t
         741             :     use physics_buffer,   only: pbuf_get_field, pbuf_old_tim_idx
         742             :     use constituents,     only: cnst_get_ind
         743             :     use tropopause,       only: tropopause_find_cam, TROP_ALG_HYBSTOB, TROP_ALG_CLIMATE
         744             :
         745             :     implicit none
         746             :
         747             :     type(drv_input_data_t), intent(inout) :: indata
         748             :     type(physics_buffer_desc), pointer         :: pbuf2d(:,:)
         749             :     type(physics_state), target, intent(inout) :: phys_state(begchunk:endchunk)
         750             :     type(cam_in_t),      target, intent(inout) :: cam_in(begchunk:endchunk)
         751             :     integer,             intent(in)            :: recno
         752             :
         753             : ! local vars
         754           0 :     type(physics_buffer_desc), pointer :: pbuf(:)
         755             :
         756           0 :     type(drv_input_3d_t) :: cld_ptrs(begchunk:endchunk)
         757           0 :     type(drv_input_3d_t) :: cldfsnow_ptrs(begchunk:endchunk)
         758             :
         759           0 :     type(drv_input_3d_t) :: rel_ptrs(begchunk:endchunk)
         760           0 :     type(drv_input_3d_t) :: rei_ptrs(begchunk:endchunk)
         761           0 :     type(drv_input_3d_t) :: dei_ptrs(begchunk:endchunk)
         762           0 :     type(drv_input_3d_t) :: des_ptrs(begchunk:endchunk)
         763           0 :     type(drv_input_3d_t) :: mu_ptrs(begchunk:endchunk)
         764           0 :     type(drv_input_3d_t) :: lambdac_ptrs(begchunk:endchunk)
         765           0 :     type(drv_input_3d_t) :: iciwp_ptrs(begchunk:endchunk)
         766           0 :     type(drv_input_3d_t) :: iclwp_ptrs(begchunk:endchunk)
         767           0 :     type(drv_input_3d_t) :: icswp_ptrs(begchunk:endchunk)
         768             :
         769           0 :     type(drv_input_3d_t) :: qrs_ptrs(begchunk:endchunk)
         770           0 :     type(drv_input_3d_t) :: qrl_ptrs(begchunk:endchunk)
         771             :
         772           0 :     type(drv_input_3d_t) :: watvap_ptrs(begchunk:endchunk)
         773           0 :     type(drv_input_3d_t) :: watliq_ptrs(begchunk:endchunk)
         774           0 :     type(drv_input_3d_t) :: watice_ptrs(begchunk:endchunk)
         775             :
         776           0 :     type(drv_input_3d_t) :: zi_ptrs(begchunk:endchunk)
         777           0 :     type(drv_input_3d_t) :: pint_ptrs(begchunk:endchunk)
         778           0 :     type(drv_input_3d_t) :: lnpint_ptrs(begchunk:endchunk)
         779             :
         780           0 :     type(drv_input_3d_t) :: temp_ptrs(begchunk:endchunk)
         781           0 :     type(drv_input_3d_t) :: pdel_ptrs(begchunk:endchunk)
         782           0 :     type(drv_input_3d_t) :: pdeldry_ptrs(begchunk:endchunk)
         783           0 :     type(drv_input_3d_t) :: lnpmid_ptrs(begchunk:endchunk)
         784           0 :     type(drv_input_3d_t) :: pmid_ptrs(begchunk:endchunk)
         785             :
         786           0 :     type(drv_input_2d_t) :: lndfrac_ptrs(begchunk:endchunk)
         787           0 :     type(drv_input_2d_t) :: icefrac_ptrs(begchunk:endchunk)
         788           0 :     type(drv_input_2d_t) :: snowhland_ptrs(begchunk:endchunk)
         789           0 :     type(drv_input_2d_t) :: asdir_ptrs(begchunk:endchunk)
         790           0 :     type(drv_input_2d_t) :: asdif_ptrs(begchunk:endchunk)
         791           0 :     type(drv_input_2d_t) :: aldir_ptrs(begchunk:endchunk)
         792           0 :     type(drv_input_2d_t) :: aldif_ptrs(begchunk:endchunk)
         793             :
         794           0 :     type(drv_input_2di_t):: nmxrgn_ptrs(begchunk:endchunk)
         795           0 :     type(drv_input_3d_t) :: pmxrgn_ptrs(begchunk:endchunk)
         796             :
         797           0 :     type(drv_input_3d_t) :: cldemis_ptrs(begchunk:endchunk)
         798           0 :     type(drv_input_3d_t) :: cldtau_ptrs(begchunk:endchunk)
         799           0 :     type(drv_input_3d_t) :: cicewp_ptrs(begchunk:endchunk)
         800           0 :     type(drv_input_3d_t) :: cliqwp_ptrs(begchunk:endchunk)
         801             :
         802           0 :     type(drv_input_2d_t) :: lwup_ptrs(begchunk:endchunk)
         803           0 :     type(drv_input_2d_t) :: ts_ptrs(begchunk:endchunk)
         804             :
         805           0 :     type(drv_input_3d_t) :: volcgeom_ptrs(begchunk:endchunk)
         806           0 :     type(drv_input_3d_t) :: volcgeom1_ptrs(begchunk:endchunk)
         807           0 :     type(drv_input_3d_t) :: volcgeom2_ptrs(begchunk:endchunk)
         808           0 :     type(drv_input_3d_t) :: volcgeom3_ptrs(begchunk:endchunk)
         809             :
         810             :     integer :: i, k, c, ncol, itim
         811             :
         812             :     integer :: ixcldice   ! cloud ice water index
         813             :     integer :: ixcldliq   ! cloud liquid water index
         814             :
         815             :     ! for Fixed Dynamical Heating
         816           0 :     real(r8), pointer, dimension(:,:) :: tcorr
         817           0 :     real(r8), pointer, dimension(:,:) :: qrsin
         818           0 :     real(r8), pointer, dimension(:,:) :: qrlin
         819           0 :     real(r8), pointer, dimension(:)   :: tropp
         820             :     integer :: troplev(pcols)
         821             :
         822             :     ! for modal aerosols
         823           0 :     type(drv_input_4d_t) :: dgnumwet_ptrs(begchunk:endchunk)
         824           0 :     type(drv_input_4d_t) :: qaerwat_ptrs(begchunk:endchunk)
         825             :
         826             :     ! get index of (liquid+ice) cloud water
         827           0 :     call cnst_get_ind('CLDICE', ixcldice)
         828           0 :     call cnst_get_ind('CLDLIQ', ixcldliq)
         829             :
         830             :     ! phys buffer time index
         831           0 :     itim = pbuf_old_tim_idx()
         832             :
         833             :     ! setup the data pointers
         834             : !$OMP PARALLEL DO PRIVATE (C,pbuf)
         835           0 :     do c=begchunk,endchunk
         836           0 :        pbuf => pbuf_get_chunk(pbuf2d, c)
         837             :
         838           0 :        watvap_ptrs (c)%array => phys_state(c)%q(:,:,1)
         839           0 :        watliq_ptrs (c)%array => phys_state(c)%q(:,:,ixcldliq)
         840           0 :        watice_ptrs (c)%array => phys_state(c)%q(:,:,ixcldice)
         841             :
         842           0 :        zi_ptrs     (c)%array => phys_state(c)%zi
         843           0 :        pint_ptrs   (c)%array => phys_state(c)%pint
         844           0 :        lnpint_ptrs (c)%array => phys_state(c)%lnpint
         845             :
         846           0 :        temp_ptrs   (c)%array => phys_state(c)%t
         847           0 :        pdel_ptrs   (c)%array => phys_state(c)%pdel
         848           0 :        pdeldry_ptrs(c)%array => phys_state(c)%pdeldry
         849           0 :        lnpmid_ptrs (c)%array => phys_state(c)%lnpmid
         850           0 :        pmid_ptrs   (c)%array => phys_state(c)%pmid
         851             :
         852           0 :        lndfrac_ptrs  (c)%array => cam_in(c)%landfrac
         853           0 :        icefrac_ptrs  (c)%array => cam_in(c)%icefrac
         854           0 :        snowhland_ptrs(c)%array => cam_in(c)%snowhland
         855           0 :        asdir_ptrs    (c)%array => cam_in(c)%asdir
         856           0 :        asdif_ptrs    (c)%array => cam_in(c)%asdif
         857           0 :        aldir_ptrs    (c)%array => cam_in(c)%aldir
         858           0 :        aldif_ptrs    (c)%array => cam_in(c)%aldif
         859           0 :        lwup_ptrs     (c)%array => cam_in(c)%lwup
         860           0 :        ts_ptrs       (c)%array => cam_in(c)%ts
         861             :
         862           0 :        call pbuf_get_field(pbuf, cld_ifld, cld_ptrs   (c)%array, start=(/1,1,itim/), kount=(/pcols,pver,1/) )
         863           0 :        call pbuf_get_field(pbuf, rel_ifld,   rel_ptrs(c)%array )
         864           0 :        call pbuf_get_field(pbuf, rei_ifld,   rei_ptrs(c)%array )
         865             :
         866           0 :        call pbuf_get_field(pbuf, qrs_ifld,   qrs_ptrs(c)%array )
         867           0 :        call pbuf_get_field(pbuf, qrl_ifld,   qrl_ptrs(c)%array )
         868             :
         869           0 :        if (mg_microphys) then
         870           0 :           call pbuf_get_field(pbuf, dei_ifld,   dei_ptrs(c)%array )
         871           0 :           call pbuf_get_field(pbuf, des_ifld,   des_ptrs(c)%array )
         872           0 :           call pbuf_get_field(pbuf, mu_ifld,    mu_ptrs     (c)%array )
         873           0 :           call pbuf_get_field(pbuf, lambdac_ifld, lambdac_ptrs(c)%array )
         874           0 :           call pbuf_get_field(pbuf, iciwp_ifld, iciwp_ptrs  (c)%array )
         875           0 :           call pbuf_get_field(pbuf, iclwp_ifld, iclwp_ptrs  (c)%array )
         876           0 :           call pbuf_get_field(pbuf, icswp_ifld, icswp_ptrs  (c)%array )
         877           0 :           call pbuf_get_field(pbuf, cldfsnow_ifld, cldfsnow_ptrs(c)%array, start=(/1,1,itim/), kount=(/pcols,pver,1/) )
         878             :        else
         879           0 :           call pbuf_get_field(pbuf, nmxrgn_ifld,   nmxrgn_ptrs(c)%array )
         880           0 :           call pbuf_get_field(pbuf, pmxrgn_ifld,   pmxrgn_ptrs(c)%array )
         881           0 :           call pbuf_get_field(pbuf, cldemis_ifld,  cldemis_ptrs(c)%array )
         882           0 :           call pbuf_get_field(pbuf, cldtau_ifld,   cldtau_ptrs(c)%array )
         883           0 :           call pbuf_get_field(pbuf, cicewp_ifld,   cicewp_ptrs(c)%array )
         884           0 :           call pbuf_get_field(pbuf, cliqwp_ifld,   cliqwp_ptrs(c)%array )
         885             :        endif
         886             :
         887           0 :        if (nmodes>0) then
         888           0 :           call pbuf_get_field(pbuf, dgnumwet_ifld, dgnumwet_ptrs(c)%array )
         889           0 :           call pbuf_get_field(pbuf, qaerwat_ifld, qaerwat_ptrs(c)%array )
         890             :        endif
         891             :
         892             :        ! stratospheric aersols geometric mean radius
         893           0 :        if (volcgeom_ifld > 0) then
         894           0 :           call pbuf_get_field(pbuf, volcgeom_ifld, volcgeom_ptrs(c)%array )
         895             :        endif
         896           0 :        if (gmean_3modes) then
         897           0 :           call pbuf_get_field(pbuf, volcgeom1_ifld, volcgeom1_ptrs(c)%array )
         898           0 :           call pbuf_get_field(pbuf, volcgeom2_ifld, volcgeom2_ptrs(c)%array )
         899           0 :           call pbuf_get_field(pbuf, volcgeom3_ifld, volcgeom3_ptrs(c)%array )
         900             :        endif
         901             :
         902             :     enddo
         903             :
         904             :
         905           0 :     if (nmodes>0) then
         906           0 :        call get_aeromode_data( indata, dgnumwet_fldn, recno, dgnumwet_ptrs )
         907           0 :        call get_aeromode_data( indata, qaerwat_fldn, recno, qaerwat_ptrs )
         908             :     endif
         909             :
         910             :     ! get the 2D data
         911             :
         912           0 :     call drv_input_data_get( indata, lndfrc_fldn, recno, lndfrac_ptrs )
         913           0 :     call drv_input_data_get( indata, icefrc_fldn, recno, icefrac_ptrs )
         914           0 :     call drv_input_data_get( indata, snowh_fldn,  recno, snowhland_ptrs )
         915           0 :     call drv_input_data_get( indata, asdir_fldn,  recno, asdir_ptrs )
         916           0 :     call drv_input_data_get( indata, asdif_fldn,  recno, asdif_ptrs )
         917           0 :     call drv_input_data_get( indata, aldir_fldn,  recno, aldir_ptrs )
         918           0 :     call drv_input_data_get( indata, aldif_fldn,  recno, aldif_ptrs )
         919           0 :     call drv_input_data_get( indata, lwup_fldn,   recno, lwup_ptrs )
         920           0 :     call drv_input_data_get( indata, ts_fldn,     recno, ts_ptrs )
         921             :
         922             :     ! get the 3D data
         923             :
         924           0 :     call drv_input_data_get( indata, cld_fldn,    'lev', pver, recno, cld_ptrs )
         925           0 :     call drv_input_data_get( indata, rel_fldn,    'lev', pver, recno, rel_ptrs )
         926           0 :     call drv_input_data_get( indata, rei_fldn,    'lev', pver, recno, rei_ptrs )
         927           0 :     call drv_input_data_get( indata, qrs_fldn,    'lev', pver, recno, qrs_ptrs )
         928           0 :     call drv_input_data_get( indata, qrl_fldn,    'lev', pver, recno, qrl_ptrs )
         929             :
         930           0 :     if (mg_microphys) then
         931           0 :        call drv_input_data_get( indata, dei_fldn,    'lev', pver, recno, dei_ptrs )
         932           0 :        call drv_input_data_get( indata, des_fldn,    'lev', pver, recno, des_ptrs )
         933           0 :        call drv_input_data_get( indata, mu_fldn,     'lev', pver, recno, mu_ptrs )
         934           0 :        call drv_input_data_get( indata, lambdac_fldn,'lev', pver, recno, lambdac_ptrs )
         935           0 :        call drv_input_data_get( indata, iciwp_fldn,  'lev', pver, recno, iciwp_ptrs )
         936           0 :        call drv_input_data_get( indata, iclwp_fldn,  'lev', pver, recno, iclwp_ptrs )
         937           0 :        call drv_input_data_get( indata, icswp_fldn,  'lev', pver, recno, icswp_ptrs )
         938           0 :        call drv_input_data_get( indata, cldfsnow_fldn,'lev',pver, recno, cldfsnow_ptrs )
         939             :     else
         940           0 :        call drv_input_data_get( indata, nmxrgn_fldn, recno, nmxrgn_ptrs )
         941           0 :        call drv_input_data_get( indata, pmxrgn_fldn, 'ilev',pverp,recno, pmxrgn_ptrs )
         942           0 :        call drv_input_data_get( indata, cldemis_fldn,'lev', pver, recno, cldemis_ptrs )
         943           0 :        call drv_input_data_get( indata, cldtau_fldn, 'lev', pver, recno, cldtau_ptrs )
         944           0 :        call drv_input_data_get( indata, cicewp_fldn, 'lev', pver, recno, cicewp_ptrs )
         945           0 :        call drv_input_data_get( indata, cliqwp_fldn, 'lev', pver, recno, cliqwp_ptrs )
         946             :     endif
         947             :
         948             :     ! stratospheric aersols geometric mean radius
         949           0 :     if (volcgeom_ifld > 0) then
         950           0 :        call drv_input_data_get( indata, volcgeom_fldn, 'lev', pver, recno, volcgeom_ptrs )
         951             :     endif
         952           0 :     if (gmean_3modes) then
         953           0 :        call drv_input_data_get( indata, volcgeom1_fldn, 'lev', pver, recno, volcgeom1_ptrs )
         954           0 :        call drv_input_data_get( indata, volcgeom2_fldn, 'lev', pver, recno, volcgeom2_ptrs )
         955           0 :        call drv_input_data_get( indata, volcgeom3_fldn, 'lev', pver, recno, volcgeom3_ptrs )
         956             :     endif
         957             :
         958           0 :     call drv_input_data_get( indata, watvap_fldn, 'lev', pver, recno, watvap_ptrs )
         959           0 :     call drv_input_data_get( indata, watliq_fldn, 'lev', pver, recno, watliq_ptrs )
         960           0 :     call drv_input_data_get( indata, watice_fldn, 'lev', pver, recno, watice_ptrs )
         961           0 :     call drv_input_data_get( indata, temp_fldn,   'lev', pver, recno, temp_ptrs )
         962           0 :     call drv_input_data_get( indata, pdel_fldn,   'lev', pver, recno, pdel_ptrs )
         963           0 :     call drv_input_data_get( indata, pdeldry_fldn,'lev', pver, recno, pdeldry_ptrs )
         964           0 :     call drv_input_data_get( indata, pmid_fldn,   'lev', pver, recno, pmid_ptrs )
         965             :
         966           0 :     call drv_input_data_get( indata, zint_fldn,   'ilev',pverp,recno, zi_ptrs )
         967           0 :     call drv_input_data_get( indata, pint_fldn,   'ilev',pverp,recno, pint_ptrs )
         968             :
         969           0 :     do c=begchunk,endchunk
         970           0 :        ncol = phys_state(c)%ncol
         971           0 :        if (all(pmid_ptrs(c)%array(:ncol,:) > 0._r8 )) then
         972           0 :           do i=1,ncol
         973           0 :              lnpmid_ptrs(c)%array(i,:) = log(pmid_ptrs(c)%array(i,:))
         974           0 :              lnpint_ptrs(c)%array(i,:) = log(pint_ptrs(c)%array(i,:))
         975             :           enddo
         976             :        endif
         977             :
         978             :        ! adjust temperatue input above tropopause for Fixed Dynamical Heating ....
         979           0 :        if (do_fdh) then
         980           0 :           pbuf => pbuf_get_chunk(pbuf2d, c)
         981             :
         982           0 :           call pbuf_get_field(pbuf, tropp_idx, tropp)
         983           0 :           call pbuf_get_field(pbuf, tcorr_idx, tcorr)
         984           0 :           call pbuf_get_field(pbuf, qrsin_idx, qrsin)
         985           0 :           call pbuf_get_field(pbuf, qrlin_idx, qrlin)
         986             :
         987             :           !REMOVECAM - no longer need this when CAM is retired and pcols no longer exists
         988           0 :           troplev(:) = 0
         989           0 :           tropp(:) = 0._r8
         990             :           !REMOVECAM_END
         991           0 :           call tropopause_find_cam(phys_state(c), troplev, tropP=tropp, primary=TROP_ALG_CLIMATE, &
         992           0 :                                backup=TROP_ALG_CLIMATE)
         993             :
         994           0 :           qrsin(:,:) = qrs_ptrs(c)%array(:,:)
         995           0 :           qrlin(:,:) = qrl_ptrs(c)%array(:,:)
         996             :
         997           0 :           do k = 1, pver
         998           0 :              do i = 1, ncol
         999           0 :                 if ( phys_state(c)%pmid(i,k) < tropp(i) ) then
        1000           0 :                    temp_ptrs(c)%array(i,k) = temp_ptrs(c)%array(i,k) + tcorr(i,k)
        1001             :                 endif
        1002             :              enddo
        1003             :           enddo
        1004             :        endif
        1005             :
        1006             :     enddo
        1007             :
        1008           0 :     call get_rad_cnst_data(indata, phys_state, pbuf2d, recno)
        1009             :
        1010           0 :   end subroutine rad_data_read
        1011             :
        1012             : !================================================================================================
        1013             : ! Private routines
        1014             : !================================================================================================
        1015             :
        1016             :
        1017             :   !================================================================================================
        1018             :   !================================================================================================
        1019           0 :   subroutine get_aeromode_data(indata, infld_names, recno, chunk_ptrs)
        1020           0 :     use drv_input_data, only: drv_input_data_read
        1021             :
        1022             :     type(drv_input_data_t), intent(inout) :: indata
        1023             :     character(len=*),    intent(in)    :: infld_names(nmodes)
        1024             :     integer,             intent(in)    :: recno
        1025             :     type(drv_input_4d_t),   intent(inout) :: chunk_ptrs(begchunk:endchunk)
        1026             :
        1027           0 :     real(r8) :: data (pcols, pver, begchunk:endchunk)
        1028             :
        1029             :     integer :: c, n
        1030             :
        1031           0 :     do n = 1,nmodes
        1032             :
        1033           0 :        data = drv_input_data_read( indata, infld_names(n), 'lev', pver, recno )
        1034           0 :        do c=begchunk,endchunk
        1035           0 :           chunk_ptrs(c)%array(:,:,n) = data(:,:,c)
        1036             :        enddo
        1037             :
        1038             :     enddo
        1039             :
        1040           0 :   end subroutine get_aeromode_data
        1041             :
        1042             :   !================================================================================================
        1043             :   !================================================================================================
        1044           0 :   subroutine get_rad_cnst_data(indata, state, pbuf2d, recno)
        1045             :
        1046           0 :     use physics_types,    only: physics_state
        1047             :     use physics_buffer,   only: physics_buffer_desc
        1048             :     use rad_constituents, only: rad_cnst_get_info
        1049             :
        1050             :     implicit none
        1051             :
        1052             :     ! Arguments
        1053             :     type(drv_input_data_t), intent(inout) :: indata
        1054             :     type(physics_buffer_desc), pointer :: pbuf2d(:,:)
        1055             :     type(physics_state), intent(inout) :: state(begchunk:endchunk)
        1056             :     integer,             intent(in)    :: recno
        1057             :
        1058             :     ! Local variables
        1059             :     integer :: i, ncol
        1060             :     integer :: m, l, nspec
        1061             :     integer :: idx
        1062             :     character(len=32) :: aername
        1063             :
        1064             :     !-----------------------------------------------------------------------------
        1065             :
        1066             :     ! read in mixing ratio of rad constituents
        1067             :
        1068           0 :     do i = 1,ngas
        1069           0 :        call read_rad_gas_data(indata, gasnames(i), i, state, pbuf2d, recno )
        1070             :     enddo
        1071             :
        1072           0 :     do i = 1,naer
        1073           0 :        call read_rad_aer_data(indata, aernames(i), i, state, pbuf2d, recno )
        1074             :     enddo
        1075             :
        1076             :     ! aerosol mode loop
        1077           0 :     do m = 1, nmodes
        1078             :
        1079             :        ! get mode info
        1080           0 :        call rad_cnst_get_info(0, m, nspec=nspec)
        1081             :        ! aerosol species loop
        1082           0 :        do l = 1, nspec
        1083           0 :           call rad_cnst_get_info(0,m,l, spec_name=aername)
        1084           0 :           call read_rad_mam_data( indata, aername, m, l, state, pbuf2d, recno )
        1085             :        end do
        1086             :     end do
        1087             :
        1088           0 :   end subroutine get_rad_cnst_data
        1089             :
        1090             :   !=================================================================================
        1091             :   !=================================================================================
        1092           0 :   subroutine read_rad_gas_data(indata, name, idx, state, pbuf2d, recno )
        1093           0 :     use rad_constituents, only: rad_cnst_get_gas
        1094             :     use drv_input_data,   only: drv_input_data_read
        1095             :
        1096             :     type(drv_input_data_t), intent(inout) :: indata
        1097             :     character(len=32),   intent(in)    :: name
        1098             :     integer,             intent(in)    :: idx
        1099             :     type(physics_state),target, intent(inout) :: state(begchunk:endchunk)
        1100             :     type(physics_buffer_desc), pointer, dimension(:,:) :: pbuf2d
        1101             :     integer,             intent(in)    :: recno
        1102             :
        1103           0 :     type(physics_buffer_desc), pointer, dimension(:) :: phys_buffer_chunk
        1104             :     character(len=32) :: radname
        1105             :     integer            :: c, ncol
        1106           0 :     real(r8)          :: mass(pcols,pver,begchunk:endchunk)
        1107           0 :     real(r8), pointer :: mmr_ptr(:,:)
        1108             :
        1109           0 :     radname = 'rad_'//trim(name)
        1110           0 :     mass = drv_input_data_read( indata, radname, 'lev', pver, recno )
        1111             :
        1112           0 :     do c = begchunk,endchunk
        1113           0 :        ncol = state(c)%ncol
        1114           0 :        phys_buffer_chunk => pbuf_get_chunk(pbuf2d, c)
        1115           0 :        call rad_cnst_get_gas(0, gaslist(idx), state(c), phys_buffer_chunk, mmr_ptr)
        1116           0 :        mmr_ptr(:ncol,:) = mass(:ncol,:,c)
        1117             :     enddo
        1118             :
        1119           0 :   end subroutine read_rad_gas_data
        1120             :
        1121             :   !=================================================================================
        1122             :   !=================================================================================
        1123           0 :   subroutine read_rad_aer_data(indata, name, idx, state, pbuf2d, recno )
        1124           0 :     use rad_constituents, only: rad_cnst_get_aer_mmr
        1125             :     use drv_input_data,   only: drv_input_data_read
        1126             :
        1127             :     type(drv_input_data_t), intent(inout) :: indata
        1128             :     character(len=32),   intent(in)    :: name
        1129             :     integer,             intent(in)    :: idx
        1130             :     type(physics_state),target, intent(inout) :: state(begchunk:endchunk)
        1131             :     type(physics_buffer_desc), pointer, dimension(:,:) :: pbuf2d
        1132             :     integer,             intent(in)    :: recno
        1133             :
        1134           0 :     type(physics_buffer_desc), pointer, dimension(:) :: phys_buffer_chunk
        1135             :     character(len=32) :: radname
        1136             :     integer :: c, ncol
        1137           0 :     real(r8)          :: mass(pcols,pver,begchunk:endchunk)
        1138           0 :     real(r8), pointer :: mmr_ptr(:,:)
        1139             :
        1140           0 :     radname = 'rad_'//trim(name)
        1141           0 :     mass = drv_input_data_read( indata, radname, 'lev', pver, recno )
        1142             :
        1143           0 :     do c = begchunk,endchunk
        1144           0 :        ncol = state(c)%ncol
        1145           0 :        phys_buffer_chunk => pbuf_get_chunk(pbuf2d, c)
        1146           0 :        call rad_cnst_get_aer_mmr(0, idx, state(c), phys_buffer_chunk, mmr_ptr)
        1147           0 :        mmr_ptr(:ncol,:) = mass(:ncol,:,c)
        1148             :     enddo
        1149             :
        1150           0 :   end subroutine read_rad_aer_data
        1151             :
        1152             :   !=================================================================================
        1153             :   !=================================================================================
        1154           0 :   subroutine read_rad_mam_data(indata, name, mode_idx, spec_idx, state, pbuf2d, recno )
        1155           0 :     use rad_constituents, only: rad_cnst_get_aer_mmr
        1156             :     use drv_input_data,   only: drv_input_data_read
        1157             :
        1158             :     type(drv_input_data_t), intent(inout) :: indata
        1159             :     character(len=32),   intent(in)    :: name
        1160             :     integer,             intent(in)    :: mode_idx
        1161             :     integer,             intent(in)    :: spec_idx
        1162             :     type(physics_state),target, intent(inout) :: state(begchunk:endchunk)
        1163             :     type(physics_buffer_desc), pointer, dimension(:,:) :: pbuf2d
        1164             :     integer,             intent(in)    :: recno
        1165             :
        1166           0 :     type(physics_buffer_desc), pointer, dimension(:) :: phys_buffer_chunk
        1167             :     character(len=32) :: radname
        1168             :     integer :: c, ncol
        1169           0 :     real(r8)          :: mass(pcols,pver,begchunk:endchunk)
        1170           0 :     real(r8), pointer :: mmr_ptr(:,:)
        1171             :
        1172           0 :     radname = 'rad_'//trim(name)
        1173           0 :     mass = drv_input_data_read( indata, radname, 'lev', pver, recno )
        1174             :
        1175           0 :     do c = begchunk,endchunk
        1176           0 :        ncol = state(c)%ncol
        1177           0 :        phys_buffer_chunk => pbuf_get_chunk(pbuf2d, c)
        1178           0 :        call rad_cnst_get_aer_mmr(0, mode_idx, spec_idx, 'a', state(c), phys_buffer_chunk, mmr_ptr)
        1179           0 :        mmr_ptr(:ncol,:) = mass(:ncol,:,c)
        1180             :     enddo
        1181             :
        1182           0 :   end subroutine read_rad_mam_data
        1183             :
        1184             : end module radiation_data

Generated by: LCOV version 1.14