LCOV - code coverage report
Current view: | top level - cpl/nuopc - atm_import_export.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 571 | 688 | 83.0 %
Date: | 2024-12-17 17:57:11 |  | Functions: | 9 | 10 | 90.0 %

              Line data    Source code
           1             : module atm_import_export
           2             :
           3             :   use NUOPC             , only : NUOPC_CompAttributeGet, NUOPC_Advertise, NUOPC_IsConnected
           4             :   use NUOPC_Model       , only : NUOPC_ModelGet
           5             :   use ESMF              , only : ESMF_GridComp, ESMF_State, ESMF_Mesh, ESMF_StateGet, ESMF_Field
           6             :   use ESMF              , only : ESMF_Clock
           7             :   use ESMF              , only : ESMF_KIND_R8, ESMF_SUCCESS, ESMF_MAXSTR, ESMF_LOGMSG_INFO
           8             :   use ESMF              , only : ESMF_LogWrite, ESMF_LOGMSG_ERROR, ESMF_LogFoundError
           9             :   use ESMF              , only : ESMF_STATEITEM_NOTFOUND, ESMF_StateItem_Flag
          10             :   use ESMF              , only : operator(/=), operator(==)
          11             :   use shr_kind_mod      , only : r8=>shr_kind_r8, i8=>shr_kind_i8, cl=>shr_kind_cl, cs=>shr_kind_cs, cx=>shr_kind_cx
          12             :   use shr_sys_mod       , only : shr_sys_abort
          13             :   use shr_mpi_mod       , only : shr_mpi_min, shr_mpi_max
          14             :   use nuopc_shr_methods , only : chkerr
          15             :   use cam_logfile       , only : iulog
          16             :   use spmd_utils        , only : masterproc, mpicom
          17             :   use srf_field_check   , only : set_active_Sl_ram1
          18             :   use srf_field_check   , only : set_active_Sl_fv
          19             :   use srf_field_check   , only : set_active_Sl_soilw
          20             :   use srf_field_check   , only : set_active_Fall_flxdst1
          21             :   use srf_field_check   , only : set_active_Fall_flxvoc
          22             :   use srf_field_check   , only : set_active_Fall_flxfire
          23             :   use srf_field_check   , only : set_active_Fall_fco2_lnd
          24             :   use srf_field_check   , only : set_active_Faoo_fco2_ocn
          25             :   use srf_field_check   , only : set_active_Faxa_nhx
          26             :   use srf_field_check   , only : set_active_Faxa_noy
          27             :   use srf_field_check   , only : active_Faxa_nhx, active_Faxa_noy
          28             :   use atm_stream_ndep   , only : stream_ndep_init, stream_ndep_interp, stream_ndep_is_initialized, use_ndep_stream
          29             :
          30             :   implicit none
          31             :   private ! except
          32             :
          33             :   public  :: read_surface_fields_namelists
          34             :   public  :: advertise_fields
          35             :   public  :: realize_fields
          36             :   public  :: import_fields
          37             :   public  :: export_fields
          38             :
          39             :   private :: fldlist_add
          40             :   private :: fldlist_realize
          41             :   private :: state_getfldptr
          42             :
          43             :   type fldlist_type
          44             :      character(len=128) :: stdname
          45             :      integer :: ungridded_lbound = 0
          46             :      integer :: ungridded_ubound = 0
          47             :   end type fldlist_type
          48             :
          49             :   integer             , parameter         :: fldsMax = 100
          50             :   integer             , public, protected :: fldsToAtm_num = 0
          51             :   integer             , public, protected :: fldsFrAtm_num = 0
          52             :   type (fldlist_type) , public, protected :: fldsToAtm(fldsMax)
          53             :   type (fldlist_type) , public, protected :: fldsFrAtm(fldsMax)
          54             :
          55             :   ! area correction factors for fluxes send and received from mediator
          56             :   real(r8), allocatable :: mod2med_areacor(:)
          57             :   real(r8), allocatable :: med2mod_areacor(:)
          58             :
          59             :   character(len=cx)      :: carma_fields = ' '      ! list of CARMA fields from lnd->atm
          60             :   integer                :: drydep_nflds = -huge(1) ! number of dry deposition velocity fields lnd-> atm
          61             :   integer                :: megan_nflds = -huge(1)  ! number of MEGAN voc fields from lnd-> atm
          62             :   integer                :: emis_nflds = -huge(1)   ! number of fire emission fields from lnd-> atm
          63             :   integer, public        :: ndep_nflds = -huge(1)   ! number of nitrogen deposition fields from atm->lnd/ocn
          64             :   logical                :: atm_provides_lightning = .false. ! cld to grnd lightning flash freq (min-1)
          65             :   character(*),parameter :: F01 = "('(cam_import_export) ',a,i8,2x,i8,2x,d21.14)"
          66             :   character(*),parameter :: F02 = "('(cam_import_export) ',a,i8,2x,i8,2x,i8,2x,d21.14)"
          67             :   character(*),parameter :: u_FILE_u = __FILE__
          68             :
          69             : !===============================================================================
          70             : contains
          71             : !===============================================================================
          72             :
          73             :   !-----------------------------------------------------------
          74             :   ! read mediator fields namelist file
          75             :   !-----------------------------------------------------------
          76        1536 :   subroutine read_surface_fields_namelists()
          77             :
          78             :     use shr_drydep_mod    , only : shr_drydep_readnl
          79             :     use shr_megan_mod     , only : shr_megan_readnl
          80             :     use shr_fire_emis_mod , only : shr_fire_emis_readnl
          81             :     use shr_carma_mod     , only : shr_carma_readnl
          82             :     use shr_ndep_mod      , only : shr_ndep_readnl
          83             :     use shr_lightning_coupling_mod, only : shr_lightning_coupling_readnl
          84             :
          85             :     character(len=*), parameter :: nl_file_name = 'drv_flds_in'
          86             :
          87             :     ! read mediator fields options
          88        1536 :     call shr_ndep_readnl(nl_file_name, ndep_nflds)
          89        1536 :     call shr_drydep_readnl(nl_file_name, drydep_nflds)
          90        1536 :     call shr_megan_readnl(nl_file_name, megan_nflds)
          91        1536 :     call shr_fire_emis_readnl(nl_file_name, emis_nflds)
          92        1536 :     call shr_carma_readnl(nl_file_name, carma_fields)
          93        1536 :     call shr_lightning_coupling_readnl(nl_file_name, atm_provides_lightning)
          94             :
          95        1536 :   end subroutine read_surface_fields_namelists
          96             :
          97             :   !-----------------------------------------------------------
          98             :   ! advertise fields
          99             :   !-----------------------------------------------------------
         100        1536 :   subroutine advertise_fields(gcomp, flds_scalar_name, rc)
         101             :
         102             :     ! input/output variables
         103             :     type(ESMF_GridComp)            :: gcomp
         104             :     character(len=*) , intent(in)  :: flds_scalar_name
         105             :     integer          , intent(out) :: rc
         106             :
         107             :     ! local variables
         108             :     type(ESMF_State)       :: importState
         109             :     type(ESMF_State)       :: exportState
         110             :     character(ESMF_MAXSTR) :: stdname
         111             :     character(ESMF_MAXSTR) :: cvalue
         112             :     integer                :: n, num
         113             :     logical                :: flds_co2a      ! use case
         114             :     logical                :: flds_co2b      ! use case
         115             :     logical                :: flds_co2c      ! use case
         116             :     character(len=128)     :: fldname
         117             :     character(len=*), parameter :: subname='(atm_import_export:advertise_fields)'
         118             :     !-------------------------------------------------------------------------------
         119             :
         120        1536 :     rc = ESMF_SUCCESS
         121             :
         122        1536 :     call NUOPC_ModelGet(gcomp, importState=importState, exportState=exportState, rc=rc)
         123        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         124             :
         125             :     !--------------------------------
         126             :     ! determine necessary toggles for below
         127             :     !--------------------------------
         128             :
         129        1536 :     call NUOPC_CompAttributeGet(gcomp, name='flds_co2a', value=cvalue, rc=rc)
         130        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         131        1536 :     read(cvalue,*) flds_co2a
         132        1536 :     if (masterproc) write(iulog,'(a)') trim(subname)//'flds_co2a = '// trim(cvalue)
         133             :
         134        1536 :     call NUOPC_CompAttributeGet(gcomp, name='flds_co2b', value=cvalue, rc=rc)
         135        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         136        1536 :     read(cvalue,*) flds_co2b
         137        1536 :     if (masterproc) write(iulog,'(a)') trim(subname)//'flds_co2b = '// trim(cvalue)
         138             :
         139        1536 :     call NUOPC_CompAttributeGet(gcomp, name='flds_co2c', value=cvalue, rc=rc)
         140        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         141        1536 :     read(cvalue,*) flds_co2c
         142        1536 :     if (masterproc) write(iulog,'(a)') trim(subname)//'flds_co2c = '// trim(cvalue)
         143             :
         144             :     !--------------------------------
         145             :     ! Export fields
         146             :     !--------------------------------
         147             :
         148        1536 :     if (masterproc) write(iulog,'(a)') trim(subname)//'export_fields '
         149             :
         150        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, trim(flds_scalar_name))
         151        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_topo'       )
         152        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_z'          )
         153        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_u'          )
         154        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_v'          )
         155        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_tbot'       )
         156        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_ptem'       )
         157        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_shum'       )
         158        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_pbot'       )
         159        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_dens'       )
         160        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_pslv'       )
         161        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_o3'         )
         162        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_rainc'    )
         163        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_rainl'    )
         164        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_snowc'    )
         165        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_snowl'    )
         166        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_lwdn'     )
         167        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_swndr'    )
         168        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_swvdr'    )
         169        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_swndf'    )
         170        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_swvdf'    )
         171        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_swnet'    )  ! only diagnostic
         172             :
         173             :     ! from atm - black carbon deposition fluxes (3)
         174             :     ! (1) => bcphidry, (2) => bcphodry, (3) => bcphiwet
         175        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_bcph', ungridded_lbound=1, ungridded_ubound=3)
         176             :
         177             :     ! from atm - organic carbon deposition fluxes (3)
         178             :     ! (1) => ocphidry, (2) => ocphodry, (3) => ocphiwet
         179        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_ocph', ungridded_lbound=1, ungridded_ubound=3)
         180             :
         181             :     ! from atm - wet dust deposition frluxes (4 sizes)
         182             :     ! (1) => dstwet1, (2) => dstwet2, (3) => dstwet3, (4) => dstwet4
         183        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_dstwet', ungridded_lbound=1, ungridded_ubound=4)
         184             :
         185             :     ! from atm - dry dust deposition frluxes (4 sizes)
         186             :     ! (1) => dstdry1, (2) => dstdry2, (3) => dstdry3, (4) => dstdry4
         187        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_dstdry', ungridded_lbound=1, ungridded_ubound=4)
         188             :
         189        1536 :     call ESMF_LogWrite(subname//' export fields co2', ESMF_LOGMSG_INFO)
         190             :
         191             :     ! from atm co2 fields
         192        1536 :     if (flds_co2a .or. flds_co2b .or. flds_co2c) then
         193        1536 :        call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_co2prog' )
         194        1536 :        call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_co2diag' )
         195             :     end if
         196             :
         197        1536 :     if (ndep_nflds > 0) then
         198             :        ! The following is when CAM/WACCM computes ndep
         199           0 :        call set_active_Faxa_nhx(.true.)
         200           0 :        call set_active_Faxa_noy(.true.)
         201             :     else
         202             :        ! The following is used for reading in stream data, or for aquaplanet or simple model
         203             :        ! cases where the ndep fluxes are not used.
         204        1536 :        call set_active_Faxa_nhx(.false.)
         205        1536 :        call set_active_Faxa_noy(.false.)
         206             :     end if
         207             :     ! Assume that 2 fields are always sent as part of Faxa_ndep
         208        1536 :     call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Faxa_ndep', ungridded_lbound=1, ungridded_ubound=2)
         209             :
         210             :     ! lightning flash freq
         211        1536 :     if (atm_provides_lightning) then
         212        1536 :        call fldlist_add(fldsFrAtm_num, fldsFrAtm, 'Sa_lightning')
         213             :     end if
         214             :
         215             :     ! Now advertise above export fields
         216        1536 :     if (masterproc) write(iulog,*) trim(subname)//' advertise export fields'
         217       47616 :     do n = 1,fldsFrAtm_num
         218       46080 :        call NUOPC_Advertise(exportState, standardName=fldsFrAtm(n)%stdname, &
         219       46080 :             TransferOfferGeomObject='will provide', rc=rc)
         220       47616 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         221             :     enddo
         222             :
         223             :     !-----------------
         224             :     ! Import fields
         225             :     !-----------------
         226             :
         227        1536 :     if (masterproc) write(iulog,'(a)') trim(subname)//' import fields '
         228             :
         229        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, trim(flds_scalar_name))
         230        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_anidr'  )
         231        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_avsdf'  )
         232        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_anidf'  )
         233        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_avsdr'  )
         234        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_lfrac'  )
         235        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Si_ifrac'  )
         236        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_ofrac'  )
         237        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_tref'   )
         238        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_qref'   )
         239        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_t'      )
         240        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_t'      )
         241        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_fv'     );  call set_active_Sl_fv(.true.)
         242        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_ram1'   );  call set_active_Sl_ram1(.true.)
         243        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_snowh'  )
         244        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Si_snowh'  )
         245        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_ssq'    )
         246        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_re'     )
         247        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_ustar'  )
         248        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sx_u10'    )
         249        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_ugustOut')
         250        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'So_u10withGust')
         251        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_taux' )
         252        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_tauy' )
         253        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_lat'  )
         254        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_sen'  )
         255        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_lwup' )
         256        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faxx_evap' )
         257             :
         258             :     ! dust fluxes from land (4 sizes)
         259        1536 :     call fldlist_add(fldsToAtm_num, fldsToAtm, 'Fall_flxdst', ungridded_lbound=1, ungridded_ubound=4)
         260        1536 :     call set_active_Fall_flxdst1(.true.)
         261             :
         262             :     ! co2 fields from land and ocean
         263        1536 :     if (flds_co2b .or. flds_co2c) then
         264           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Fall_fco2_lnd')
         265           0 :        call set_active_Fall_fco2_lnd(.true.)
         266             :     end if
         267        1536 :     if (flds_co2c) then
         268           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Faoo_fco2_ocn')
         269           0 :        call set_active_Faoo_fco2_ocn(.true.)
         270             :     end if
         271             :
         272             :     ! dry deposition velocities from land - ALSO initialize drydep here
         273        1536 :     if (drydep_nflds > 0) then
         274           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_ddvel', ungridded_lbound=1, ungridded_ubound=drydep_nflds)
         275             :     end if
         276             :
         277             :     ! MEGAN VOC emissions fluxes from land
         278        1536 :     if (megan_nflds > 0) then
         279           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Fall_voc', ungridded_lbound=1, ungridded_ubound=megan_nflds)
         280           0 :        call set_active_Fall_flxvoc(.true.)
         281             :     end if
         282             :
         283             :     ! fire emissions fluxes from land
         284        1536 :     if (emis_nflds > 0) then
         285           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Fall_fire', ungridded_lbound=1, ungridded_ubound=emis_nflds)
         286           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_fztop')
         287           0 :        call set_active_Fall_flxfire(.true.)
         288             :     end if
         289             :
         290             :     ! CARMA volumetric soil water from land
         291        1536 :     if (carma_fields /= ' ') then
         292           0 :        call fldlist_add(fldsToAtm_num, fldsToAtm, 'Sl_soilw') ! optional for carma
         293           0 :        call set_active_Sl_soilw(.true.) ! check for carma
         294             :     end if
         295             :
         296             :     ! ------------------------------------------
         297             :     ! Now advertise above import fields
         298             :     ! ------------------------------------------
         299        1536 :     call ESMF_LogWrite(trim(subname)//' advertise import fields ', ESMF_LOGMSG_INFO)
         300       46080 :     do n = 1,fldsToAtm_num
         301       44544 :        call NUOPC_Advertise(importState, standardName=fldsToAtm(n)%stdname, &
         302       44544 :             TransferOfferGeomObject='will provide', rc=rc)
         303       46080 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         304             :     enddo
         305             :
         306        3072 :   end subroutine advertise_fields
         307             :
         308             :   !===============================================================================
         309             :
         310        1536 :   subroutine realize_fields(gcomp, Emesh, flds_scalar_name, flds_scalar_num, single_column, rc)
         311             :
         312             :     use ESMF      , only : ESMF_MeshGet, ESMF_StateGet
         313             :     use ESMF      , only : ESMF_FieldRegridGetArea,ESMF_FieldGet
         314             :     use ppgrid    , only : pcols, begchunk, endchunk
         315             :     use phys_grid , only : get_area_all_p, get_ncols_p
         316             :
         317             :     ! input/output variables
         318             :     type(ESMF_GridComp) , intent(inout) :: gcomp
         319             :     type(ESMF_Mesh)     , intent(in)    :: Emesh
         320             :     character(len=*)    , intent(in)    :: flds_scalar_name
         321             :     integer             , intent(in)    :: flds_scalar_num
         322             :     logical             , intent(in)    :: single_column
         323             :     integer             , intent(out)   :: rc
         324             :
         325             :     ! local variables
         326             :     type(ESMF_State)      :: importState
         327             :     type(ESMF_State)      :: exportState
         328             :     type(ESMF_Field)      :: lfield
         329             :     integer               :: numOwnedElements
         330             :     integer               :: c,i,n,ncols
         331        1536 :     real(r8), allocatable :: mesh_areas(:)
         332        1536 :     real(r8), allocatable :: model_areas(:)
         333        1536 :     real(r8), allocatable :: area(:)
         334        1536 :     real(r8), pointer     :: dataptr(:)
         335             :     real(r8)              :: max_mod2med_areacor
         336             :     real(r8)              :: max_med2mod_areacor
         337             :     real(r8)              :: min_mod2med_areacor
         338             :     real(r8)              :: min_med2mod_areacor
         339             :     real(r8)              :: max_mod2med_areacor_glob
         340             :     real(r8)              :: max_med2mod_areacor_glob
         341             :     real(r8)              :: min_mod2med_areacor_glob
         342             :     real(r8)              :: min_med2mod_areacor_glob
         343             :     character(len=cl)     :: cvalue
         344             :     character(len=cl)     :: mesh_atm
         345             :     character(len=cl)     :: mesh_lnd
         346             :     character(len=cl)     :: mesh_ocn
         347             :     logical               :: samegrid_atm_lnd_ocn
         348             :     character(len=*), parameter :: subname='(atm_import_export:realize_fields)'
         349             :     !---------------------------------------------------------------------------
         350             :
         351        1536 :     rc = ESMF_SUCCESS
         352             :
         353        1536 :     call ESMF_LogWrite(subname//' called', ESMF_LOGMSG_INFO)
         354             :
         355        1536 :     call NUOPC_ModelGet(gcomp, importState=importState, exportState=exportState, rc=rc)
         356        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         357             :
         358             :     call fldlist_realize( &
         359             :          state=ExportState, &
         360             :          fldList=fldsFrAtm, &
         361             :          numflds=fldsFrAtm_num, &
         362             :          flds_scalar_name=flds_scalar_name, &
         363             :          flds_scalar_num=flds_scalar_num, &
         364             :          tag=subname//':camExport',&
         365        1536 :          mesh=Emesh, rc=rc)
         366        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         367             :
         368             :     call fldlist_realize( &
         369             :          state=importState, &
         370             :          fldList=fldsToAtm, &
         371             :          numflds=fldsToAtm_num, &
         372             :          flds_scalar_name=flds_scalar_name, &
         373             :          flds_scalar_num=flds_scalar_num, &
         374             :          tag=subname//':camImport',&
         375        1536 :          mesh=Emesh, rc=rc)
         376        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         377             :
         378             :     ! Determine if atm/lnd/ocn are on the same grid - if so set area correction factors to 1
         379        1536 :     call NUOPC_CompAttributeGet(gcomp, name='mesh_atm', value=mesh_atm, rc=rc)
         380        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         381        1536 :     call NUOPC_CompAttributeGet(gcomp, name='mesh_lnd', value=mesh_lnd, rc=rc)
         382        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         383        1536 :     call NUOPC_CompAttributeGet(gcomp, name='mesh_ocn', value=mesh_ocn, rc=rc)
         384        1536 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         385             :
         386        1536 :     samegrid_atm_lnd_ocn = .false.
         387             :     if ( trim(mesh_lnd) /= 'UNSET' .and. trim(mesh_atm) == trim(mesh_lnd) .and. &
         388        1536 :          trim(mesh_ocn) /= 'UNSET' .and. trim(mesh_atm) == trim(mesh_ocn)) then
         389             :        samegrid_atm_lnd_ocn = .true.
         390           0 :     elseif ( trim(mesh_lnd) == 'UNSET' .and. trim(mesh_atm) == trim(mesh_ocn)) then
         391             :        samegrid_atm_lnd_ocn = .true.
         392           0 :     elseif ( trim(mesh_ocn) == 'UNSET' .and. trim(mesh_atm) == trim(mesh_lnd)) then
         393           0 :        samegrid_atm_lnd_ocn = .true.
         394             :     end if
         395             :
         396             :     ! allocate area correction factors
         397        1536 :     call ESMF_MeshGet(Emesh, numOwnedElements=numOwnedElements, rc=rc)
         398        1536 :     if (chkerr(rc,__LINE__,u_FILE_u)) return
         399        4608 :     allocate (mod2med_areacor(numOwnedElements))
         400        3072 :     allocate (med2mod_areacor(numOwnedElements))
         401             :
         402        1536 :     if (single_column .or. samegrid_atm_lnd_ocn) then
         403             :
         404       98736 :        mod2med_areacor(:) = 1._r8
         405       98736 :        med2mod_areacor(:) = 1._r8
         406             :
         407             :     else
         408             :
         409             :        ! Determine areas for regridding
         410           0 :        call ESMF_StateGet(exportState, itemName=trim(fldsFrAtm(2)%stdname), field=lfield, rc=rc)
         411           0 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         412           0 :        call ESMF_FieldRegridGetArea(lfield, rc=rc)
         413           0 :        if (chkerr(rc,__LINE__,u_FILE_u)) return
         414           0 :        call ESMF_FieldGet(lfield, farrayPtr=dataptr, rc=rc)
         415           0 :        if (chkerr(rc,__LINE__,u_FILE_u)) return
         416           0 :        allocate(mesh_areas(numOwnedElements))
         417           0 :        mesh_areas(:) = dataptr(:)
         418             :
         419             :        ! Determine model areas
         420           0 :        allocate(model_areas(numOwnedElements))
         421           0 :        allocate(area(numOwnedElements))
         422           0 :        n = 0
         423           0 :        do c = begchunk, endchunk
         424           0 :           ncols = get_ncols_p(c)
         425           0 :           call get_area_all_p(c, ncols, area)
         426           0 :           do i = 1,ncols
         427           0 :              n = n + 1
         428           0 :              model_areas(n) = area(i)
         429             :           end do
         430             :        end do
         431           0 :        deallocate(area)
         432             :
         433             :        ! Determine flux correction factors (module variables)
         434           0 :        do n = 1,numOwnedElements
         435           0 :           mod2med_areacor(n) = model_areas(n) / mesh_areas(n)
         436           0 :           med2mod_areacor(n) = 1._r8 / mod2med_areacor(n)
         437             :        end do
         438           0 :        deallocate(model_areas)
         439           0 :        deallocate(mesh_areas)
         440             :
         441             :     end if
         442             :
         443      100272 :     min_mod2med_areacor = minval(mod2med_areacor)
         444      100272 :     max_mod2med_areacor = maxval(mod2med_areacor)
         445      100272 :     min_med2mod_areacor = minval(med2mod_areacor)
         446      100272 :     max_med2mod_areacor = maxval(med2mod_areacor)
         447        1536 :     call shr_mpi_max(max_mod2med_areacor, max_mod2med_areacor_glob, mpicom)
         448        1536 :     call shr_mpi_min(min_mod2med_areacor, min_mod2med_areacor_glob, mpicom)
         449        1536 :     call shr_mpi_max(max_med2mod_areacor, max_med2mod_areacor_glob, mpicom)
         450        1536 :     call shr_mpi_min(min_med2mod_areacor, min_med2mod_areacor_glob, mpicom)
         451             :
         452        1536 :     if (masterproc) then
         453           2 :        write(iulog,'(2A,2g23.15,A )') trim(subname),' :  min_mod2med_areacor, max_mod2med_areacor ',&
         454           4 :             min_mod2med_areacor_glob, max_mod2med_areacor_glob, 'CAM'
         455           2 :        write(iulog,'(2A,2g23.15,A )') trim(subname),' :  min_med2mod_areacor, max_med2mod_areacor ',&
         456           4 :             min_med2mod_areacor_glob, max_med2mod_areacor_glob, 'CAM'
         457             :     end if
         458             :
         459        1536 :     call ESMF_LogWrite(trim(subname)//' done', ESMF_LOGMSG_INFO)
         460             :
         461        6144 :   end subroutine realize_fields
         462             :
         463             :   !===============================================================================
         464             :
         465      740352 :   subroutine import_fields( gcomp, cam_in, restart_init, rc)
         466             :
         467             :     ! -----------------------------------------------------
         468             :     ! Set field pointers in import state and
         469             :     ! copy from field pointer to chunk array data structure
         470             :     ! -----------------------------------------------------
         471             :
         472        1536 :     use camsrfexch        , only : cam_in_t
         473             :     use phys_grid         , only : get_ncols_p
         474             :     use ppgrid            , only : begchunk, endchunk
         475             :     use shr_const_mod     , only : shr_const_stebol
         476             :     use co2_cycle         , only : c_i, co2_readFlux_ocn, co2_readFlux_fuel
         477             :     use co2_cycle         , only : co2_transport, co2_time_interp_ocn, co2_time_interp_fuel
         478             :     use co2_cycle         , only : data_flux_ocn, data_flux_fuel
         479             :     use physconst         , only : mwco2
         480             :     use time_manager      , only : is_first_step, get_nstep
         481             :
         482             :     ! input/output variabes
         483             :     type(ESMF_GridComp)               :: gcomp
         484             :     type(cam_in_t)    , intent(inout) :: cam_in(begchunk:endchunk)
         485             :     logical, optional , intent(in)    :: restart_init
         486             :     integer           , intent(out)   :: rc
         487             :
         488             :     ! local variables
         489             :     type(ESMF_State)   :: importState
         490             :     integer            :: i,n,c,g, num  ! indices
         491             :     integer            :: ncols         ! number of columns
         492             :     integer            :: nstep
         493             :     logical            :: overwrite_flds
         494             :     logical            :: exists
         495             :     logical            :: exists_fco2_ocn
         496             :     logical            :: exists_fco2_lnd
         497             :     character(len=128) :: fldname
         498      370176 :     real(r8), pointer  :: fldptr2d(:,:)
         499      370176 :     real(r8), pointer  :: fldptr1d(:)
         500      370176 :     real(r8), pointer  :: fldptr_lat(:)
         501      370176 :     real(r8), pointer  :: fldptr_lwup(:)
         502      370176 :     real(r8), pointer  :: fldptr_avsdr(:)
         503      370176 :     real(r8), pointer  :: fldptr_anidr(:)
         504      370176 :     real(r8), pointer  :: fldptr_avsdf(:)
         505      370176 :     real(r8), pointer  :: fldptr_anidf(:)
         506      370176 :     real(r8), pointer  :: fldptr_tsurf(:)
         507      370176 :     real(r8), pointer  :: fldptr_tocn(:)
         508      370176 :     real(r8), pointer  :: fldptr_tref(:)
         509      370176 :     real(r8), pointer  :: fldptr_qref(:)
         510      370176 :     real(r8), pointer  :: fldptr_u10(:)
         511      370176 :     real(r8), pointer  :: fldptr_snowhland(:)
         512      370176 :     real(r8), pointer  :: fldptr_snowhice(:)
         513      370176 :     real(r8), pointer  :: fldptr_ifrac(:)
         514      370176 :     real(r8), pointer  :: fldptr_ofrac(:)
         515      370176 :     real(r8), pointer  :: fldptr_lfrac(:)
         516      370176 :     real(r8), pointer  :: fldptr_taux(:)
         517      370176 :     real(r8), pointer  :: fldptr_tauy(:)
         518      370176 :     real(r8), pointer  :: fldptr_sen(:)
         519      370176 :     real(r8), pointer  :: fldptr_evap(:)
         520             :     logical, save      :: first_time = .true.
         521             :     character(len=*), parameter :: subname='(atm_import_export:import_fields)'
         522             :     !---------------------------------------------------------------------------
         523             :
         524      370176 :     rc = ESMF_SUCCESS
         525             :
         526             :     ! Get import state
         527      370176 :     call NUOPC_ModelGet(gcomp, importState=importState, rc=rc)
         528      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         529             :
         530             :     ! don't overwrite fields if invoked during the initialization phase
         531             :     ! of a 'continue' or 'branch' run type with data from .rs file
         532      370176 :     overwrite_flds = .true.
         533      370176 :     if (present(restart_init)) overwrite_flds = .not. restart_init
         534             :
         535             :     !--------------------------
         536             :     ! Required atmosphere input fields
         537             :     !--------------------------
         538             :
         539         768 :     if (overwrite_flds) then
         540      369408 :        call state_getfldptr(importState, 'Faxx_taux', fldptr=fldptr_taux, rc=rc)
         541      369408 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         542      369408 :        call state_getfldptr(importState, 'Faxx_tauy', fldptr=fldptr_tauy, rc=rc)
         543      369408 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         544      369408 :        call state_getfldptr(importState, 'Faxx_sen' , fldptr=fldptr_sen, rc=rc)
         545      369408 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         546      369408 :        call state_getfldptr(importState, 'Faxx_evap', fldptr=fldptr_evap, rc=rc)
         547      369408 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
         548      369408 :        g = 1
         549     1858584 :        do c = begchunk,endchunk
         550    25235184 :           do i = 1,get_ncols_p(c)
         551    23376600 :              cam_in(c)%wsx(i)    = -fldptr_taux(g) * med2mod_areacor(g)
         552    23376600 :              cam_in(c)%wsy(i)    = -fldptr_tauy(g) * med2mod_areacor(g)
         553    23376600 :              cam_in(c)%shf(i)    = -fldptr_sen(g)  * med2mod_areacor(g)
         554    23376600 :              cam_in(c)%cflx(i,1) = -fldptr_evap(g) * med2mod_areacor(g)
         555    24865776 :              g = g + 1
         556             :           end do
         557             :        end do
         558             :     end if  ! end of overwrite_flds
         559             :
         560      370176 :     call state_getfldptr(importState, 'Faxx_lat', fldptr=fldptr_lat, rc=rc)
         561      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         562      370176 :     call state_getfldptr(importState, 'Faxx_lwup', fldptr=fldptr_lwup, rc=rc)
         563      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         564      370176 :     call state_getfldptr(importState, 'Sx_avsdr', fldptr=fldptr_avsdr, rc=rc)
         565      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         566      370176 :     call state_getfldptr(importState, 'Sx_anidr', fldptr=fldptr_anidr, rc=rc)
         567      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         568      370176 :     call state_getfldptr(importState, 'Sx_avsdf', fldptr=fldptr_avsdf, rc=rc)
         569      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         570      370176 :     call state_getfldptr(importState, 'Sx_anidf', fldptr=fldptr_anidf, rc=rc)
         571      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         572      370176 :     call state_getfldptr(importState, 'Sx_t', fldptr=fldptr_tsurf, rc=rc)
         573      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         574      370176 :     call state_getfldptr(importState, 'So_t', fldptr=fldptr_tocn, rc=rc)
         575      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         576      370176 :     call state_getfldptr(importState, 'Sl_snowh', fldptr=fldptr_snowhland, rc=rc)
         577      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         578      370176 :     call state_getfldptr(importState, 'Si_snowh', fldptr=fldptr_snowhice,  rc=rc)
         579      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         580      370176 :     call state_getfldptr(importState, 'Sx_tref', fldptr=fldptr_tref, rc=rc)
         581      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         582      370176 :     call state_getfldptr(importState, 'Sx_qref', fldptr=fldptr_qref, rc=rc)
         583      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         584      370176 :     call state_getfldptr(importState, 'Sx_u10', fldptr=fldptr_u10, rc=rc)
         585      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         586      370176 :     call state_getfldptr(importState, 'Si_ifrac', fldptr=fldptr_ifrac, rc=rc)
         587      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         588      370176 :     call state_getfldptr(importState, 'So_ofrac', fldptr=fldptr_ofrac, rc=rc)
         589      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         590      370176 :     call state_getfldptr(importState, 'Sl_lfrac', fldptr=fldptr_lfrac, rc=rc)
         591      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         592             :
         593             :     ! Only do area correction on fluxes
         594      370176 :     g = 1
         595     1862448 :     do c = begchunk,endchunk
         596    25287648 :        do i = 1,get_ncols_p(c)
         597    23425200 :           cam_in(c)%lhf(i)       = -fldptr_lat(g)  * med2mod_areacor(g)
         598    23425200 :           cam_in(c)%lwup(i)      = -fldptr_lwup(g) * med2mod_areacor(g)
         599    23425200 :           cam_in(c)%asdir(i)     =  fldptr_avsdr(g)
         600    23425200 :           cam_in(c)%aldir(i)     =  fldptr_anidr(g)
         601    23425200 :           cam_in(c)%asdif(i)     =  fldptr_avsdf(g)
         602    23425200 :           cam_in(c)%aldif(i)     =  fldptr_anidf(g)
         603    23425200 :           cam_in(c)%ts(i)        =  fldptr_tsurf(g)
         604    23425200 :           cam_in(c)%sst(i)       =  fldptr_tocn(g)
         605    23425200 :           cam_in(c)%tref(i)      =  fldptr_tref(g)
         606    23425200 :           cam_in(c)%qref(i)      =  fldptr_qref(g)
         607    23425200 :           cam_in(c)%u10(i)       =  fldptr_u10(g)
         608    23425200 :           cam_in(c)%snowhland(i) =  fldptr_snowhland(g)
         609    23425200 :           cam_in(c)%snowhice(i)  =  fldptr_snowhice(g)
         610    23425200 :           cam_in(c)%icefrac(i)   =  fldptr_ifrac(g)
         611    23425200 :           cam_in(c)%ocnfrac(i)   =  fldptr_ofrac(g)
         612    23425200 :           cam_in(c)%landfrac(i)  =  fldptr_lfrac(g)
         613    24917472 :           g = g + 1
         614             :        end do
         615             :     end do
         616             :
         617             :     ! Optional fields
         618             :
         619      370176 :     call state_getfldptr(importState, 'Sl_ram1', fldptr=fldptr1d, exists=exists, rc=rc)
         620      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         621      370176 :     if (exists) then
         622      370176 :        g = 1
         623     1862448 :        do c = begchunk,endchunk
         624     1862448 :           if ( associated(cam_in(c)%ram1) ) then
         625    24917472 :              do i = 1, get_ncols_p(c)
         626    23425200 :                 cam_in(c)%ram1(i) = fldptr1d(g)
         627    24917472 :                 g = g + 1
         628             :              end do
         629             :           end if
         630             :        end do
         631             :     end if
         632             :
         633      370176 :     call state_getfldptr(importState, 'Sl_fv', fldptr=fldptr1d, exists=exists, rc=rc)
         634      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         635      370176 :     if (exists) then
         636      370176 :        g = 1
         637     1862448 :        do c = begchunk,endchunk
         638     1862448 :           if ( associated(cam_in(c)%fv) ) then
         639    24917472 :              do i = 1,get_ncols_p(c)
         640    23425200 :                 cam_in(c)%fv(i) = fldptr1d(g)
         641    24917472 :                 g = g + 1
         642             :              end do
         643             :           end if
         644             :        end do
         645             :     end if
         646             :
         647             :     ! For CARMA - soil water from land
         648      370176 :     call state_getfldptr(importState, 'Sl_soilw', fldptr=fldptr1d, exists=exists, rc=rc)
         649      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         650      370176 :     if (exists) then
         651           0 :        g = 1
         652           0 :        do c = begchunk,endchunk
         653           0 :           if ( associated(cam_in(c)%soilw)) then
         654           0 :              do i = 1,get_ncols_p(c)
         655           0 :                 cam_in(c)%soilw(i) = fldptr1d(g)
         656           0 :                 g = g+1
         657             :              end do
         658             :           end if
         659             :        end do
         660             :     end if
         661             :
         662             :     ! dry deposition fluxes from land
         663      370176 :     call state_getfldptr(importState, 'Fall_flxdst', fldptr2d=fldptr2d, exists=exists, rc=rc)
         664      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         665      370176 :     if (exists) then
         666      370176 :        g = 1
         667     1862448 :        do c = begchunk,endchunk
         668     1862448 :           if ( associated(cam_in(c)%dstflx) ) then
         669    24917472 :              do i = 1,get_ncols_p(c)
         670   117126000 :                 do n = 1, size(fldptr2d, dim=1)
         671   117126000 :                    cam_in(c)%dstflx(i,n) = fldptr2d(n,g) * med2mod_areacor(g)
         672             :                 end do
         673    24917472 :                 g = g + 1
         674             :              end do
         675             :           end if
         676             :        end do
         677             :     end if
         678             :
         679             :     ! MEGAN VOC emis fluxes from land
         680      370176 :     call state_getfldptr(importState, 'Fall_voc', fldptr2d=fldptr2d, exists=exists, rc=rc)
         681      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         682      370176 :     if (exists) then
         683           0 :        g = 1
         684           0 :        do c=begchunk,endchunk
         685           0 :           if ( associated(cam_in(c)%meganflx) ) then
         686           0 :              do i = 1,get_ncols_p(c)
         687           0 :                 do n = 1, size(fldptr2d, dim=1)
         688           0 :                    cam_in(c)%meganflx(i,n) = fldptr2d(n,g) * med2mod_areacor(g)
         689             :                 end do
         690           0 :                 g = g + 1
         691             :              end do
         692             :           end if
         693             :        end do
         694             :     end if
         695             :
         696             :     ! fire emission fluxes from land
         697      370176 :     call state_getfldptr(importState, 'Fall_fire', fldptr2d=fldptr2d, exists=exists, rc=rc)
         698      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         699      370176 :     if (exists) then
         700           0 :        g = 1
         701           0 :        do c = begchunk,endchunk
         702           0 :           if ( associated(cam_in(c)%fireflx) .and. associated(cam_in(c)%fireztop) ) then
         703           0 :              do i = 1,get_ncols_p(c)
         704           0 :                 do n = 1, size(fldptr2d, dim=1)
         705           0 :                    cam_in(c)%fireflx(i,n) = fldptr2d(n,g) * med2mod_areacor(g)
         706             :                 end do
         707           0 :                 g = g + 1
         708             :              end do
         709             :           end if
         710             :        end do
         711             :     end if
         712      370176 :     call state_getfldptr(importState, 'Sl_fztop', fldptr=fldptr1d, exists=exists, rc=rc)
         713      370176 :     if (exists) then
         714           0 :        g = 1
         715           0 :        do c = begchunk,endchunk
         716           0 :           do i = 1,get_ncols_p(c)
         717           0 :              cam_in(c)%fireztop(i) = fldptr1d(g)
         718           0 :              g = g + 1
         719             :           end do
         720             :        end do
         721             :     end if
         722             :
         723             :     ! dry dep velocities
         724      370176 :     call state_getfldptr(importState, 'Sl_ddvel', fldptr2d=fldptr2d, exists=exists, rc=rc)
         725      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         726      370176 :     if (exists) then
         727           0 :        g = 1
         728           0 :        do c = begchunk,endchunk
         729           0 :           do i = 1,get_ncols_p(c)
         730           0 :              do n = 1, size(fldptr2d, dim=1)
         731           0 :                 cam_in(c)%depvel(i,n) = fldptr2d(n,g)
         732             :              end do
         733           0 :              g = g + 1
         734             :           end do
         735             :        end do
         736             :     end if
         737             :
         738             :     ! fields needed to calculate water isotopes to ocean evaporation processes
         739      370176 :     call state_getfldptr(importState,  'So_ustar', fldptr=fldptr1d, exists=exists, rc=rc)
         740      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         741      370176 :     if (exists) then
         742      370176 :        g = 1
         743     1862448 :        do c = begchunk,endchunk
         744    25287648 :           do i = 1,get_ncols_p(c)
         745    23425200 :              cam_in(c)%ustar(i) = fldptr1d(g)
         746    24917472 :              g = g + 1
         747             :           end do
         748             :        end do
         749             :     end if
         750      370176 :     call state_getfldptr(importState,  'So_re', fldptr=fldptr1d, exists=exists, rc=rc)
         751      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         752      370176 :     if (exists) then
         753      370176 :        g = 1
         754     1862448 :        do c = begchunk,endchunk
         755    25287648 :           do i = 1,get_ncols_p(c)
         756    23425200 :              cam_in(c)%re(i)= fldptr1d(g)
         757    24917472 :              g = g + 1
         758             :           end do
         759             :        end do
         760             :     end if
         761      370176 :     call state_getfldptr(importState,  'So_ssq', fldptr=fldptr1d, exists=exists, rc=rc)
         762      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         763      370176 :     if (exists) then
         764      370176 :        g = 1
         765     1862448 :        do c = begchunk,endchunk
         766    25287648 :           do i = 1,get_ncols_p(c)
         767    23425200 :              cam_in(c)%ssq(i) = fldptr1d(g)
         768    24917472 :              g = g + 1
         769             :           end do
         770             :        end do
         771             :     end if
         772             :
         773      370176 :     call state_getfldptr(importState,  'So_ugustOut', fldptr=fldptr1d, exists=exists, rc=rc)
         774      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         775      370176 :     if (exists) then
         776      370176 :        g = 1
         777     1862448 :        do c = begchunk,endchunk
         778    25287648 :           do i = 1,get_ncols_p(c)
         779    23425200 :              cam_in(c)%ugustOut(i) = fldptr1d(g)
         780    24917472 :              g = g + 1
         781             :           end do
         782             :        end do
         783             :     end if
         784             :
         785      370176 :     call state_getfldptr(importState,  'So_u10withGust', fldptr=fldptr1d, exists=exists, rc=rc)
         786      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         787      370176 :     if (exists) then
         788      370176 :        g = 1
         789     1862448 :        do c = begchunk,endchunk
         790    25287648 :           do i = 1,get_ncols_p(c)
         791    23425200 :              cam_in(c)%u10withGusts(i) = fldptr1d(g)
         792    24917472 :              g = g + 1
         793             :           end do
         794             :        end do
         795             :     end if
         796             :
         797             :     ! bgc scenarios
         798      370176 :     call state_getfldptr(importState,  'Fall_fco2_lnd', fldptr=fldptr1d, exists=exists_fco2_lnd, rc=rc)
         799      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         800      370176 :     if (exists_fco2_lnd) then
         801           0 :        g = 1
         802           0 :        do c = begchunk,endchunk
         803           0 :           do i = 1,get_ncols_p(c)
         804           0 :              cam_in(c)%fco2_lnd(i) = -fldptr1d(g) * med2mod_areacor(g)
         805           0 :              g = g + 1
         806             :           end do
         807             :        end do
         808             :     end if
         809      370176 :     call state_getfldptr(importState,  'Faoo_fco2_ocn', fldptr=fldptr1d, exists=exists_fco2_ocn, rc=rc)
         810      370176 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         811      370176 :     if (exists_fco2_ocn) then
         812           0 :        g = 1
         813           0 :        do c = begchunk,endchunk
         814           0 :           do i = 1,get_ncols_p(c)
         815           0 :              cam_in(c)%fco2_ocn(i) = -fldptr1d(g) * med2mod_areacor(g)
         816           0 :              g = g + 1
         817             :           end do
         818             :        end do
         819             :     else
         820             :        ! Consistency check
         821      370176 :        if (co2_readFlux_ocn) then
         822           0 :           call shr_sys_abort(subname // ':: co2_readFlux_ocn and x2a_Faoo_fco2_ocn cannot both be active')
         823             :        end if
         824             :     end if
         825      370176 :     call state_getfldptr(importState,  'Faoo_dms_ocn', fldptr=fldptr1d, exists=exists, rc=rc)
         826      370176 :     if (exists) then
         827           0 :        g = 1
         828           0 :        do c = begchunk,endchunk
         829           0 :           do i = 1,get_ncols_p(c)
         830           0 :              cam_in(c)%fdms(i) = -fldptr1d(g) * med2mod_areacor(g)
         831           0 :              g = g + 1
         832             :           end do
         833             :        end do
         834             :     end if
         835             :
         836             :     ! -----------------------------------
         837             :     ! Get total co2 flux from components,
         838             :     ! -----------------------------------
         839             :
         840             :     ! Note - co2_transport determines if cam_in(c)%cflx(i,c_i(1:4)) is allocated
         841             :
         842      370176 :     if (co2_transport() .and. overwrite_flds) then
         843             :
         844             :        ! Interpolate in time for flux data read in
         845           0 :        if (co2_readFlux_ocn) then
         846           0 :           call co2_time_interp_ocn
         847             :        end if
         848           0 :        if (co2_readFlux_fuel) then
         849           0 :           call co2_time_interp_fuel
         850             :        end if
         851             :
         852             :        ! from ocn : data read in or from coupler or zero
         853             :        ! from fuel: data read in or zero
         854             :        ! from lnd : through coupler or zero
         855             :        ! all co2 fluxes in unit kgCO2/m2/s
         856             :
         857           0 :        do c=begchunk,endchunk
         858           0 :           do i=1, get_ncols_p(c)
         859             :
         860             :              ! co2 flux from ocn
         861           0 :              if (exists_fco2_ocn) then
         862           0 :                 cam_in(c)%cflx(i,c_i(1)) = cam_in(c)%fco2_ocn(i)
         863           0 :              else if (co2_readFlux_ocn) then
         864             :                 ! convert from molesCO2/m2/s to kgCO2/m2/s
         865           0 :                 cam_in(c)%cflx(i,c_i(1)) = &
         866           0 :                      -data_flux_ocn%co2flx(i,c)*(1._r8- cam_in(c)%landfrac(i))*mwco2*1.0e-3_r8
         867             :              else
         868           0 :                 cam_in(c)%cflx(i,c_i(1)) = 0._r8
         869             :              end if
         870             :
         871             :              ! co2 flux from fossil fuel
         872           0 :              if (co2_readFlux_fuel) then
         873           0 :                 cam_in(c)%cflx(i,c_i(2)) = data_flux_fuel%co2flx(i,c)
         874             :              else
         875           0 :                 cam_in(c)%cflx(i,c_i(2)) = 0._r8
         876             :              end if
         877             :
         878             :              ! co2 flux from land (cpl already multiplies flux by land fraction)
         879           0 :              if (exists_fco2_lnd) then
         880           0 :                 cam_in(c)%cflx(i,c_i(3)) = cam_in(c)%fco2_lnd(i)
         881             :              else
         882           0 :                 cam_in(c)%cflx(i,c_i(3)) = 0._r8
         883             :              end if
         884             :
         885             :              ! merged co2 flux
         886           0 :              cam_in(c)%cflx(i,c_i(4)) = cam_in(c)%cflx(i,c_i(1)) + cam_in(c)%cflx(i,c_i(2)) + cam_in(c)%cflx(i,c_i(3))
         887             :           end do
         888             :        end do
         889             :     end if
         890             :
         891             :     ! if first step, determine longwave up flux from the surface temperature
         892      370176 :     if (first_time) then
         893        1536 :        if (is_first_step()) then
         894        3864 :           do c=begchunk, endchunk
         895       52464 :              do i=1, get_ncols_p(c)
         896       51696 :                 cam_in(c)%lwup(i) = shr_const_stebol*(cam_in(c)%ts(i)**4)
         897             :              end do
         898             :           end do
         899             :        end if
         900        1536 :        first_time = .false.
         901             :     end if
         902             :
         903      740352 :   end subroutine import_fields
         904             :
         905             :   !===============================================================================
         906             :
         907      743424 :   subroutine export_fields( gcomp, model_mesh, model_clock, cam_out, rc)
         908             :
         909             :     ! -----------------------------------------------------
         910             :     ! Set field pointers in export set
         911             :     ! Copy from chunk array data structure into state fldptr
         912             :     ! -----------------------------------------------------
         913             :
         914      370176 :     use camsrfexch   , only : cam_out_t
         915             :     use phys_grid    , only : get_ncols_p
         916             :     use ppgrid       , only : begchunk, endchunk
         917             :     use time_manager , only : is_first_step, get_nstep
         918             :     use spmd_utils   , only : masterproc
         919             :
         920             :     !-------------------------------
         921             :     ! Pack the export state
         922             :     !-------------------------------
         923             :
         924             :     ! input/output variables
         925             :     type(ESMF_GridComp)              :: gcomp
         926             :     type(ESMF_Mesh) , intent(in)     :: model_mesh
         927             :     type(ESMF_Clock), intent(in)     :: model_clock
         928             :     type(cam_out_t) , intent(inout)  :: cam_out(begchunk:endchunk)
         929             :     integer         , intent(out)    :: rc
         930             :
         931             :     ! local variables
         932             :     type(ESMF_State)  :: exportState
         933             :     type(ESMF_Clock)  :: clock
         934             :     integer           :: i,m,c,n,g  ! indices
         935             :     integer           :: ncols      ! Number of columns
         936             :     integer           :: nstep
         937             :     logical           :: exists
         938             :     real(r8)          :: scale_ndep
         939             :     ! 2d pointers
         940      371712 :     real(r8), pointer :: fldptr_ndep(:,:)
         941      371712 :     real(r8), pointer :: fldptr_bcph(:,:)  , fldptr_ocph(:,:)
         942      371712 :     real(r8), pointer :: fldptr_dstwet(:,:), fldptr_dstdry(:,:)
         943             :     ! 1d pointers
         944      371712 :     real(r8), pointer :: fldptr_soll(:)    , fldptr_sols(:)
         945      371712 :     real(r8), pointer :: fldptr_solld(:)   , fldptr_solsd(:)
         946      371712 :     real(r8), pointer :: fldptr_snowc(:)   , fldptr_snowl(:)
         947      371712 :     real(r8), pointer :: fldptr_rainc(:)   , fldptr_rainl(:)
         948      371712 :     real(r8), pointer :: fldptr_lwdn(:)    , fldptr_swnet(:)
         949      371712 :     real(r8), pointer :: fldptr_topo(:)    , fldptr_zbot(:)
         950      371712 :     real(r8), pointer :: fldptr_ubot(:)    , fldptr_vbot(:)
         951      371712 :     real(r8), pointer :: fldptr_pbot(:)    , fldptr_tbot(:)
         952      371712 :     real(r8), pointer :: fldptr_shum(:)    , fldptr_dens(:)
         953      371712 :     real(r8), pointer :: fldptr_ptem(:)    , fldptr_pslv(:)
         954      371712 :     real(r8), pointer :: fldptr_co2prog(:) , fldptr_co2diag(:)
         955      371712 :     real(r8), pointer :: fldptr_ozone(:)
         956      371712 :     real(r8), pointer :: fldptr_lght(:)
         957             :     character(len=*), parameter :: subname='(atm_import_export:export_fields)'
         958             :     !---------------------------------------------------------------------------
         959             :
         960      371712 :     rc = ESMF_SUCCESS
         961             :
         962             :     ! Get export state
         963      371712 :     call NUOPC_ModelGet(gcomp, exportState=exportState, rc=rc)
         964      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         965             :
         966             :     ! required export state variables
         967      371712 :     call state_getfldptr(exportState, 'Sa_topo', fldptr=fldptr_topo, rc=rc)
         968      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         969      371712 :     call state_getfldptr(exportState, 'Sa_z'   , fldptr=fldptr_zbot, rc=rc)
         970      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         971      371712 :     call state_getfldptr(exportState, 'Sa_u'   , fldptr=fldptr_ubot, rc=rc)
         972      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         973      371712 :     call state_getfldptr(exportState, 'Sa_v'   , fldptr=fldptr_vbot, rc=rc)
         974      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         975      371712 :     call state_getfldptr(exportState, 'Sa_tbot', fldptr=fldptr_tbot, rc=rc)
         976      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         977      371712 :     call state_getfldptr(exportState, 'Sa_pbot', fldptr=fldptr_pbot, rc=rc)
         978      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         979      371712 :     call state_getfldptr(exportState, 'Sa_shum', fldptr=fldptr_shum, rc=rc)
         980      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         981      371712 :     call state_getfldptr(exportState, 'Sa_dens', fldptr=fldptr_dens, rc=rc)
         982      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         983      371712 :     call state_getfldptr(exportState, 'Sa_ptem', fldptr=fldptr_ptem, rc=rc)
         984      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         985      371712 :     call state_getfldptr(exportState, 'Sa_pslv', fldptr=fldptr_pslv, rc=rc)
         986      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
         987      371712 :     g = 1
         988     1870176 :     do c = begchunk,endchunk
         989    25392576 :        do i = 1,get_ncols_p(c)
         990    23522400 :           fldptr_topo(g) = cam_out(c)%topo(i)
         991    23522400 :           fldptr_zbot(g) = cam_out(c)%zbot(i)
         992    23522400 :           fldptr_ubot(g) = cam_out(c)%ubot(i)
         993    23522400 :           fldptr_vbot(g) = cam_out(c)%vbot(i)
         994    23522400 :           fldptr_pbot(g) = cam_out(c)%pbot(i)
         995    23522400 :           fldptr_tbot(g) = cam_out(c)%tbot(i)
         996    23522400 :           fldptr_shum(g) = cam_out(c)%qbot(i,1)
         997    23522400 :           fldptr_dens(g) = cam_out(c)%rho(i)
         998    23522400 :           fldptr_ptem(g) = cam_out(c)%thbot(i)
         999    23522400 :           fldptr_pslv(g) = cam_out(c)%psl(i)
        1000    25020864 :           g = g + 1
        1001             :        end do
        1002             :     end do
        1003             :
        1004             :     ! required export flux variables
        1005      371712 :     call state_getfldptr(exportState, 'Faxa_swnet', fldptr=fldptr_swnet, rc=rc)
        1006      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1007      371712 :     call state_getfldptr(exportState, 'Faxa_lwdn' , fldptr=fldptr_lwdn , rc=rc)
        1008      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1009      371712 :     call state_getfldptr(exportState, 'Faxa_rainc', fldptr=fldptr_rainc, rc=rc)
        1010      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1011      371712 :     call state_getfldptr(exportState, 'Faxa_rainl', fldptr=fldptr_rainl, rc=rc)
        1012      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1013      371712 :     call state_getfldptr(exportState, 'Faxa_snowc', fldptr=fldptr_snowc, rc=rc)
        1014      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1015      371712 :     call state_getfldptr(exportState, 'Faxa_snowl', fldptr=fldptr_snowl, rc=rc)
        1016      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1017      371712 :     call state_getfldptr(exportState, 'Faxa_swndr', fldptr=fldptr_soll, rc=rc)
        1018      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1019      371712 :     call state_getfldptr(exportState, 'Faxa_swvdr', fldptr=fldptr_sols, rc=rc)
        1020      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1021      371712 :     call state_getfldptr(exportState, 'Faxa_swndf', fldptr=fldptr_solld, rc=rc)
        1022      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1023      371712 :     call state_getfldptr(exportState, 'Faxa_swvdf', fldptr=fldptr_solsd, rc=rc)
        1024      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1025      371712 :     g = 1
        1026     1870176 :     do c = begchunk,endchunk
        1027    25392576 :        do i = 1,get_ncols_p(c)
        1028    23522400 :           fldptr_lwdn(g)  = cam_out(c)%flwds(i) * mod2med_areacor(g)
        1029    23522400 :           fldptr_swnet(g) = cam_out(c)%netsw(i) * mod2med_areacor(g)
        1030    23522400 :           fldptr_snowc(g) = cam_out(c)%precsc(i)*1000._r8 * mod2med_areacor(g)
        1031    23522400 :           fldptr_snowl(g) = cam_out(c)%precsl(i)*1000._r8 * mod2med_areacor(g)
        1032    23522400 :           fldptr_rainc(g) = (cam_out(c)%precc(i) - cam_out(c)%precsc(i))*1000._r8 * mod2med_areacor(g)
        1033    23522400 :           fldptr_rainl(g) = (cam_out(c)%precl(i) - cam_out(c)%precsl(i))*1000._r8 * mod2med_areacor(g)
        1034    23522400 :           fldptr_soll(g)  = cam_out(c)%soll(i)  * mod2med_areacor(g)
        1035    23522400 :           fldptr_sols(g)  = cam_out(c)%sols(i)  * mod2med_areacor(g)
        1036    23522400 :           fldptr_solld(g) = cam_out(c)%solld(i) * mod2med_areacor(g)
        1037    23522400 :           fldptr_solsd(g) = cam_out(c)%solsd(i) * mod2med_areacor(g)
        1038    25020864 :           g = g + 1
        1039             :        end do
        1040             :     end do
        1041             :
        1042             :     ! aerosol deposition fluxes
        1043      371712 :     call state_getfldptr(exportState, 'Faxa_bcph', fldptr2d=fldptr_bcph, rc=rc)
        1044      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1045      371712 :     call state_getfldptr(exportState, 'Faxa_ocph', fldptr2d=fldptr_ocph, rc=rc)
        1046      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1047      371712 :     call state_getfldptr(exportState, 'Faxa_dstdry', fldptr2d=fldptr_dstdry, rc=rc)
        1048      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1049      371712 :     call state_getfldptr(exportState, 'Faxa_dstwet', fldptr2d=fldptr_dstwet, rc=rc)
        1050      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1051             :     ! (1) => bcphidry, (2) => bcphodry, (3) => bcphiwet
        1052             :     ! (1) => ocphidry, (2) => ocphodry, (3) => ocphiwet
        1053      371712 :     g = 1
        1054     1870176 :     do c = begchunk,endchunk
        1055    25392576 :        do i = 1,get_ncols_p(c)
        1056    23522400 :           fldptr_bcph(1,g)   = cam_out(c)%bcphidry(i) * mod2med_areacor(g)
        1057    23522400 :           fldptr_bcph(2,g)   = cam_out(c)%bcphodry(i) * mod2med_areacor(g)
        1058    23522400 :           fldptr_bcph(3,g)   = cam_out(c)%bcphiwet(i) * mod2med_areacor(g)
        1059    23522400 :           fldptr_ocph(1,g)   = cam_out(c)%ocphidry(i) * mod2med_areacor(g)
        1060    23522400 :           fldptr_ocph(2,g)   = cam_out(c)%ocphodry(i) * mod2med_areacor(g)
        1061    23522400 :           fldptr_ocph(3,g)   = cam_out(c)%ocphiwet(i) * mod2med_areacor(g)
        1062    23522400 :           fldptr_dstdry(1,g) = cam_out(c)%dstdry1(i)  * mod2med_areacor(g)
        1063    23522400 :           fldptr_dstdry(2,g) = cam_out(c)%dstdry2(i)  * mod2med_areacor(g)
        1064    23522400 :           fldptr_dstdry(3,g) = cam_out(c)%dstdry3(i)  * mod2med_areacor(g)
        1065    23522400 :           fldptr_dstdry(4,g) = cam_out(c)%dstdry4(i)  * mod2med_areacor(g)
        1066    23522400 :           fldptr_dstwet(1,g) = cam_out(c)%dstwet1(i)  * mod2med_areacor(g)
        1067    23522400 :           fldptr_dstwet(2,g) = cam_out(c)%dstwet2(i)  * mod2med_areacor(g)
        1068    23522400 :           fldptr_dstwet(3,g) = cam_out(c)%dstwet3(i)  * mod2med_areacor(g)
        1069    23522400 :           fldptr_dstwet(4,g) = cam_out(c)%dstwet4(i)  * mod2med_areacor(g)
        1070    25020864 :           g = g + 1
        1071             :        end do
        1072             :     end do
        1073             :
        1074      371712 :     call state_getfldptr(exportState, 'Sa_o3', fldptr=fldptr_ozone, exists=exists, rc=rc)
        1075      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1076      371712 :     if (exists) then
        1077      371712 :        g = 1
        1078     1870176 :        do c = begchunk,endchunk
        1079    25392576 :           do i = 1,get_ncols_p(c)
        1080    23522400 :              fldptr_ozone(g) = cam_out(c)%ozone(i) ! atm ozone
        1081    25020864 :              g = g + 1
        1082             :           end do
        1083             :        end do
        1084             :     end if
        1085             :
        1086      371712 :     call state_getfldptr(exportState, 'Sa_lightning', fldptr=fldptr_lght, exists=exists, rc=rc)
        1087      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1088      371712 :     if (exists) then
        1089      371712 :        g = 1
        1090     1870176 :        do c = begchunk,endchunk
        1091    25392576 :           do i = 1,get_ncols_p(c)
        1092    23522400 :              fldptr_lght(g) = cam_out(c)%lightning_flash_freq(i) ! cloud-to-ground lightning flash frequency (/min)
        1093    25020864 :              g = g + 1
        1094             :           end do
        1095             :        end do
        1096             :     end if
        1097             :
        1098      371712 :     call state_getfldptr(exportState, 'Sa_co2prog', fldptr=fldptr_co2prog, exists=exists, rc=rc)
        1099      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1100      371712 :     if (exists) then
        1101      371712 :        g = 1
        1102     1870176 :        do c = begchunk,endchunk
        1103    25392576 :           do i = 1,get_ncols_p(c)
        1104    23522400 :              fldptr_co2prog(g) = cam_out(c)%co2prog(i) ! atm prognostic co2
        1105    25020864 :              g = g + 1
        1106             :           end do
        1107             :        end do
        1108             :     end if
        1109             :
        1110      371712 :     call state_getfldptr(exportState, 'Sa_co2diag', fldptr=fldptr_co2diag, exists=exists, rc=rc)
        1111      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1112      371712 :     if (exists) then
        1113      371712 :        g = 1
        1114     1870176 :        do c = begchunk,endchunk
        1115    25392576 :           do i = 1,get_ncols_p(c)
        1116    23522400 :              fldptr_co2diag(g) = cam_out(c)%co2diag(i) ! atm diagnostic co2
        1117    25020864 :              g = g + 1
        1118             :           end do
        1119             :        end do
        1120             :     end if
        1121             :
        1122      371712 :     call state_getfldptr(exportState, 'Faxa_ndep', fldptr2d=fldptr_ndep, rc=rc)
        1123      371712 :     if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1124      371712 :     if (.not. active_Faxa_nhx .and. .not. active_Faxa_noy) then
        1125             :
        1126             :        ! ndep fields not active (i.e., not computed by WACCM).  Either they are not needed,
        1127             :        ! or they are obtained from the ndep input stream.
        1128             :
        1129             :        ! The ndep_stream_nl namelist group is read in stream_ndep_init.  This sets whether
        1130             :        ! or not the stream will be used.
        1131      371712 :        if (.not. stream_ndep_is_initialized) then
        1132        1536 :           call stream_ndep_init(model_mesh, model_clock, rc)
        1133        1536 :           if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1134        1536 :           stream_ndep_is_initialized = .true.
        1135             :        end if
        1136             :
        1137      371712 :        if (use_ndep_stream) then
        1138             :
        1139             :          ! get ndep fluxes from the stream
        1140      371712 :          call stream_ndep_interp(cam_out, rc)
        1141      371712 :          if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1142             :          ! NDEP read from forcing is expected to be in units of gN/m2/sec - but the mediator
        1143             :          ! expects units of kgN/m2/sec
        1144             :          scale_ndep = .001_r8
        1145             :
        1146             :       else
        1147             :
        1148             :           ! ndep fluxes not used.  Set to zero.
        1149           0 :           do c = begchunk,endchunk
        1150           0 :              do i = 1,get_ncols_p(c)
        1151           0 :                 cam_out(c)%nhx_nitrogen_flx(i) = 0._r8
        1152           0 :                 cam_out(c)%noy_nitrogen_flx(i) = 0._r8
        1153             :              end do
        1154             :           end do
        1155             :           scale_ndep = 1._r8
        1156             :
        1157             :       end if
        1158             :
        1159             :     else
        1160             :
        1161             :        ! If waccm computes ndep, then its in units of kgN/m2/s - and the mediator expects
        1162             :        ! units of kgN/m2/sec, so the following conversion needs to happen
        1163             :        scale_ndep = 1._r8
        1164             :
        1165             :     end if
        1166             :
        1167      371712 :     g = 1
        1168     1870176 :     do c = begchunk,endchunk
        1169    25392576 :        do i = 1,get_ncols_p(c)
        1170    23522400 :           fldptr_ndep(1,g) = cam_out(c)%nhx_nitrogen_flx(i) * scale_ndep * mod2med_areacor(g)
        1171    23522400 :           fldptr_ndep(2,g) = cam_out(c)%noy_nitrogen_flx(i) * scale_ndep * mod2med_areacor(g)
        1172    25020864 :           g = g + 1
        1173             :        end do
        1174             :     end do
        1175             :
        1176      743424 :   end subroutine export_fields
        1177             :
        1178             :   !===============================================================================
        1179             :
        1180       90624 :   subroutine fldlist_add(num, fldlist, stdname, ungridded_lbound, ungridded_ubound)
        1181             :
        1182             :     ! input/otuput variables
        1183             :     integer            , intent(inout) :: num
        1184             :     type(fldlist_type) , intent(inout) :: fldlist(:)
        1185             :     character(len=*)   , intent(in)    :: stdname
        1186             :     integer, optional  , intent(in)    :: ungridded_lbound
        1187             :     integer, optional  , intent(in)    :: ungridded_ubound
        1188             :
        1189             :     ! local variables
        1190             :     character(len=*), parameter :: subname='(atm_import_export:fldlist_add)'
        1191             :     !-------------------------------------------------------------------------------
        1192             :
        1193             :     ! Set up a list of field information
        1194             :
        1195       90624 :     num = num + 1
        1196       90624 :     if (num > fldsMax) then
        1197             :        call ESMF_LogWrite(trim(subname)//": ERROR num > fldsMax "//trim(stdname), &
        1198           0 :             ESMF_LOGMSG_ERROR, line=__LINE__, file=__FILE__)
        1199           0 :        return
        1200             :     endif
        1201       90624 :     fldlist(num)%stdname = trim(stdname)
        1202             :
        1203       90624 :     if (present(ungridded_lbound) .and. present(ungridded_ubound)) then
        1204        9216 :        fldlist(num)%ungridded_lbound = ungridded_lbound
        1205        9216 :        fldlist(num)%ungridded_ubound = ungridded_ubound
        1206             :     end if
        1207             :
        1208      371712 :   end subroutine fldlist_add
        1209             :
        1210             :   !===============================================================================
        1211             :
        1212        3072 :   subroutine fldlist_realize(state, fldList, numflds, flds_scalar_name, flds_scalar_num, mesh, tag, rc)
        1213             :
        1214             :     use NUOPC , only : NUOPC_IsConnected, NUOPC_Realize
        1215             :     use ESMF  , only : ESMF_MeshLoc_Element, ESMF_FieldCreate, ESMF_TYPEKIND_R8
        1216             :     use ESMF  , only : ESMF_MAXSTR, ESMF_Field, ESMF_State, ESMF_Mesh, ESMF_StateRemove
        1217             :     use ESMF  , only : ESMF_LogFoundError, ESMF_LOGMSG_INFO, ESMF_SUCCESS
        1218             :     use ESMF  , only : ESMF_LogWrite, ESMF_LOGMSG_ERROR, ESMF_LOGERR_PASSTHRU
        1219             :
        1220             :     ! input/output variables
        1221             :     type(ESMF_State)    , intent(inout) :: state
        1222             :     type(fldlist_type) , intent(in)     :: fldList(:)
        1223             :     integer             , intent(in)    :: numflds
        1224             :     character(len=*)    , intent(in)    :: flds_scalar_name
        1225             :     integer             , intent(in)    :: flds_scalar_num
        1226             :     character(len=*)    , intent(in)    :: tag
        1227             :     type(ESMF_Mesh)     , intent(in)    :: mesh
        1228             :     integer             , intent(inout) :: rc
        1229             :
        1230             :     ! local variables
        1231             :     integer                :: n
        1232             :     type(ESMF_Field)       :: field
        1233             :     character(len=80)      :: stdname
        1234             :     character(CL)          :: msg
        1235             :     character(len=*),parameter  :: subname='(atm_import_export:fldlist_realize)'
        1236             :     ! ----------------------------------------------
        1237             :
        1238        3072 :     rc = ESMF_SUCCESS
        1239             :
        1240       96768 :     do n = 1, numflds
        1241       90624 :        stdname = fldList(n)%stdname
        1242       93696 :        if (NUOPC_IsConnected(state, fieldName=stdname)) then
        1243       90624 :           if (stdname == trim(flds_scalar_name)) then
        1244        3072 :              if (masterproc) then
        1245           4 :                 write(iulog,'(a)') trim(subname)//trim(tag)//" field = "//trim(stdname)//" is connected on root pe"
        1246             :              end if
        1247             :              ! Create the scalar field
        1248        3072 :              call SetScalarField(field, flds_scalar_name, flds_scalar_num, rc=rc)
        1249        3072 :              if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1250             :           else
        1251             :              ! Create the field
        1252       87552 :              if (fldlist(n)%ungridded_lbound > 0 .and. fldlist(n)%ungridded_ubound > 0) then
        1253             :                 field = ESMF_FieldCreate(mesh, ESMF_TYPEKIND_R8, name=stdname, meshloc=ESMF_MESHLOC_ELEMENT, &
        1254             :                      ungriddedLbound=(/fldlist(n)%ungridded_lbound/), &
        1255             :                      ungriddedUbound=(/fldlist(n)%ungridded_ubound/), &
        1256       27648 :                      gridToFieldMap=(/2/), rc=rc)
        1257        9216 :                 if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1258        9216 :                 if (masterproc) then
        1259             :                    write(iulog,'(a,i8,a,i8)') trim(subname)// trim(tag)//" Field = "//trim(stdname)// &
        1260          12 :                         " is connected using mesh with lbound ", fldlist(n)%ungridded_lbound,&
        1261          24 :                         " and with ubound ",fldlist(n)%ungridded_ubound
        1262             :                 end if
        1263             :              else
        1264       78336 :                 field = ESMF_FieldCreate(mesh, ESMF_TYPEKIND_R8, name=stdname, meshloc=ESMF_MESHLOC_ELEMENT, rc=rc)
        1265       78336 :                 if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1266       78336 :                 if (masterproc) then
        1267         102 :                    write(iulog,'(a)') trim(subname)// trim(tag)//" Field = "//trim(stdname)// " is connected using mesh "
        1268             :                 end if
        1269             :              end if
        1270             :           endif
        1271             :
        1272             :           ! NOW call NUOPC_Realize
        1273       90624 :           call NUOPC_Realize(state, field=field, rc=rc)
        1274       90624 :           if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1275             :        else
        1276           0 :           if (stdname /= trim(flds_scalar_name)) then
        1277           0 :              if (masterproc) then
        1278           0 :                 write(iulog,'(a)')trim(subname)//trim(tag)//" Field = "//trim(stdname)//" is not connected"
        1279             :              end if
        1280           0 :              call ESMF_StateRemove(state, (/stdname/), rc=rc)
        1281           0 :              if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1282             :           end if
        1283             :        end if
        1284             :     end do
        1285             :
        1286             :   contains  !- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
        1287             :
        1288        3072 :     subroutine SetScalarField(field, flds_scalar_name, flds_scalar_num, rc)
        1289             :       ! ----------------------------------------------
        1290             :       ! create a field with scalar data on the root pe
        1291             :       ! ----------------------------------------------
        1292             :
        1293        3072 :       use ESMF, only : ESMF_Field, ESMF_DistGrid, ESMF_Grid
        1294             :       use ESMF, only : ESMF_DistGridCreate, ESMF_GridCreate, ESMF_LogFoundError, ESMF_LOGERR_PASSTHRU
        1295             :       use ESMF, only : ESMF_FieldCreate, ESMF_GridCreate, ESMF_TYPEKIND_R8
        1296             :
        1297             :       ! input/output variables
        1298             :       type(ESMF_Field) , intent(inout) :: field
        1299             :       character(len=*) , intent(in)    :: flds_scalar_name
        1300             :       integer          , intent(in)    :: flds_scalar_num
        1301             :       integer          , intent(inout) :: rc
        1302             :
        1303             :       ! local variables
        1304             :       type(ESMF_Distgrid) :: distgrid
        1305             :       type(ESMF_Grid)     :: grid
        1306             :       character(len=*), parameter :: subname='(atm_import_export:SetScalarField)'
        1307             :       ! ----------------------------------------------
        1308             :
        1309        3072 :       rc = ESMF_SUCCESS
        1310             :
        1311             :       ! create a DistGrid with a single index space element, which gets mapped onto DE 0.
        1312        3072 :       distgrid = ESMF_DistGridCreate(minIndex=(/1/), maxIndex=(/1/), rc=rc)
        1313        3072 :       if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1314             :
        1315        3072 :       grid = ESMF_GridCreate(distgrid, rc=rc)
        1316        3072 :       if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1317             :
        1318             :       field = ESMF_FieldCreate(name=trim(flds_scalar_name), grid=grid, typekind=ESMF_TYPEKIND_R8, &
        1319        6144 :            ungriddedLBound=(/1/), ungriddedUBound=(/flds_scalar_num/), gridToFieldMap=(/2/), rc=rc)
        1320        3072 :       if (ESMF_LogFoundError(rcToCheck=rc, msg=ESMF_LOGERR_PASSTHRU, line=__LINE__, file=u_FILE_u)) return
        1321             :
        1322        6144 :     end subroutine SetScalarField
        1323             :
        1324             :   end subroutine fldlist_realize
        1325             :
        1326             :   !===============================================================================
        1327    24102912 :   subroutine state_getfldptr(State, fldname, fldptr, fldptr2d, exists, rc)
        1328             :
        1329             :     ! ----------------------------------------------
        1330             :     ! Get pointer to a state field
        1331             :     ! ----------------------------------------------
        1332             :
        1333             :     use ESMF , only : ESMF_State, ESMF_Field, ESMF_Mesh, ESMF_FieldStatus_Flag
        1334             :     use ESMF , only : ESMF_StateGet, ESMF_FieldGet, ESMF_MeshGet
        1335             :     use ESMF , only : ESMF_FIELDSTATUS_COMPLETE, ESMF_FAILURE
        1336             :
        1337             :     ! input/output variables
        1338             :     type(ESMF_State)  , intent(in)    :: State
        1339             :     character(len=*)  , intent(in)    :: fldname
        1340             :     real(R8), optional, pointer       :: fldptr(:)
        1341             :     real(R8), optional, pointer       :: fldptr2d(:,:)
        1342             :     logical , optional, intent(out)   :: exists
        1343             :     integer           , intent(out)   :: rc
        1344             :
        1345             :     ! local variables
        1346             :     type(ESMF_FieldStatus_Flag) :: status
        1347             :     type(ESMF_StateItem_Flag)   :: itemFlag
        1348             :     type(ESMF_Field)            :: lfield
        1349             :     type(ESMF_Mesh)             :: lmesh
        1350             :     integer                     :: nnodes, nelements
        1351             :     logical                     :: lexists
        1352             :     character(len=*), parameter :: subname='(atm_import_export:state_getfldptr)'
        1353             :     ! ----------------------------------------------
        1354             :
        1355    24102912 :     rc = ESMF_SUCCESS
        1356             :
        1357    24102912 :     lexists = .true.
        1358             :
        1359             :     ! Determine if field with name fldname exists in state
        1360    24102912 :     if (present(exists)) then
        1361     7409664 :        call ESMF_StateGet(state, trim(fldname), itemFlag, rc=rc)
        1362     7409664 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1363     7409664 :        if (itemflag == ESMF_STATEITEM_NOTFOUND) then
        1364             :           lexists = .false.
        1365             :        end if
        1366     7409664 :        exists = lexists
        1367             :     end if
        1368             :
        1369             :     if (lexists) then
        1370    21141504 :        call ESMF_StateGet(State, itemName=trim(fldname), field=lfield, rc=rc)
        1371    21141504 :        if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1372    21141504 :        if (present(fldptr)) then
        1373    18912768 :           call ESMF_FieldGet(lfield, farrayPtr=fldptr, rc=rc)
        1374    18912768 :           if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1375     2228736 :        else if (present(fldptr2d)) then
        1376     2228736 :           call ESMF_FieldGet(lfield, farrayPtr=fldptr2d, rc=rc)
        1377     2228736 :           if (ChkErr(rc,__LINE__,u_FILE_u)) return
        1378             :        end if
        1379             :     end if
        1380             :
        1381    48205824 :   end subroutine state_getfldptr
        1382             :
        1383    24102912 : end module atm_import_export

Generated by: LCOV version 1.14