LCOV - code coverage report
Current view: | top level - physics/cam - cam_diagnostics.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 791 | 1086 | 72.8 %
Date: | 2024-12-17 17:57:11 |  | Functions: | 28 | 30 | 93.3 %

Function Name | Hit count
__cam_diagnostics_MOD___copy_cam_diagnostics_Dqcond_t | 0
__cam_diagnostics_MOD___final_cam_diagnostics_Dqcond_t | 0
__cam_diagnostics_MOD_diag_init | 1536
__cam_diagnostics_MOD_diag_init_dry | 1536
__cam_diagnostics_MOD_diag_init_moist | 1536
__cam_diagnostics_MOD_diag_readnl | 1536
__cam_diagnostics_MOD_diag_register | 1536
__cam_diagnostics_MOD_diag_register_dry | 1536
__cam_diagnostics_MOD_diag_register_moist | 1536
__cam_diagnostics_MOD_diag_deallocate | 369408
__cam_diagnostics_MOD_diag_deallocate_dry | 369408
__cam_diagnostics_MOD_diag_deallocate_moist | 369408
__cam_diagnostics_MOD_diag_allocate | 370944
__cam_diagnostics_MOD_diag_allocate_dry | 370944
__cam_diagnostics_MOD_diag_allocate_moist | 370944
__cam_diagnostics_MOD_diag_conv | 1489176
__cam_diagnostics_MOD_diag_phys_tend_writeout | 1489176
__cam_diagnostics_MOD_diag_phys_tend_writeout_dry | 1489176
__cam_diagnostics_MOD_diag_phys_tend_writeout_moist | 1489176
__cam_diagnostics_MOD_diag_phys_writeout | 1489176
__cam_diagnostics_MOD_diag_phys_writeout_dry | 1489176
__cam_diagnostics_MOD_diag_phys_writeout_moist | 1489176
__cam_diagnostics_MOD_diag_surf | 1489176
__cam_diagnostics_MOD_diag_conv_tend_ini | 1495368
__cam_diagnostics_MOD_diag_export | 1495368
__cam_diagnostics_MOD_diag_physvar_ic | 1495368
__cam_diagnostics_MOD_diag_state_b4_phys_write | 1495368
__cam_diagnostics_MOD_diag_state_b4_phys_write_dry | 1495368
__cam_diagnostics_MOD_diag_state_b4_phys_write_moist | 1495368
__cam_diagnostics_MOD_diag_clip_tend_writeout | 4467528

Generated by: LCOV version 1.14