LCOV - code coverage report
Current view: | top level - hemco/HEMCO/src/Core - hco_fluxarr_mod.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 0 | 254 | 0.0 %
Date: | 2024-12-17 17:57:11 |  | Functions: | 0 | 12 | 0.0 %

              Line data    Source code
           1             : !------------------------------------------------------------------------------
           2             : !                   Harmonized Emissions Component (HEMCO)                    !
           3             : !------------------------------------------------------------------------------
           4             : !BOP
           5             : !
           6             : ! !MODULE: hco_fluxarr_mod.F90
           7             : !
           8             : ! !DESCRIPTION: Module HCO\_FluxArr\_Mod contains routines to handle
           9             : ! the HEMCO flux arrays. These are the emissions and deposition arrays
          10             : ! listed in the HEMCO state object.
          11             : !\\
          12             : !\\
          13             : ! !INTERFACE:
          14             : !
          15             : MODULE HCO_FluxArr_Mod
          16             : !
          17             : ! USES:
          18             : !
          19             :   USE HCO_Error_Mod
          20             :   USE HCO_Arr_Mod
          21             :   USE HCO_Scale_Mod
          22             :   USE HCO_State_Mod, ONLY : HCO_State
          23             :
          24             :   IMPLICIT NONE
          25             :   PRIVATE
          26             : !
          27             : ! !PUBLIC MEMBER FUNCTIONS:
          28             : !
          29             :   PUBLIC  :: HCO_EmisAdd
          30             :   PUBLIC  :: HCO_DepvAdd
          31             :   PUBLIC  :: HCO_FluxarrReset
          32             : !
          33             : ! !PRIVATE MEMBER FUNCTIONS:
          34             : !
          35             :   PRIVATE :: DiagnCheck
          36             : !
          37             : ! !REMARKS:
          38             : !
          39             : ! !REVISION HISTORY:
          40             : !  05 Jan 2014 - C. Keller - Initial version, adapted from hco_state_mod.F90
          41             : !  See https://github.com/geoschem/hemco for complete history
          42             : !EOP
          43             : !------------------------------------------------------------------------------
          44             : !BOC
          45             : !
          46             : ! !PRIVATE TYPES:
          47             : !
          48             :   INTERFACE HCO_EmisAdd
          49             :      MODULE PROCEDURE HCO_EmisAdd_3D_Dp
          50             :      MODULE PROCEDURE HCO_EmisAdd_3D_Sp
          51             :      MODULE PROCEDURE HCO_EmisAdd_2D_Sp
          52             :      MODULE PROCEDURE HCO_EmisAdd_2D_Dp
          53             :      MODULE PROCEDURE HCO_EmisAdd_Dp
          54             :      MODULE PROCEDURE HCO_EmisAdd_Sp
          55             :   END INTERFACE
          56             :
          57             :   INTERFACE HCO_DepvAdd
          58             :      MODULE PROCEDURE HCO_DepvAdd_2D_Sp
          59             :      MODULE PROCEDURE HCO_DepvAdd_2D_Dp
          60             :      MODULE PROCEDURE HCO_DepvAdd_Dp
          61             :      MODULE PROCEDURE HCO_DepvAdd_Sp
          62             :   END INTERFACE
          63             :
          64             : CONTAINS
          65             : !EOC
          66             : !------------------------------------------------------------------------------
          67             : !                   Harmonized Emissions Component (HEMCO)                    !
          68             : !------------------------------------------------------------------------------
          69             : !BOP
          70             : !
          71             : ! !IROUTINE: HCO_FluxarrReset
          72             : !
          73             : ! !DESCRIPTION: Routine HCO\_FluxarrReset (re)sets all data arrays
          74             : ! of the passed HEMCO state object. The (optional) argument Typ
          75             : ! indicates whether only emissions (1), deposition (2), or concentration
          76             : ! (3) arrays shall be reset. To reset all, set Typ to 0 (default).
          77             : !\\
          78             : !\\
          79             : ! !INTERFACE:
          80             : !
          81           0 :   SUBROUTINE HCO_FluxarrReset( HcoState, RC, Typ )
          82             : !
          83             : ! !INPUT/OUTPUT PARAMETERS:
          84             : !
          85             :     TYPE(HCO_State), POINTER                 :: HcoState
          86             :     INTEGER,         INTENT(INOUT)           :: RC
          87             : !
          88             : ! !INPUT PARAMETERS:
          89             : !
          90             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Typ
          91             : !
          92             : ! !REMARKS:
          93             : !
          94             : ! !REVISION HISTORY:
          95             : !  01 May 2013 - C. Keller - Initial version
          96             : !  See https://github.com/geoschem/hemco for complete history
          97             : !EOP
          98             : !------------------------------------------------------------------------------
          99             : !BOC
         100             :     INTEGER :: N, thisTyp
         101             :
         102             :     !=====================================================================
         103             :     ! HCO_FluxarrReset begins here!
         104             :     !=====================================================================
         105             :
         106             :     ! Set local flux direction flag
         107           0 :     IF ( PRESENT(Typ) ) THEN
         108           0 :        thisTyp = Typ
         109             :     ELSE
         110             :        thisTyp = 0
         111             :     ENDIF
         112             :
         113             :     ! Loop over all arrays.
         114           0 :     DO N = 1, HcoState%nSpc
         115             :
         116             :        ! 3D flux rates array
         117           0 :        IF ( thisTyp == 0 .OR. thisTyp == 1 ) THEN
         118           0 :           IF ( ASSOCIATED(HcoState%Spc(N)%Emis) ) THEN
         119           0 :              IF ( ASSOCIATED(HcoState%Spc(N)%Emis%Val) ) THEN
         120           0 :                 HcoState%Spc(N)%Emis%Val = 0.0_hp
         121             :              ENDIF
         122             :           ENDIF
         123             :        ENDIF
         124             :
         125             :        ! 2D deposition velocity array
         126           0 :        IF ( thisTyp == 0 .OR. thisTyp == 2 ) THEN
         127           0 :           IF ( ASSOCIATED(HcoState%Spc(N)%Depv) ) THEN
         128           0 :              IF ( ASSOCIATED(HcoState%Spc(N)%Depv%Val) ) THEN
         129           0 :                 HcoState%Spc(N)%Depv%Val = 0.0_hp
         130             :              ENDIF
         131             :           ENDIF
         132             :        ENDIF
         133             :
         134             :        ! 3D concentrations
         135           0 :        IF ( thisTyp == 0 .OR. thisTyp == 3 ) THEN
         136           0 :           IF ( ASSOCIATED(HcoState%Spc(N)%Conc) ) THEN
         137           0 :              IF ( ASSOCIATED(HcoState%Spc(N)%Conc%Val) ) THEN
         138           0 :                 HcoState%Spc(N)%Conc%Val = 0.0_hp
         139             :              ENDIF
         140             :           ENDIF
         141             :        ENDIF
         142             :
         143             :     ENDDO
         144             :
         145             :     ! Return w/ success
         146           0 :     RC = HCO_SUCCESS
         147             :
         148           0 :   END SUBROUTINE HCO_FluxarrReset
         149             : !EOC
         150             : !------------------------------------------------------------------------------
         151             : !                   Harmonized Emissions Component (HEMCO)                    !
         152             : !------------------------------------------------------------------------------
         153             : !BOP
         154             : !
         155             : ! !IROUTINE: HCO_EmisAdd_3D_Dp
         156             : !
         157             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_3D adds the 3D-array Arr3D
         158             : ! to the emissions array of species HcoID in HEMCO object HcoState.
         159             : ! This routine also updates all autofill diagnostics that are defined
         160             : ! for the givne species, extension number, emission category and
         161             : ! hierarchy.
         162             : !\\
         163             : !\\
         164             : ! !INTERFACE:
         165             : !
         166           0 :   SUBROUTINE HCO_EmisAdd_3D_Dp( HcoState,  Arr3D,    HcoID, &
         167             :                                 RC,        ExtNr,    Cat,   Hier,  &
         168             :                                 MinDiagnLev )
         169             : !
         170             : ! !INPUT/OUTPUT PARAMETERS:
         171             : !
         172             :     TYPE(HCO_State), POINTER                 :: HcoState
         173             :     REAL(dp),        INTENT(INOUT)           :: Arr3D( HcoState%NX, &
         174             :                                                        HcoState%NY, &
         175             :                                                        HcoState%NZ )
         176             :     INTEGER,         INTENT(INOUT)           :: RC
         177             : !
         178             : ! !INPUT PARAMETERS:
         179             : !
         180             :     INTEGER,         INTENT(IN   )           :: HcoID
         181             :     INTEGER,         INTENT(IN   ), OPTIONAL :: ExtNr
         182             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Cat
         183             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Hier
         184             :     INTEGER,         INTENT(IN   ), OPTIONAL :: MinDiagnLev
         185             : !
         186             : ! !REVISION HISTORY:
         187             : !  01 May 2013 - C. Keller - Initial version
         188             : !  See https://github.com/geoschem/hemco for complete history
         189             : !EOP
         190             : !------------------------------------------------------------------------------
         191             : !BOC
         192             : !
         193             : ! !LOCAL VARIABLES:
         194             : !
         195             :     CHARACTER(LEN=255)  :: LOC
         196             :
         197             :     !=====================================================================
         198             :     ! HCO_EmisAdd_3D_Dp begins here!
         199             :     !=====================================================================
         200           0 :     LOC = 'HCO_EmisAdd_3D_Dp (HCO_FLUXARR_MOD.F90)'
         201             :
         202             :     ! Make sure target flux array in HcoState is allocated
         203           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         204           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         205           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         206             :
         207             :     ! Check for negative values. NegFlag determines the behavior for
         208             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         209           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         210           0 :        IF ( ANY( Arr3D < 0.0_hp ) ) THEN
         211             :
         212             :           ! Negative flag is 1: set to zero and prompt warning
         213           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         214           0 :              WHERE ( Arr3D < 0.0_hp ) Arr3D = 0.0_hp
         215             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         216             :                 'Negative values found - set to zero!', &
         217           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         218             :
         219             :           ! Negative flag is 0: return w/ error
         220             :           ELSE
         221             :              CALL HCO_ERROR ( &
         222             :                 'Negative values found!', &
         223           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         224           0 :              RETURN
         225             :           ENDIF
         226             :        ENDIF
         227             :     ENDIF
         228             :
         229             :     ! Eventually add universal scale factor
         230           0 :     CALL HCO_ScaleArr( HcoState, HcoID, Arr3D, RC )
         231           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         232           0 :         CALL HCO_ERROR( 'ERROR 0', RC, THISLOC=LOC )
         233           0 :         RETURN
         234             :     ENDIF
         235             :
         236             :     ! Add array
         237             :     HcoState%Spc(HcoID)%Emis%Val(:,:,:) = &
         238           0 :        HcoState%Spc(HcoID)%Emis%Val(:,:,:) + Arr3D(:,:,:)
         239             :
         240             :     ! Check for diagnostics
         241             :     CALL DiagnCheck( HcoState,   ExtNr=ExtNr, Cat=Cat, &
         242             :                      Hier=Hier,  HcoID=HcoID, Arr3D=Arr3D, &
         243           0 :                      MinDiagnLev=MinDiagnLev, RC=RC     )
         244           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         245           0 :         CALL HCO_ERROR( 'ERROR 1', RC, THISLOC=LOC )
         246           0 :         RETURN
         247             :     ENDIF
         248             :
         249             :     ! Return w/ success
         250           0 :     RC = HCO_SUCCESS
         251             :
         252             :   END SUBROUTINE HCO_EmisAdd_3D_Dp
         253             : !EOC
         254             : !------------------------------------------------------------------------------
         255             : !                   Harmonized Emissions Component (HEMCO)                    !
         256             : !------------------------------------------------------------------------------
         257             : !BOP
         258             : !
         259             : ! !IROUTINE: HCO_EmisAdd_3D_Sp
         260             : !
         261             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_3D adds the 3D-array Arr3D to the
         262             : ! emissions array of species HcoID in HEMCO object HcoState.
         263             : ! This routine also updates all autofill diagnostics that are defined
         264             : ! for the givne species, extension number, emission category and
         265             : ! hierarchy.
         266             : !\\
         267             : !\\
         268             : ! !INTERFACE:
         269             : !
         270           0 :   SUBROUTINE HCO_EmisAdd_3D_Sp ( HcoState,  Arr3D,    HcoID, &
         271             :                                  RC,        ExtNr,    Cat,   Hier,  &
         272             :                                  MinDiagnLev )
         273             : !
         274             : ! !INPUT/OUTPUT PARAMETERS:
         275             : !
         276             :     TYPE(HCO_State), POINTER                 :: HcoState
         277             :     REAL(sp),        INTENT(INOUT)           :: Arr3D( HcoState%NX, &
         278             :                                                        HcoState%NY, &
         279             :                                                        HcoState%NZ )
         280             :     INTEGER,         INTENT(INOUT)           :: RC
         281             : !
         282             : ! !INPUT PARAMETERS:
         283             : !
         284             :     INTEGER,         INTENT(IN   )           :: HcoID
         285             :     INTEGER,         INTENT(IN   ), OPTIONAL :: ExtNr
         286             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Cat
         287             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Hier
         288             :     INTEGER,         INTENT(IN   ), OPTIONAL :: MinDiagnLev
         289             : !
         290             : ! !REVISION HISTORY:
         291             : !  01 May 2013 - C. Keller - Initial version
         292             : !  See https://github.com/geoschem/hemco for complete history
         293             : !EOP
         294             : !------------------------------------------------------------------------------
         295             : !BOC
         296             : !
         297             : ! !LOCAL VARIABLES:
         298             : !
         299             :     CHARACTER(LEN=255)  :: LOC
         300             :
         301             :     !=====================================================================
         302             :     ! HCO_EmisAdd_3D_Sp begins here!
         303             :     !=====================================================================
         304           0 :     LOC = 'HCO_EmisAdd_3D_Sp (HCO_FLUXARR_MOD.F90)'
         305             :
         306             :     ! Make sure target flux array in HcoState is allocated
         307           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         308           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         309           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         310             :
         311             :     ! Check for negative values. NegFlag determines the behavior for
         312             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         313           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         314           0 :        IF ( ANY( Arr3D < 0.0_sp ) ) THEN
         315             :
         316             :           ! Negative flag is 1: set to zero and prompt warning
         317           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         318           0 :              WHERE ( Arr3D < 0.0_sp ) Arr3D = 0.0_sp
         319             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         320             :                'Negative values found - set to zero!', &
         321           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         322             :
         323             :           ! Negative flag is 0: return w/ error
         324             :           ELSE
         325             :              CALL HCO_ERROR ( &
         326             :                'Negative values found!', &
         327           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         328           0 :              RETURN
         329             :           ENDIF
         330             :        ENDIF
         331             :     ENDIF
         332             :
         333             :     ! Eventually add universal scale factor
         334           0 :     CALL HCO_ScaleArr( HcoState, HcoID, Arr3D, RC )
         335           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         336           0 :         CALL HCO_ERROR( 'ERROR 2', RC, THISLOC=LOC )
         337           0 :         RETURN
         338             :     ENDIF
         339             :
         340             :     ! Add array
         341             :     HcoState%Spc(HcoID)%Emis%Val(:,:,:) = &
         342           0 :        HcoState%Spc(HcoID)%Emis%Val(:,:,:) + Arr3D(:,:,:)
         343             :
         344             :     ! Check for diagnostics
         345             :     CALL DiagnCheck( HcoState,   ExtNr=ExtNr, Cat=Cat, &
         346             :                      Hier=Hier,  HcoID=HcoID, Arr3Dsp=Arr3D, &
         347           0 :                      MinDiagnLev=MinDiagnLev, RC=RC     )
         348           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         349           0 :         CALL HCO_ERROR( 'ERROR 3', RC, THISLOC=LOC )
         350           0 :         RETURN
         351             :     ENDIF
         352             :
         353             :     ! Return w/ success
         354           0 :     RC = HCO_SUCCESS
         355             :
         356             :   END SUBROUTINE HCO_EmisAdd_3D_Sp
         357             : !EOC
         358             : !------------------------------------------------------------------------------
         359             : !                   Harmonized Emissions Component (HEMCO)                    !
         360             : !------------------------------------------------------------------------------
         361             : !BOP
         362             : !
         363             : ! !IROUTINE: HCO_EmisAdd_2D_Dp
         364             : !
         365             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_2D\_Dp adds the real*8 2D-array Arr2D
         366             : ! to the emission array of species HcoID in HEMCO object HcoState.
         367             : ! This routine also updates all autofill diagnostics that are defined
         368             : ! for the givne species, extension number, emission category and
         369             : ! hierarchy.
         370             : !\\
         371             : !\\
         372             : ! !INTERFACE:
         373             : !
         374           0 :   SUBROUTINE HCO_EmisAdd_2D_Dp( HcoState,  Arr2D,    HcoID, &
         375             :                                 RC,        ExtNr,    Cat,   Hier,  &
         376             :                                 MinDiagnLev )
         377             : !
         378             : ! !INPUT/OUTPUT PARAMETERS:
         379             : !
         380             :     TYPE(HCO_State), POINTER                 :: HcoState
         381             :     REAL(dp),        INTENT(INOUT)           :: Arr2D(HcoState%NX,HcoState%NY)
         382             :     INTEGER,         INTENT(INOUT)           :: RC
         383             : !
         384             : ! !INPUT PARAMETERS:
         385             : !
         386             :     INTEGER,         INTENT(IN   )           :: HcoID
         387             :     INTEGER,         INTENT(IN   ), OPTIONAL :: ExtNr
         388             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Cat
         389             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Hier
         390             :     INTEGER,         INTENT(IN   ), OPTIONAL :: MinDiagnLev
         391             : !
         392             : ! !REVISION HISTORY:
         393             : !  01 May 2013 - C. Keller - Initial version
         394             : !  See https://github.com/geoschem/hemco for complete history
         395             : !EOP
         396             : !------------------------------------------------------------------------------
         397             : !BOC
         398             : !
         399             : ! !LOCAL VARIABLES:
         400             : !
         401             :     CHARACTER(LEN=255)  :: LOC
         402             :
         403             :     !=====================================================================
         404             :     ! HCO_EmisAdd_2D_Dp begins here!
         405             :     !=====================================================================
         406           0 :     LOC = 'HCO_EmisAdd_2D_Dp (HCO_FLUXARR_MOD)'
         407             :
         408             :     ! Make sure target flux array in HcoState is allocated
         409           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         410           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         411           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         412             :
         413             :     ! Check for negative values. NegFlag determines the behavior for
         414             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         415           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         416           0 :        IF ( ANY( Arr2D < 0.0_hp ) ) THEN
         417             :
         418             :           ! Negative flag is 1: set to zero and prompt warning
         419           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         420           0 :              WHERE ( Arr2D < 0.0_hp ) Arr2D = 0.0_hp
         421             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         422             :                'Negative values found - set to zero!', &
         423           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         424             :
         425             :           ! Negative flag is 0: return w/ error
         426             :           ELSE
         427             :              CALL HCO_ERROR ( &
         428             :                'Negative values found!', &
         429           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         430           0 :              RETURN
         431             :           ENDIF
         432             :        ENDIF
         433             :     ENDIF
         434             :
         435             :     ! Eventually add universal scale factor
         436           0 :     CALL HCO_ScaleArr( HcoState, HcoID, Arr2D, RC )
         437           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         438           0 :         CALL HCO_ERROR( 'ERROR 4', RC, THISLOC=LOC )
         439           0 :         RETURN
         440             :     ENDIF
         441             :
         442             :     ! Add array
         443             :     HcoState%Spc(HcoID)%Emis%Val(:,:,1) = &
         444           0 :        HcoState%Spc(HcoID)%Emis%Val(:,:,1) + Arr2D(:,:)
         445             :
         446             :     ! Check for diagnostics
         447             :     CALL DiagnCheck( HcoState,   ExtNr=ExtNr, Cat=Cat, &
         448             :                      Hier=Hier,  HcoID=HcoID, Arr2D=Arr2D, &
         449           0 :                      MinDiagnLev=MinDiagnLev, RC=RC     )
         450           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         451           0 :         CALL HCO_ERROR( 'ERROR 5', RC, THISLOC=LOC )
         452           0 :         RETURN
         453             :     ENDIF
         454             :
         455             :     ! Return w/ success
         456           0 :     RC = HCO_SUCCESS
         457             :
         458             :   END SUBROUTINE HCO_EmisAdd_2D_Dp
         459             : !EOC
         460             : !------------------------------------------------------------------------------
         461             : !                   Harmonized Emissions Component (HEMCO)                    !
         462             : !------------------------------------------------------------------------------
         463             : !BOP
         464             : !
         465             : ! !IROUTINE: HCO_EmisAdd_2D_Sp
         466             : !
         467             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_2D\_Sp adds the real*4 2D-array Arr2D
         468             : ! to the emission array of species HcoID in HEMCO object HcoState.
         469             : ! This routine also updates all autofill diagnostics that are defined
         470             : ! for the givne species, extension number, emission category and
         471             : ! hierarchy.
         472             : !\\
         473             : !\\
         474             : ! !INTERFACE:
         475             : !
         476           0 :   SUBROUTINE HCO_EmisAdd_2D_Sp( HcoState,  Arr2D,    HcoID, &
         477             :                                 RC,        ExtNr,    Cat,   Hier,  &
         478             :                                 MinDiagnLev )
         479             : !
         480             : ! !INPUT/OUTPUT PARAMETERS:
         481             : !
         482             : !
         483             :     TYPE(HCO_State), POINTER                 :: HcoState
         484             :     REAL(sp),        INTENT(INOUT)           :: Arr2D(HcoState%NX,HcoState%NY)
         485             :     INTEGER,         INTENT(INOUT)           :: RC
         486             : !
         487             : ! !INPUT PARAMETERS:
         488             : !
         489             :     INTEGER,         INTENT(IN   )           :: HcoID
         490             :     INTEGER,         INTENT(IN   ), OPTIONAL :: ExtNr
         491             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Cat
         492             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Hier
         493             :     INTEGER,         INTENT(IN   ), OPTIONAL :: MinDiagnLev
         494             : !
         495             : ! !REVISION HISTORY:
         496             : !  01 May 2013 - C. Keller - Initial version
         497             : !  See https://github.com/geoschem/hemco for complete history
         498             : !EOP
         499             : !------------------------------------------------------------------------------
         500             : !BOC
         501             : !
         502             : ! !LOCAL VARIABLES:
         503             : !
         504             :     CHARACTER(LEN=255)  :: LOC
         505             :
         506             :     !=====================================================================
         507             :     ! HCO_EmisAdd_2D_Sp begins here!
         508             :     !=====================================================================
         509           0 :     LOC = 'HCO_EmisAdd_2D_Sp (HCO_FLUXARR_MOD.F90)'
         510             :
         511             :     ! Make sure target flux array in HcoState is allocated
         512           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         513           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         514           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         515             :
         516             :     ! Check for negative values. NegFlag determines the behavior for
         517             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         518           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         519           0 :        IF ( ANY( Arr2D < 0.0_sp ) ) THEN
         520             :
         521             :           ! Negative flag is 1: set to zero and prompt warning
         522           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         523           0 :              WHERE ( Arr2D < 0.0_sp ) Arr2D = 0.0_sp
         524             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         525             :                'Negative values found - set to zero!', &
         526           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         527             :
         528             :           ! Negative flag is 0: return w/ error
         529             :           ELSE
         530             :              CALL HCO_ERROR ( &
         531             :                'Negative values found!', &
         532           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         533           0 :              RETURN
         534             :           ENDIF
         535             :        ENDIF
         536             :     ENDIF
         537             :
         538             :     ! Eventually add universal scale factor
         539           0 :     CALL HCO_ScaleArr( HcoState, HcoID, Arr2D, RC )
         540           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         541           0 :         CALL HCO_ERROR( 'ERROR 6', RC, THISLOC=LOC )
         542           0 :         RETURN
         543             :     ENDIF
         544             :
         545             :     ! Add array
         546             :     HcoState%Spc(HcoID)%Emis%Val(:,:,1) = &
         547           0 :        HcoState%Spc(HcoID)%Emis%Val(:,:,1) + Arr2D(:,:)
         548             :
         549             :     ! Check for diagnostics
         550             :     CALL DiagnCheck( HcoState,   ExtNr=ExtNr, Cat=Cat, &
         551             :                      Hier=Hier,  HcoID=HcoID, Arr2Dsp=Arr2D, &
         552           0 :                      MinDiagnLev=MinDiagnLev, RC=RC     )
         553           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         554           0 :         CALL HCO_ERROR( 'ERROR 7', RC, THISLOC=LOC )
         555           0 :         RETURN
         556             :     ENDIF
         557             :
         558             :     ! Return w/ success
         559           0 :     RC = HCO_SUCCESS
         560             :
         561             :   END SUBROUTINE HCO_EmisAdd_2D_Sp
         562             : !EOC
         563             : !------------------------------------------------------------------------------
         564             : !                   Harmonized Emissions Component (HEMCO)                    !
         565             : !------------------------------------------------------------------------------
         566             : !BOP
         567             : !
         568             : ! !IROUTINE: HCO_EmisAdd_Dp
         569             : !
         570             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_Dp adds value iVal to the emission
         571             : ! array of species HcoID in HEMCO object HcoState. The value is placed at
         572             : ! location I, J, L of the array.
         573             : !\\
         574             : !\\
         575             : ! !INTERFACE:
         576             : !
         577           0 :   SUBROUTINE HCO_EmisAdd_Dp( HcoState, iVal, HcoID, I, J, L, RC )
         578             : !
         579             : ! !INPUT/OUTPUT PARAMETERS:
         580             : !
         581             :     TYPE(HCO_State), POINTER       :: HcoState
         582             :     REAL(dp),        INTENT(INOUT) :: iVal
         583             :     INTEGER,         INTENT(INOUT) :: RC
         584             : !
         585             : ! !INPUT PARAMETERS:
         586             : !
         587             :     INTEGER,         INTENT(IN   ) :: HcoID
         588             :     INTEGER,         INTENT(IN   ) :: I
         589             :     INTEGER,         INTENT(IN   ) :: J
         590             :     INTEGER,         INTENT(IN   ) :: L
         591             : !
         592             : ! !REVISION HISTORY:
         593             : !  01 May 2013 - C. Keller - Initial version
         594             : !  See https://github.com/geoschem/hemco for complete history
         595             : !EOP
         596             : !------------------------------------------------------------------------------
         597             : !BOC
         598             :     CHARACTER(LEN=255) :: MSG, LOC
         599             :
         600             :     !=====================================================================
         601             :     ! HCO_EmisAdd_Dp begins here!
         602             :     !=====================================================================
         603           0 :     LOC = 'HCO_EmisAdd_Dp (HCO_FLUXARR_MOD.F90)'
         604             :
         605             :     ! Check size dimensions
         606           0 :     IF ( I > HcoState%NX ) THEN
         607           0 :        MSG = 'Cannot add DP - i too high!'
         608           0 :        CALL HCO_ERROR ( MSG, RC )
         609           0 :        RETURN
         610             :     ENDIF
         611           0 :     IF ( J > HcoState%NY ) THEN
         612           0 :        MSG = 'Cannot add DP - j too high!'
         613           0 :        CALL HCO_ERROR ( MSG, RC )
         614           0 :        RETURN
         615             :     ENDIF
         616           0 :     IF ( L > HcoState%NZ ) THEN
         617           0 :        MSG = 'Cannot add DP - l too high!'
         618           0 :        CALL HCO_ERROR ( MSG, RC )
         619           0 :        RETURN
         620             :     ENDIF
         621             :
         622             :     ! Make sure target flux array in HcoState is allocated
         623           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         624           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         625           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         626             :
         627             :     ! Check for negative values. NegFlag determines the behavior for
         628             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         629           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         630           0 :        IF ( iVal < 0.0_hp ) THEN
         631             :
         632             :           ! Negative flag is 1: set to zero and prompt warning
         633           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         634           0 :              iVal = 0.0_hp
         635             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         636             :                'Negative values found - set to zero!', &
         637           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         638             :
         639             :           ! Negative flag is 0: return w/ error
         640             :           ELSE
         641             :              CALL HCO_ERROR ( &
         642             :                'Negative values found!', &
         643           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         644           0 :              RETURN
         645             :           ENDIF
         646             :        ENDIF
         647             :     ENDIF
         648             :
         649             :     ! Eventually add universal scale factor
         650           0 :     CALL HCO_ScaleArr( HcoState, HcoID, iVal, RC )
         651           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         652           0 :         CALL HCO_ERROR( 'ERROR 8', RC, THISLOC=LOC )
         653           0 :         RETURN
         654             :     ENDIF
         655             :
         656             :     ! Add array
         657           0 :     HcoState%Spc(HcoID)%Emis%Val(I,J,L) = &
         658           0 :        HcoState%Spc(HcoID)%Emis%Val(I,J,L) + iVal
         659             :
         660             :     ! Return w/ success
         661           0 :     RC = HCO_SUCCESS
         662             :
         663             :   END SUBROUTINE HCO_EmisAdd_Dp
         664             : !EOC
         665             : !------------------------------------------------------------------------------
         666             : !                   Harmonized Emissions Component (HEMCO)                    !
         667             : !------------------------------------------------------------------------------
         668             : !BOP
         669             : !
         670             : ! !IROUTINE: HCO_EmisAdd_Sp
         671             : !
         672             : ! !DESCRIPTION: Routine HCO\_EmisAdd\_Sp adds value iVal to the emission
         673             : ! array of species HcoID in HEMCO object HcoState. The value is placed
         674             : ! at location I, J, L of the array.
         675             : !\\
         676             : !\\
         677             : ! !INTERFACE:
         678             : !
         679           0 :   SUBROUTINE HCO_EmisAdd_Sp( HcoState, iVal, HcoID, I, J, L, RC )
         680             : !
         681             : ! !INPUT/OUTPUT PARAMETERS:
         682             : !
         683             :     TYPE(HCO_State), POINTER       :: HcoState
         684             :     REAL(sp),        INTENT(INOUT) :: iVal
         685             :     INTEGER,         INTENT(INOUT) :: RC
         686             : !
         687             : ! !INPUT PARAMETERS:
         688             : !
         689             :     INTEGER,         INTENT(IN   ) :: HcoID
         690             :     INTEGER,         INTENT(IN   ) :: I
         691             :     INTEGER,         INTENT(IN   ) :: J
         692             :     INTEGER,         INTENT(IN   ) :: L
         693             : !
         694             : ! !REVISION HISTORY:
         695             : !  01 May 2013 - C. Keller - Initial version
         696             : !  See https://github.com/geoschem/hemco for complete history
         697             : !EOP
         698             : !------------------------------------------------------------------------------
         699             : !BOC
         700             :     CHARACTER(LEN=255) :: MSG, LOC
         701             :
         702             :     !=====================================================================
         703             :     ! HCO_EmisAdd_Sp begins here!
         704             :     !=====================================================================
         705           0 :     LOC = 'HCO_EmisAdd_Sp (HCO_FLUXARR_MOD.F90)'
         706             :
         707             :     ! Check size dimensions
         708           0 :     IF ( I > HcoState%NX ) THEN
         709           0 :        MSG = 'Cannot add SP - i too high!'
         710           0 :        CALL HCO_ERROR ( MSG, RC )
         711           0 :        RETURN
         712             :     ENDIF
         713           0 :     IF ( J > HcoState%NY ) THEN
         714           0 :        MSG = 'Cannot add SP - j too high!'
         715           0 :        CALL HCO_ERROR ( MSG, RC )
         716           0 :        RETURN
         717             :     ENDIF
         718           0 :     IF ( L > HcoState%NZ ) THEN
         719           0 :        MSG = 'Cannot add SP - l too high!'
         720           0 :        CALL HCO_ERROR ( MSG, RC )
         721           0 :        RETURN
         722             :     ENDIF
         723             :
         724             :     ! Make sure target flux array in HcoState is allocated
         725           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Emis, &
         726           0 :                          HcoState%NX, HcoState%NY, HcoState%NZ, RC )
         727           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         728             :
         729             :     ! Check for negative values. NegFlag determines the behavior for
         730             :     ! negative values: 2 = allow; 1 = set to zero + warning; 0 = error.
         731           0 :     IF ( HcoState%Options%NegFlag /= 2 ) THEN
         732           0 :        IF ( iVal < 0.0_sp ) THEN
         733             :
         734             :           ! Negative flag is 1: set to zero and prompt warning
         735           0 :           IF ( HcoState%Options%NegFlag == 1 ) THEN
         736           0 :              iVal = 0.0_sp
         737             :              CALL HCO_WARNING ( HcoState%Config%Err, &
         738             :                'Negative values found - set to zero!', &
         739           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         740             :
         741             :           ! Negative flag is 0: return w/ error
         742             :           ELSE
         743             :              CALL HCO_ERROR ( &
         744             :                'Negative values found!', &
         745           0 :                 RC, THISLOC = 'HCO_EmisAdd (HCO_FLUXARR_MOD.F90)' )
         746           0 :              RETURN
         747             :           ENDIF
         748             :        ENDIF
         749             :     ENDIF
         750             :
         751             :     ! Eventually add universal scale factor
         752           0 :     CALL HCO_ScaleArr( HcoState, HcoID, iVal, RC )
         753           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         754           0 :         CALL HCO_ERROR( 'ERROR 9', RC, THISLOC=LOC )
         755           0 :         RETURN
         756             :     ENDIF
         757             :
         758             :     ! Add array
         759           0 :     HcoState%Spc(HcoID)%Emis%Val(I,J,L) = &
         760           0 :        HcoState%Spc(HcoID)%Emis%Val(I,J,L) + iVal
         761             :
         762             :     ! Return w/ success
         763           0 :     RC = HCO_SUCCESS
         764             :
         765             :   END SUBROUTINE HCO_EmisAdd_Sp
         766             : !EOC
         767             : !------------------------------------------------------------------------------
         768             : !                   Harmonized Emissions Component (HEMCO)                    !
         769             : !------------------------------------------------------------------------------
         770             : !BOP
         771             : !
         772             : ! !IROUTINE: HCO_DepvAdd_2D_Dp
         773             : !
         774             : ! !DESCRIPTION: Routine HCO\_DepvAdd\_2D\_Dp adds the real*8 2D-array Arr2D
         775             : ! to the depostion array of species HcoID in HEMCO object HcoState.
         776             : !\\
         777             : !\\
         778             : ! !INTERFACE:
         779             : !
         780           0 :   SUBROUTINE HCO_DepvAdd_2D_Dp( HcoState, Arr2D, HcoID, RC )
         781             : !
         782             : ! !INPUT/OUTPUT PARAMETERS:
         783             : !
         784             :     TYPE(HCO_State), POINTER       :: HcoState
         785             :     INTEGER,         INTENT(INOUT) :: RC
         786             : !
         787             : ! !INPUT PARAMETERS:
         788             : !
         789             :     REAL(dp),        INTENT(IN   ) :: Arr2D(HcoState%NX,HcoState%NY)
         790             :     INTEGER,         INTENT(IN   ) :: HcoID
         791             : !
         792             : ! !REVISION HISTORY:
         793             : !  01 May 2013 - C. Keller - Initial version
         794             : !  See https://github.com/geoschem/hemco for complete history
         795             : !EOP
         796             : !------------------------------------------------------------------------------
         797             : !BOC
         798             :     CHARACTER(LEN=255) :: MSG
         799             :
         800             :     !=====================================================================
         801             :     ! HCO_DepvAdd_2D_Dp begins here!
         802             :     !=====================================================================
         803             :
         804             :     ! Make sure target flux array in HcoState is allocated
         805           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Depv, &
         806           0 :                          HcoState%NX, HcoState%NY, RC )
         807           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         808             :
         809             :     ! Add array
         810             :     HcoState%Spc(HcoID)%Depv%Val(:,:) = &
         811           0 :        HcoState%Spc(HcoID)%Depv%Val(:,:) + Arr2D(:,:)
         812             :
         813             :     ! Return w/ success
         814           0 :     RC = HCO_SUCCESS
         815             :
         816             :   END SUBROUTINE HCO_DepvAdd_2D_Dp
         817             : !EOC
         818             : !------------------------------------------------------------------------------
         819             : !                   Harmonized Emissions Component (HEMCO)                    !
         820             : !------------------------------------------------------------------------------
         821             : !BOP
         822             : !
         823             : ! !IROUTINE: HCO_DepvAdd_2D_Sp
         824             : !
         825             : ! !DESCRIPTION: Routine HCO\_DepvAdd\_2D\_Sp adds the real*4 2D-array Arr2D
         826             : ! to the depostion array of species HcoID in HEMCO object HcoState.
         827             : !\\
         828             : !\\
         829             : ! !INTERFACE:
         830             : !
         831           0 :   SUBROUTINE HCO_DepvAdd_2D_Sp( HcoState, Arr2D, HcoID, RC )
         832             : !
         833             : ! !INPUT/OUTPUT PARAMETERS:
         834             : !
         835             :     TYPE(HCO_State), POINTER       :: HcoState
         836             :     INTEGER,         INTENT(INOUT) :: RC
         837             : !
         838             : ! !INPUT PARAMETERS:
         839             : !
         840             :     REAL(sp),        INTENT(IN   ) :: Arr2D(HcoState%NX,HcoState%NY)
         841             :     INTEGER,         INTENT(IN   ) :: HcoID
         842             : !
         843             : ! !REVISION HISTORY:
         844             : !  01 May 2013 - C. Keller - Initial version
         845             : !  See https://github.com/geoschem/hemco for complete history
         846             : !EOP
         847             : !------------------------------------------------------------------------------
         848             : !BOC
         849             :
         850             :     !=====================================================================
         851             :     ! HCO_DepvAdd_2D_Sp begins here!
         852             :     !=====================================================================
         853             :
         854             :     ! Make sure target flux array in HcoState is allocated
         855           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Depv, &
         856           0 :                          HcoState%NX, HcoState%NY, RC )
         857           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         858             :
         859             :     ! Add array
         860             :     HcoState%Spc(HcoID)%Depv%Val(:,:) = &
         861           0 :        HcoState%Spc(HcoID)%Depv%Val(:,:) + Arr2D(:,:)
         862             :
         863             :     ! Return w/ success
         864           0 :     RC = HCO_SUCCESS
         865             :
         866             :   END SUBROUTINE HCO_DepvAdd_2D_Sp
         867             : !EOC
         868             : !------------------------------------------------------------------------------
         869             : !                   Harmonized Emissions Component (HEMCO)                    !
         870             : !------------------------------------------------------------------------------
         871             : !BOP
         872             : !
         873             : ! !IROUTINE: HCO_DepvAdd_Dp
         874             : !
         875             : ! !DESCRIPTION: Routine HCO\_DepvAdd\_Dp adds value iVal to the deposition
         876             : ! array of species HcoID in HEMCO object HcoState. The value is placed at
         877             : ! location I, J of the array.
         878             : !\\
         879             : !\\
         880             : ! !INTERFACE:
         881             : !
         882           0 :   SUBROUTINE HCO_DepvAdd_Dp( HcoState, iVal, HcoID, I, J, RC )
         883             : !
         884             : ! !INPUT/OUTPUT PARAMETERS:
         885             : !
         886             :     TYPE(HCO_State), POINTER       :: HcoState
         887             :     INTEGER,         INTENT(INOUT) :: RC
         888             : !
         889             : ! !INPUT PARAMETERS:
         890             : !
         891             :     REAL(dp),        INTENT(IN   ) :: iVal
         892             :     INTEGER,         INTENT(IN   ) :: HcoID
         893             :     INTEGER,         INTENT(IN   ) :: I
         894             :     INTEGER,         INTENT(IN   ) :: J
         895             : !
         896             : ! !REVISION HISTORY:
         897             : !  01 May 2013 - C. Keller - Initial version
         898             : !  See https://github.com/geoschem/hemco for complete history
         899             : !EOP
         900             : !------------------------------------------------------------------------------
         901             : !BOC
         902             :     CHARACTER(LEN=255) :: MSG
         903             :
         904             :     !=====================================================================
         905             :     ! HCO_DepvAdd_Dp begins here!
         906             :     !=====================================================================
         907             :
         908             :     ! Check size dimensions
         909           0 :     IF ( I > HcoState%NX ) THEN
         910           0 :        MSG = 'Cannot add DP - i too high!'
         911           0 :        CALL HCO_ERROR ( MSG, RC )
         912           0 :        RETURN
         913             :     ENDIF
         914           0 :     IF ( J > HcoState%NY ) THEN
         915           0 :        MSG = 'Cannot add DP - j too high!'
         916           0 :        CALL HCO_ERROR ( MSG, RC )
         917           0 :        RETURN
         918             :     ENDIF
         919             :
         920             :     ! Make sure target flux array in HcoState is allocated
         921           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Depv, &
         922           0 :                          HcoState%NX, HcoState%NY, RC )
         923           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         924             :
         925             :     ! Add array
         926           0 :     HcoState%Spc(HcoID)%Depv%Val(I,J) = &
         927           0 :        HcoState%Spc(HcoID)%Depv%Val(I,J) + iVal
         928             :
         929             :     ! Return w/ success
         930           0 :     RC = HCO_SUCCESS
         931             :
         932             :   END SUBROUTINE HCO_DepvAdd_Dp
         933             : !EOC
         934             : !------------------------------------------------------------------------------
         935             : !                   Harmonized Emissions Component (HEMCO)                    !
         936             : !------------------------------------------------------------------------------
         937             : !BOP
         938             : !
         939             : ! !IROUTINE: HCO_DepvAdd_Sp
         940             : !
         941             : ! !DESCRIPTION: Routine HCO\_DepvAdd\_Sp adds value iVal to the deposition
         942             : ! array of species HcoID in HEMCO object HcoState. The value is placed at
         943             : ! location I, J of the array.
         944             : !\\
         945             : !\\
         946             : ! !INTERFACE:
         947             : !
         948           0 :   SUBROUTINE HCO_DepvAdd_Sp( HcoState, iVal, HcoID, I, J, RC )
         949             : !
         950             : ! !INPUT/OUTPUT PARAMETERS:
         951             : !
         952             :     TYPE(HCO_State), POINTER       :: HcoState
         953             :     INTEGER,         INTENT(INOUT) :: RC
         954             : !
         955             : ! !INPUT PARAMETERS:
         956             : !
         957             :     REAL(sp),        INTENT(IN   ) :: iVal
         958             :     INTEGER,         INTENT(IN   ) :: HcoID
         959             :     INTEGER,         INTENT(IN   ) :: I
         960             :     INTEGER,         INTENT(IN   ) :: J
         961             : !
         962             : ! !REVISION HISTORY:
         963             : !  01 May 2013 - C. Keller - Initial version
         964             : !  See https://github.com/geoschem/hemco for complete history
         965             : !EOP
         966             : !------------------------------------------------------------------------------
         967             : !BOC
         968             :     CHARACTER(LEN=255) :: MSG
         969             :
         970             :     !=====================================================================
         971             :     ! HCO_DepvAdd_Sp begins here!
         972             :     !=====================================================================
         973             :
         974             :     ! Check size dimensions
         975           0 :     IF ( I > HcoState%NX ) THEN
         976           0 :        MSG = 'Cannot add iVal - i too high!'
         977           0 :        CALL HCO_ERROR ( MSG, RC )
         978           0 :        RETURN
         979             :     ENDIF
         980           0 :     IF ( J > HcoState%NY ) THEN
         981           0 :        MSG = 'Cannot add iVal - j too high!'
         982           0 :        CALL HCO_ERROR ( MSG, RC )
         983           0 :        RETURN
         984             :     ENDIF
         985             :
         986             :     ! Make sure target flux array in HcoState is allocated
         987           0 :     CALL HCO_ArrAssert ( HcoState%Spc(HcoID)%Depv, &
         988           0 :                          HcoState%NX, HcoState%NY, RC )
         989           0 :     IF ( RC /=HCO_SUCCESS ) RETURN
         990             :
         991             :     ! Add array
         992           0 :     HcoState%Spc(HcoID)%Depv%Val(I,J) = &
         993           0 :        HcoState%Spc(HcoID)%Depv%Val(I,J) + iVal
         994             :
         995             :     ! Return w/ success
         996           0 :     RC = HCO_SUCCESS
         997             :
         998             :   END SUBROUTINE HCO_DepvAdd_Sp
         999             : !EOC
        1000             : !------------------------------------------------------------------------------
        1001             : !                   Harmonized Emissions Component (HEMCO)                    !
        1002             : !------------------------------------------------------------------------------
        1003             : !BOP
        1004             : !
        1005             : ! !IROUTINE: DiagnCheck
        1006             : !
        1007             : ! !DESCRIPTION: Subroutine DiagnCheck checks if the given emission array needs
        1008             : !               to be added to any auto-fill diagnostics. The diagnostics to be
        1009             : !               filled (if any) depend on the passed extension number, emission
        1010             : !               category and hierarchy, and the HEMCO species ID.
        1011             : !\\
        1012             : !\\
        1013             : ! !INTERFACE:
        1014             : !
        1015           0 :   SUBROUTINE DiagnCheck( HcoState,  ExtNr,    Cat,     &
        1016           0 :                          Hier,      HcoID,    Arr3D,   Arr3Dsp, &
        1017           0 :                          Arr2D,     Arr2Dsp,  MinDiagnLev,  RC   )
        1018             : !
        1019             : ! !USES:
        1020             : !
        1021             :     USE HCO_DIAGN_MOD
        1022             : !
        1023             : ! !INPUT PARAMETERS:
        1024             : !
        1025             :     INTEGER,         INTENT(IN   )           :: HcoID
        1026             :     INTEGER,         INTENT(IN   ), OPTIONAL :: ExtNr
        1027             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Cat
        1028             :     INTEGER,         INTENT(IN   ), OPTIONAL :: Hier
        1029             :     INTEGER,         INTENT(IN   ), OPTIONAL :: MinDiagnLev
        1030             : !
        1031             : ! !INPUT/OUTPUT PARAMETERS:
        1032             : !
        1033             :     TYPE(HCO_State), POINTER                 :: HcoState
        1034             :     REAL(dp),        INTENT(INOUT), OPTIONAL :: Arr3D(   HcoState%NX, &
        1035             :                                                          HcoState%NY, &
        1036             :                                                          HcoState%NZ )
        1037             :     REAL(sp),        INTENT(INOUT), OPTIONAL :: Arr3Dsp( HcoState%NX, &
        1038             :                                                          HcoState%NY, &
        1039             :                                                          HcoState%NZ )
        1040             :     REAL(dp),        INTENT(INOUT), OPTIONAL :: Arr2D(   HcoState%NX, &
        1041             :                                                          HcoState%NY )
        1042             :     REAL(sp),        INTENT(INOUT), OPTIONAL :: Arr2Dsp( HcoState%NX, &
        1043             :                                                          HcoState%NY )
        1044             :     INTEGER,         INTENT(INOUT)           :: RC
        1045             : !
        1046             : ! !REVISION HISTORY:
        1047             : !  20 Apr 2015 - C. Keller - Initial version
        1048             : !  See https://github.com/geoschem/hemco for complete history
        1049             : !EOP
        1050             : !------------------------------------------------------------------------------
        1051             : !BOC
        1052             : !
        1053             : ! !LOCAL VARIABLES:
        1054             : !
        1055             :     INTEGER             :: AFL, XT, CT, HR
        1056             :     CHARACTER(LEN=255)  :: LOC
        1057             :
        1058             :     !=====================================================================
        1059             :     ! DiagnCheck begins here!
        1060             :     !=====================================================================
        1061             :
        1062             :     ! Initialize values
        1063           0 :     LOC = 'DiagnCheck (HCO_FLUXARR_MOD.F90)'
        1064             :
        1065             :     ! Autofill level:
        1066             :     ! 1=species level, 2=ExtNr level, 3=Cat level, 4=Hier level
        1067           0 :     AFL =  1
        1068             :
        1069             :     ! ExtNr, Cat & Hier
        1070           0 :     XT  = -1
        1071           0 :     CT  = -1
        1072           0 :     HR  = -1
        1073             :
        1074             :     ! Set extension number, category, and hierarchy
        1075           0 :     IF ( PRESENT(ExtNr) ) THEN
        1076           0 :        XT  = ExtNr
        1077           0 :        AFL = 2
        1078             :
        1079             :        ! Consider category only within extension ...
        1080           0 :        IF ( PRESENT(Cat) ) THEN
        1081           0 :           IF ( Cat > 0 ) THEN
        1082           0 :              CT  = Cat
        1083           0 :              AFL = 3
        1084             :           ENDIF
        1085             :
        1086             :           ! Consider hierarchy only within category ...
        1087           0 :           IF ( AFL==3 .AND. PRESENT(Hier) ) THEN
        1088           0 :              IF ( Hier > 0 ) THEN
        1089           0 :                 HR  = Hier
        1090           0 :                 AFL = 4
        1091             :              ENDIF
        1092             :           ENDIF
        1093             :        ENDIF
        1094             :     ENDIF
        1095             :
        1096           0 :     IF ( PRESENT(MinDiagnLev) ) THEN
        1097           0 :        AFL = MIN(AFL,MinDiagnLev)
        1098             :     ENDIF
        1099             :
        1100             :     ! Check if we need to call diagnostics
        1101           0 :     IF ( Diagn_AutoFillLevelDefined(HcoState%Diagn,AFL) ) THEN
        1102             :
        1103             :        ! 3D HP array
        1104           0 :        IF ( PRESENT(Arr3D) ) THEN
        1105             :           CALL Diagn_Update( HcoState, ExtNr=XT,    Cat=CT,     &
        1106             :                              Hier=HR,  HcoID=HcoID, AutoFill=1, &
        1107           0 :                              Array3D=Arr3D, MinDiagnLev=MinDiagnLev, RC=RC )
        1108           0 :           IF ( RC /= HCO_SUCCESS ) THEN
        1109           0 :               CALL HCO_ERROR( 'ERROR 10', RC, THISLOC=LOC )
        1110           0 :               RETURN
        1111             :           ENDIF
        1112             :        ENDIF
        1113             :
        1114             :        ! 3D SP array
        1115           0 :        IF ( PRESENT(Arr3Dsp) ) THEN
        1116             :           CALL Diagn_Update( HcoState, ExtNr=XT,    Cat=CT,     &
        1117             :                              Hier=HR,  HcoID=HcoID, AutoFill=1, &
        1118           0 :                              Array3D=Arr3Dsp, MinDiagnLev=MinDiagnLev, RC=RC )
        1119           0 :           IF ( RC /= HCO_SUCCESS ) THEN
        1120           0 :               CALL HCO_ERROR( 'ERROR 11', RC, THISLOC=LOC )
        1121           0 :               RETURN
        1122             :           ENDIF
        1123             :        ENDIF
        1124             :
        1125             :        ! 2D HP array
        1126           0 :        IF ( PRESENT(Arr2D) ) THEN
        1127             :           CALL Diagn_Update( HcoState, ExtNr=XT,    Cat=CT,     &
        1128             :                              Hier=HR,  HcoID=HcoID, AutoFill=1, &
        1129           0 :                              Array2D=Arr2D, MinDiagnLev=MinDiagnLev, RC=RC )
        1130           0 :           IF ( RC /= HCO_SUCCESS ) THEN
        1131           0 :               CALL HCO_ERROR( 'ERROR 12', RC, THISLOC=LOC )
        1132           0 :               RETURN
        1133             :           ENDIF
        1134             :        ENDIF
        1135             :
        1136             :        ! 2D SP array
        1137           0 :        IF ( PRESENT(Arr2Dsp) ) THEN
        1138             :           CALL Diagn_Update( HcoState, ExtNr=XT,    Cat=CT,     &
        1139             :                              Hier=HR,  HcoID=HcoID, AutoFill=1, &
        1140           0 :                              Array2D=Arr2Dsp, MinDiagnLev=MinDiagnLev, RC=RC )
        1141           0 :           IF ( RC /= HCO_SUCCESS ) THEN
        1142           0 :               CALL HCO_ERROR( 'ERROR 13', RC, THISLOC=LOC )
        1143           0 :               RETURN
        1144             :           ENDIF
        1145             :        ENDIF
        1146             :
        1147             :     ENDIF
        1148             :
        1149             :     ! Return w/ success
        1150           0 :     RC = HCO_SUCCESS
        1151             :
        1152           0 :   END SUBROUTINE DiagnCheck
        1153             : !EOC
        1154             : END MODULE HCO_FluxArr_Mod

Generated by: LCOV version 1.14