LCOV - code coverage report
Current view: | top level - hemco - hemco_interface.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 27 | 904 | 3.0 %
Date: | 2024-12-17 22:39:59 |  | Functions: | 1 | 9 | 11.1 %

              Line data    Source code
           1             : #define VERIFY_(A) if(.not.HCO_ESMF_VRFY(A,subname,__LINE__)) stop -1
           2             : #define ASSERT_(A) if(.not.HCO_ESMF_ASRT(A,subname,__LINE__)) stop -1
           3             : !------------------------------------------------------------------------------
           4             : !                    Harmonized Emissions Component (HEMCO)                   !
           5             : !------------------------------------------------------------------------------
           6             : !BOP
           7             : !
           8             : ! !MODULE: hemco_interface
           9             : !
          10             : ! !DESCRIPTION: Module HEMCO\_INTERFACE is the HEMCO-CESM interface module.
          11             : !               CESM operates on chunks thus the interface is called HCOI\_Chunk.
          12             : !               Internally it uses a gridded component to interact with the CAM
          13             : !               physics grid; these functions are internal and called HCO\_GC...
          14             : !\\
          15             : !\\
          16             : ! !INTERFACE:
          17             : !
          18             : module hemco_interface
          19             : !
          20             : ! !USES:
          21             : !
          22             :     ! ESMF function wrappers
          23             :     use hco_esmf_wrappers,        only: HCO_ESMF_VRFY, HCO_ESMF_ASRT
          24             :
          25             :     ! HEMCO ESMF Grid helpers and properties
          26             :     use hco_esmf_grid,            only: HCO_Grid_Init, HCO_Grid_UpdateRegrid
          27             :     use hco_esmf_grid,            only: HCO_Grid_HCO2CAM_2D, HCO_Grid_HCO2CAM_3D
          28             :     use hco_esmf_grid,            only: HCO_Grid_CAM2HCO_2D, HCO_Grid_CAM2HCO_3D
          29             :     use hco_esmf_grid,            only: IM, JM, LM
          30             :     use hco_esmf_grid,            only: XMid, XEdge, YMid, YEdge, YEdge_R, YSin, AREA_M2, Ap, Bp
          31             :     use hco_esmf_grid,            only: my_IM, my_JM
          32             :     use hco_esmf_grid,            only: my_IS, my_IE, my_JS, my_JE, my_CE
          33             :
          34             :     ! CAM export helpers
          35             :     use hco_cam_exports,          only: HCO_Exports_Init
          36             :     use hco_cam_exports,          only: HCO_Export_Pbuf_AddField
          37             :     use hco_cam_exports,          only: HCO_Export_History_CAM2D, HCO_Export_History_CAM3D
          38             :     use hco_cam_exports,          only: HCO_Export_Pbuf_CAM2D, HCO_Export_Pbuf_CAM3D
          39             :     use hco_cam_exports,          only: hco_pbuf2d  ! Allow for pbuf handler to be passed to exports component.
          40             :
          41             :     ! CAM import helpers
          42             :     use hco_cam_convert_state_mod,only: HCOI_Allocate_All, CAM_GetBefore_HCOI, CAM_RegridSet_HCOI
          43             :
          44             :     ! Controls
          45             :     use cam_abortutils,           only: endrun      ! fatal terminator
          46             :     use cam_logfile,              only: iulog       ! output log handle
          47             :
          48             :     ! Species information
          49             :     use constituents,             only: pcnst       ! # of species
          50             :     use constituents,             only: cnst_name   ! species names
          51             :     use constituents,             only: cnst_mw     ! advected mass
          52             :     use mo_chem_utls,             only: get_spc_ndx ! IND_ equivalent
          53             :
          54             :     ! Check chemistry option
          55             :     use chemistry,                only: chem_is
          56             :
          57             :     ! Grid
          58             :     use ppgrid,                   only: pcols, pver ! Cols, verts
          59             :     use ppgrid,                   only: begchunk, endchunk ! Chunk idxs
          60             :
          61             :     ! Time
          62             :     use time_manager,             only: get_curr_time, get_prev_time, get_curr_date
          63             :     use time_manager,             only: get_step_size
          64             :
          65             :     ! ESMF types
          66             :     use ESMF,                     only: ESMF_State, ESMF_Clock, ESMF_GridComp
          67             :     use ESMF,                     only: ESMF_KIND_R8, ESMF_KIND_I4, ESMF_SUCCESS
          68             :
          69             :     ! HEMCO types
          70             :     use HCO_Error_Mod,            only: hp          ! HEMCO precision
          71             :     use HCO_Error_Mod,            only: sp          ! HEMCO single precision used for Ptrs
          72             :     use HCO_Error_Mod,            only: HCO_SUCCESS, HCO_FAIL, HCO_VERSION
          73             :     use HCO_State_Mod,            only: HCO_State
          74             :     use HCOX_State_Mod,           only: Ext_State
          75             :     use HCO_Types_Mod,            only: ConfigObj
          76             :
          77             :     use shr_kind_mod,             only: r8 => shr_kind_r8
          78             :
          79             :     implicit none
          80             :     private
          81             : !
          82             : ! !PRIVATE MEMBER FUNCTIONS:
          83             : !
          84             :     private :: HCO_GC_Init
          85             :     private :: HCO_GC_SetServices
          86             :     private :: HCO_GC_Run
          87             :     private :: HCO_GC_Final
          88             :
          89             :     private :: HCOI_Initialize_Pbuf
          90             : !
          91             : ! !PUBLIC MEMBER FUNCTIONS:
          92             : !
          93             :     public  :: hemco_readnl
          94             :     public  :: HCOI_Chunk_Init
          95             :     public  :: HCOI_Chunk_Run
          96             :     public  :: HCOI_Chunk_Final
          97             : !
          98             : ! !REMARKS:
          99             : !  This file is both the interface of HEMCO component to CAM and the manager of the
         100             : !  underlying HEMCO gridded component (HCO\_GC\_*).
         101             : !
         102             : !  The whole file is getting a little long in the tooth, though. It might be reorg-
         103             : !  anized in the future to service hemco_init/run/final which manages the gridded
         104             : !  components, which in turn call the HEMCO chunk interface (HCOI\_Chunk\_*).
         105             : !
         106             : !  For now, the HEMCO chunk interfaces (HCOI\_Chunk\_*) are called in directly from
         107             : !  CAM cam_control.F90. I am not in the mood of writing a wrapper for now, but this
         108             : !  could be abstracted in the future. (hplin, 3/29/20)
         109             : !
         110             : !  On a side note, this is the 8th day of living in the 2019-nCoV scare. I miss
         111             : !  matcha tea and would die to eat some sweets.
         112             : !
         113             : !  It is now October 29 and COVID-19 is still raging across the globe; it feels
         114             : !  like time has frozen itself since March 21, and we've all been "on one long Zoom call"
         115             : !  ever since.
         116             : !
         117             : !  All I hope for 2021, is that the world does not pull a "You can now play as Luigi" on me.
         118             : !
         119             : !  Updated 2/24/21 from T. Fritz: Now uses constituents list, since short-term species are
         120             : !  not emitted. See PR: https://github.com/jimmielin/HEMCO_CESM/pull/5
         121             : !
         122             : !  It is now May 15, 2021 and I am vaccinated. Can we visit other peoples homes now?
         123             : !  ref: xkcd.com/2454
         124             : !
         125             : ! !REVISION HISTORY:
         126             : !  29 Jan 2020 - H.P. Lin    - Initial version
         127             : !EOP
         128             : !------------------------------------------------------------------------------
         129             : !BOC
         130             : !
         131             : ! !PRIVATE TYPES:
         132             : !
         133             :     type(ESMF_GridComp)              :: HCO_GridComp        ! HEMCO GridComp
         134             :     type(ESMF_State)                 :: HCO_GridCompState   ! HEMCO GridComp Import/Export State
         135             :
         136             :     character(len=256)               :: HcoRoot             ! HEMCO data root path
         137             :     character(len=256)               :: HcoConfigFile       ! HEMCO configuration file path
         138             :     character(len=256)               :: HcoDiagnFile        ! HEMCO diagnostics config file path
         139             :     type(ConfigObj), pointer         :: HcoConfig => NULL()
         140             :
         141             :     type(HCO_State), pointer, public :: HcoState  => NULL()
         142             :     type(Ext_State), pointer, public :: ExtState  => NULL()
         143             :
         144             :     ! HEMCO internal grid parameters
         145             :     integer                          :: HcoGridIM           ! # of lons
         146             :     integer                          :: HcoGridJM           ! # of lats
         147             :
         148             :     ! HEMCO configuration parameters that are set by namelist in CESM
         149             :     integer                          :: HcoFixYY            ! if > 0, force 'Emission year'
         150             :
         151             :     ! Last execution times for the HEMCO component. We are assuming that time
         152             :     ! flows unidirectionally (and forwards, for now). (hplin, 3/30/20)
         153             :     integer                          :: last_HCO_day, last_HCO_second
         154             :
         155             :     ! Meteorological fields used by HEMCO to be regridded to the HEMCO grid (hplin, 3/31/20)
         156             :     ! We have to store the fields because the regridding can only take place within the GridComp.
         157             :     ! Fields are allocated after the internal grid is initialized (so my_* are avail)
         158             :     !
         159             :     ! Moved to hco_cam_convert_state_mod, 12/16/20
         160             :
         161             : contains
         162             : !EOC
         163             : !------------------------------------------------------------------------------
         164             : !                    Harmonized Emissions Component (HEMCO)                   !
         165             : !------------------------------------------------------------------------------
         166             : !BOP
         167             : !
         168             : ! !IROUTINE: hemco_readnl
         169             : !
         170             : ! !DESCRIPTION: Reads the namelist from cam/src/control/runtime_opts.
         171             : !\\
         172             : !\\
         173             : ! !INTERFACE:
         174             : !
         175        1536 :     subroutine hemco_readnl( nlfile )
         176             : !
         177             : ! !USES:
         178             : !
         179             :         use namelist_utils, only: find_group_name
         180             :         use units,          only: getunit, freeunit
         181             :         use spmd_utils,     only: mpi_real8, mpi_logical, mpi_integer, mpi_character
         182             :         use spmd_utils,     only: masterproc, mpicom, masterprocid
         183             : !
         184             : ! !INPUT PARAMETERS:
         185             : !
         186             :         character(len=*), intent(in) :: nlfile ! namelist file
         187             : !
         188             : ! !REVISION HISTORY:
         189             : !  31 Jan 2020 - H.P. Lin    - Initial version
         190             : !EOP
         191             : !------------------------------------------------------------------------------
         192             : !BOC
         193             : !
         194             : ! !LOCAL VARIABLES:
         195             : !
         196             :         integer :: unitn, ierr
         197             :         character(len=*), parameter  :: subname = 'hemco_readnl'
         198             :         character(len=256)           :: hemco_data_root = ''
         199             :         character(len=256)           :: hemco_config_file = 'HEMCO_Config.rc'
         200             :         character(len=256)           :: hemco_diagn_file = 'HEMCO_Diagn.rc'
         201             :         integer                      :: hemco_grid_xdim = 0
         202             :         integer                      :: hemco_grid_ydim = 0
         203             :         integer                      :: hemco_emission_year = -1
         204             :
         205             :         namelist /hemco_nl/ hemco_data_root, hemco_config_file, hemco_diagn_file, hemco_grid_xdim, hemco_grid_ydim, hemco_emission_year
         206             :
         207             :         ! Read namelist on master proc
         208             :         ! ...
         209        1536 :         if(masterproc) then
         210           2 :             unitn = getunit()
         211           2 :             open(unitn, file=trim(nlfile), status='old')
         212           2 :             call find_group_name(unitn, 'hemco_nl', status=ierr)
         213           2 :             if(ierr == 0) then
         214           0 :                 read(unitn, hemco_nl, iostat=ierr)
         215           0 :                 if(ierr /= 0) then
         216           0 :                     call endrun(subname // ':: ERROR reading namelist')
         217             :                 endif
         218             :             endif
         219           2 :             close(unitn)
         220           2 :             call freeunit(unitn)
         221             :
         222           2 :             write(iulog,*) "hemco_readnl: hemco data root is at = ", trim(hemco_data_root)
         223           2 :             write(iulog,*) "hemco_readnl: hemco config file = ", trim(hemco_config_file)
         224           2 :             write(iulog,*) "hemco_readnl: hemco diagn file = ", trim(hemco_diagn_file)
         225           2 :             write(iulog,*) "hemco_readnl: hemco internal grid dimensions will be ", hemco_grid_xdim, " x ", hemco_grid_ydim
         226             :
         227           2 :             if(hemco_emission_year .gt. 0) then
         228           0 :                 write(iulog,*) "hemco_readnl: hemco will force emissions year at = ", hemco_emission_year
         229             :             else
         230           2 :                 write(iulog,*) "hemco_readnl: hemco will use emissions from the CESM clock"
         231             :             endif
         232             :         endif
         233             :
         234             :         ! MPI Broadcast Namelist variables
         235        1536 :         call mpi_bcast(hemco_data_root, len(hemco_data_root), mpi_character, masterprocid, mpicom, ierr)
         236        1536 :         call mpi_bcast(hemco_config_file, len(hemco_config_file), mpi_character, masterprocid, mpicom, ierr)
         237        1536 :         call mpi_bcast(hemco_diagn_file, len(hemco_diagn_file), mpi_character, masterprocid, mpicom, ierr)
         238        1536 :         call mpi_bcast(hemco_grid_xdim, 1, mpi_integer, masterprocid, mpicom, ierr)
         239        1536 :         call mpi_bcast(hemco_grid_ydim, 1, mpi_integer, masterprocid, mpicom, ierr)
         240        1536 :         call mpi_bcast(hemco_emission_year, 1, mpi_integer, masterprocid, mpicom, ierr)
         241             :
         242             :         ! Save this to the module information
         243        1536 :         HcoRoot       = hemco_data_root
         244        1536 :         HcoConfigFile = hemco_config_file
         245        1536 :         HcoDiagnFile  = hemco_diagn_file
         246        1536 :         HcoGridIM     = hemco_grid_xdim
         247        1536 :         HcoGridJM     = hemco_grid_ydim
         248        1536 :         HcoFixYY      = hemco_emission_year
         249        1536 :     end subroutine hemco_readnl
         250             : !EOC
         251             : !------------------------------------------------------------------------------
         252             : !                    Harmonized Emissions Component (HEMCO)                   !
         253             : !------------------------------------------------------------------------------
         254             : !BOP
         255             : !
         256             : ! !IROUTINE: HCOI_Chunk_Init
         257             : !
         258             : ! !DESCRIPTION: HCOI\_Chunk\_Init is the initialization method for the CAM
         259             : !  interface to HEMCO.
         260             : !\\
         261             : !\\
         262             : ! !INTERFACE:
         263             : !
         264           0 :     subroutine HCOI_Chunk_Init()
         265             : !
         266             : ! !USES:
         267             : !
         268             :         use cam_logfile,      only: iulog
         269             :         use spmd_utils,       only: masterproc, mpicom, masterprocid
         270             :         use spmd_utils,       only: npes, iam
         271             :         use perf_mod,         only: t_startf, t_stopf
         272             :
         273             :         use mpi,              only: MPI_INTEGER
         274             :         use ESMF,             only: ESMF_VM, ESMF_VMGetCurrent, ESMF_VMGet
         275             :         use ESMF,             only: ESMF_GridCompCreate, ESMF_GridCompInitialize
         276             :         use ESMF,             only: ESMF_GridCompSetServices
         277             :         use ESMF,             only: ESMF_StateCreate
         278             :
         279             :         use ESMF,             only: ESMF_Initialize, ESMF_LOGKIND_MULTI
         280             :
         281             :         ! CAM instance information
         282             :         use cam_instance,     only: inst_index, inst_name
         283             :
         284             :         ! CAM history output (to be moved somewhere later)
         285             :         use cam_history,      only: addfld, add_default, horiz_only
         286             :
         287             :         ! Get extfrc list check for 3-D emissions capability
         288             :         use mo_chem_utls,     only: get_extfrc_ndx
         289             :
         290             :         ! HEMCO Initialization
         291             :         use HCO_Config_Mod,   only: Config_ReadFile, ConfigInit
         292             :         use HCO_Driver_Mod,   only: HCO_Init
         293             :         use HCO_Error_Mod,    only: HCO_LOGFILE_OPEN
         294             :         use HCO_LogFile_Mod,  only: HCO_Spec2Log
         295             :         use HCO_State_Mod,    only: HcoState_Init
         296             :         use HCO_Types_Mod,    only: ConfigObj
         297             :         use HCO_Types_Mod,    only: ListCont
         298             :         use HCO_VertGrid_Mod, only: HCO_VertGrid_Define
         299             :
         300             :         ! For some overriding work in HEMCO configuration
         301             :         use HCO_ExtList_Mod,  only: CoreNr
         302             :         use HCO_Types_Mod,    only: Opt, Ext
         303             :
         304             :         ! HEMCO extensions initialization
         305             :         use HCOX_Driver_Mod,  only: HCOX_Init
         306             : !
         307             : ! !REMARKS:
         308             : !  None currently.
         309             : !
         310             : ! !REVISION HISTORY:
         311             : !  06 Feb 2020 - H.P. Lin    - Initial version
         312             : !  15 Dec 2020 - H.P. Lin    - Implement HEMCO extensions that do require met
         313             : !  23 Mar 2021 - H.P. Lin    - Now export for diagnostics too
         314             : !  12 Jan 2023 - H.P. Lin    - Optimize memory usage by only allocating 2-D/3-D as needed
         315             : !  15 Jun 2023 - H.P. Lin    - Now override HEMCO_Diagn.rc file path and ROOT path in CESM env.
         316             : !EOP
         317             : !------------------------------------------------------------------------------
         318             : !BOC
         319             : !
         320             : ! !LOCAL VARIABLES:
         321             : !
         322             :         character(len=*), parameter  :: subname = 'HCOI_Chunk_Init'
         323             :         integer                      :: RC                   ! ESMF return code
         324             :         integer                      :: HMRC                 ! HEMCO return code
         325             :
         326             :         integer                      :: N                    ! Loop idx
         327             :
         328             :         ! Gridded component properties.
         329             :         ! Note that while edyn_grid_comp initializes the GridComp directly using
         330             :         ! cam_instance's inst_name, I think this may cause namespace clashing.
         331             :         ! So I'll be prefixing this with hco_ just incase.
         332             :         character(len=32)            :: HCO_GC_InstName = ''
         333             :         type(ESMF_VM)                :: hco_esmf_vm
         334             :
         335             :         ! MPI stuff
         336             :         integer                      :: localPET, PETcount
         337           0 :         integer, allocatable         :: PETlist(:)           ! PETs for each instance of the physics grid
         338             :
         339             :         ! HEMCO properties
         340             :         integer                      :: nHcoSpc
         341             :
         342             :         ! Temporary string for species naming in exports
         343             :         character(len=128)           :: exportName, exportDesc
         344             :         character(len=128)           :: exportNameTmp
         345             :
         346             :         ! Timing properties
         347             :         integer                      :: year, month, day, tod
         348             :         integer                      :: hour, minute, second, dt
         349             :         integer                      :: prev_day, prev_s, now_day, now_s
         350             :         integer                      :: stepsize_tmp
         351             :
         352             :         ! Temporaries
         353             :         logical                      :: IsExtfrc3DEmis
         354             :
         355             :         ! Temporaries for HEMCO cycling
         356             :         logical                      :: OptFound
         357             :         type(Ext), pointer           :: ThisExt
         358             :         type(Opt), pointer           :: ThisOpt
         359             :
         360             :         !-----------------------------------------------------------------------
         361             :
         362           0 :         call t_startf('HCOI_Chunk_Init')
         363             :
         364           0 :         if(masterproc) then
         365           0 :             write(iulog,*) "%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%"
         366           0 :             write(iulog,*) "HEMCO: Harmonized Emissions Component"
         367           0 :             write(iulog,*) "https://doi.org/10.5194/gmd-14-5487-2021 (Lin et al., 2021)"
         368           0 :             write(iulog,*) "HEMCO_CESM interface version 2.0.0"
         369           0 :             write(iulog,*) "You are using HEMCO version ", ADJUSTL(HCO_VERSION)
         370           0 :             write(iulog,*) "ROOT: ", HcoRoot
         371           0 :             write(iulog,*) "Config File: ", HcoConfigFile
         372           0 :             write(iulog,*) "Diagn File: ", HcoDiagnFile
         373           0 :             write(iulog,*) "%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%"
         374             :         endif
         375             :
         376             :         ! Assume success
         377           0 :         RC = ESMF_SUCCESS
         378           0 :         HMRC = HCO_SUCCESS
         379             :
         380             :         !-----------------------------------------------------------------------
         381             :         ! Get time properties
         382             :         !-----------------------------------------------------------------------
         383           0 :         call get_prev_time(prev_day, prev_s) ! 0 0
         384           0 :         call get_curr_time(now_day, now_s)   ! 0 0
         385           0 :         call get_curr_date(year, month, day, tod) ! 2005 1 1 0
         386             :
         387             :         ! In order to allow first timestep to be ran, set last HEMCO day and hour to
         388             :         ! negative at initialization. prev_time from ESMF is always zero.
         389           0 :         last_HCO_day    = -1
         390           0 :         last_HCO_second = -1
         391           0 :         write(iulog,*) "HEMCO debug: prev_day, prev_s, now_day, now_s, y, m, d, tod", prev_day, prev_s, now_day, now_s, year, month, day, tod
         392             :
         393             :         !-----------------------------------------------------------------------
         394             :         ! Setup ESMF wrapper gridded component
         395             :         ! Adapted from edyn_grid_comp_init
         396             :         !-----------------------------------------------------------------------
         397           0 :         call ESMF_VMGetCurrent(hco_esmf_vm, rc=RC)
         398           0 :         ASSERT_(RC==ESMF_SUCCESS)
         399             :
         400           0 :         call ESMF_VMGet(hco_esmf_vm, localPet=localPET, petCount=PETcount, rc=RC)
         401           0 :         ASSERT_(RC==ESMF_SUCCESS)
         402             :
         403             :         ! Allocate and collect PETs for each instance of the physics grid
         404           0 :         allocate(PETlist(npes))
         405             :             ! sendbuf, sendcount, sendtype, recvbuf, recvcount, recvtype, comm, ierror
         406           0 :         call mpi_allgather(localPET, 1, MPI_INTEGER, PETlist, 1, MPI_INTEGER, mpicom, RC)
         407             :
         408             :         ! Create ESMF gridded component
         409             :         ! This gridded component's IRF routines are defined in hemco_interface::HCO_GC_SetServices
         410             :         ! See there for more information. (hplin, 2/6/20)
         411           0 :         HCO_GC_InstName = 'HCO_' // trim(inst_name)
         412           0 :         HCO_GridComp = ESMF_GridCompCreate(name=trim(HCO_GC_InstName), petList=PETlist, rc=RC)
         413           0 :         ASSERT_(RC==ESMF_SUCCESS)
         414             :
         415             :         ! Create a dummy import / export state.
         416           0 :         call ESMF_GridCompSetServices(HCO_GridComp, HCO_GC_SetServices, rc=RC)
         417           0 :         ASSERT_(RC==ESMF_SUCCESS)
         418             :
         419           0 :         HCO_GridCompState = ESMF_StateCreate(name='HEMCO GridComp State', rc=RC)
         420           0 :         ASSERT_(RC==ESMF_SUCCESS)
         421             :
         422           0 :         call ESMF_GridCompInitialize(HCO_GridComp, importState=HCO_GridCompState, exportState=HCO_GridCompState, rc=RC)
         423           0 :         ASSERT_(RC==ESMF_SUCCESS)
         424             :
         425             :         !if(masterproc) then
         426             :         !    write(iulog,*) "> Initialized ESMF environment successfully! localPET, PETcount", localPET, PETcount
         427             :         !    write(iulog,*) "> iam, npes", iam, npes
         428             :         !    write(iulog,*) "> PETlist", PETlist
         429             :         !endif
         430             :
         431             :         !-----------------------------------------------------------------------
         432             :         ! Setup a lat-lon "HEMCO" intermediate grid
         433             :         !-----------------------------------------------------------------------
         434             :         ! TODO: For now, # of PEs to use for HEMCO will be total # of PEs.
         435             :         ! These will all have to be specified in the HEMCO namelist later on.
         436             :
         437             :         ! The number of grid dimensions can be specified in atm namelist for
         438             :         ! hemco_grid_xdim, hemco_grid_ydim. note that half-sized polar boxes are made
         439             :         ! so increase the y-dim by one.
         440             :         ! 288x201 = 0.9x1.25
         441             :         ! 144x91  = 2.0x2.5
         442             :
         443             :         ! Verify that the grid is in a reasonable state
         444           0 :         if(HcoGridIM .le. 1 .or. HcoGridJM .le. 1) then
         445           0 :             call endrun("Invalid HEMCO grid parameters - too small - in &hemco namelist. Specify hemco_grid_xdim and hemco_grid_ydim as # of grid boxes in each dimension")
         446             :         endif
         447             :
         448           0 :         if(mod(HcoGridJM, 2) .ne. 1) then
         449           0 :             call endrun("Invalid HEMCO grid parameters - hemco_grid_ydim needs to be odd - in &hemco namelist. This is because y-dim has half-sized polar boxes.")
         450             :         endif
         451             :
         452             :         ! Initialize the HEMCO intermediate grid
         453           0 :         call HCO_Grid_Init (IM_in = HcoGridIM, JM_in = HcoGridJM, nPET_in = npes, RC=RC)
         454           0 :         ASSERT_(RC==ESMF_SUCCESS)
         455             :
         456           0 :         if(masterproc) then
         457           0 :             write(iulog,*) "> Initialized HEMCO Grid environment successfully!"
         458           0 :             write(iulog,*) "> Global Dimensions: ", HcoGridIM, HcoGridJM, LM
         459           0 :             write(iulog,*) "> my_IM, my_JM, LM, my_CE", my_IM, my_JM, LM, my_CE
         460             :         endif
         461             :
         462             :         !-----------------------------------------------------------------------
         463             :         ! Update HEMCO regrid descriptors for the first time.
         464             :         !-----------------------------------------------------------------------
         465           0 :         call HCO_Grid_UpdateRegrid(RC=RC)
         466           0 :         ASSERT_(RC==ESMF_SUCCESS)
         467             :
         468           0 :         if(masterproc) then
         469           0 :             write(iulog,*) "> First refresh of HEMCO Regrid descriptors"
         470             :         endif
         471             :
         472             :         !-----------------------------------------------------------------------
         473             :         ! Allocate HEMCO meteorological objects
         474             :         ! We are allocating globally for the whole HEMCO component here. This may
         475             :         ! clash if my_CE changes (multiple CAM instances). To be verified.
         476             :         ! Should be a easy fix regardless, simply allocate and dealloc in the run
         477             :         ! (hplin, 3/31/20)
         478             :         !-----------------------------------------------------------------------
         479           0 :         call HCOI_Allocate_All()
         480             :
         481           0 :         if(masterproc) then
         482           0 :             write(iulog,*) "> Allocated HEMCO temporary met fields"
         483             :         endif
         484             :
         485             :         !-----------------------------------------------------------------------
         486             :         ! Initialize CAM export component
         487             :         !-----------------------------------------------------------------------
         488           0 :         call HCO_Exports_Init()
         489             :
         490           0 :         if(masterproc) then
         491           0 :             write(iulog,*) "> Initialize HEMCO/CAM exports component"
         492             :         endif
         493             :
         494             :         ! Test only hplin 3/3/20: add a dummy history field in CAM to test HEMCO
         495             :         ! grid is correctly reflected.
         496             :         ! HCO_TEST outputs in the physics mesh.
         497             :         ! AvgFlag: (cam_history) A mean, B mean00z, I instant, X max, M min, S stddev
         498             :         !
         499             :         ! This call should eventually be reflected elsewhere?
         500             :         call addfld("DIAG_CAM_TEST", (/'lev'/), 'I', '1',          &
         501             :                     'HEMCO Debug, PETID written on CAM',             &
         502           0 :                     gridname="physgrid")
         503             :
         504             :         ! Enable default for debugging:
         505             :         ! call add_default("DIAG_CAM_TEST", 2, 'I')      ! Make this field always ON
         506             :
         507             :         call addfld("DIAG_HCO_TEST", (/'lev'/), 'I', '1',          &
         508             :                     'HEMCO Debug Data',             &
         509           0 :                     gridname="physgrid")
         510             :
         511             :         ! Enable default for debugging:
         512             :         ! call add_default("DIAG_HCO_TEST", 2, 'I')      ! Make this field always ON
         513             :
         514             :         !-----------------------------------------------------------------------
         515             :         ! Initialize the HEMCO configuration object...
         516             :         !-----------------------------------------------------------------------
         517             :         !if(masterproc) write(iulog,*) "> Initializing HCO configuration object"
         518             :
         519             :         ! We are using pcnst here, which is # of constituents.
         520           0 :         nHcoSpc             = pcnst          ! # of hco species?
         521             :
         522           0 :         call ConfigInit(HcoConfig, HMRC, nModelSpecies=nHcoSpc)
         523           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         524             :
         525           0 :         HcoConfig%amIRoot   = masterproc
         526             :         ! HcoConfig%amIRoot   = .true. ! for debug only so verbosity is higher
         527             :
         528           0 :         HcoConfig%MetField  = 'MERRA2'
         529           0 :         HcoConfig%GridRes   = ''
         530             :
         531             :         !-----------------------------------------------------------------------
         532             :         ! Retrieve the species list and register exports
         533             :         !-----------------------------------------------------------------------
         534             :         ! Below we directly use nHcoSpc which corresponds to the number of constituents
         535             :         ! (nHcoSpc = pcnst). Only constituents may be advected.
         536           0 :         HcoConfig%nModelSpc = nHcoSpc
         537           0 :         HcoConfig%nModelAdv = nHcoSpc            ! # of adv spc?
         538             :
         539             :         !if(masterproc) write(iulog,*) "> Initializing HCO species list!"
         540             :
         541           0 :         do N = 1, nHcoSpc
         542           0 :             HcoConfig%ModelSpc(N)%ModID   = N ! model id
         543             :
         544           0 :             HcoConfig%ModelSpc(N)%SpcName = trim(cnst_name(N)) ! only constituents can be emitted
         545             :
         546             :             !----------------------------------------------
         547             :             ! Register export properties.
         548             :             !----------------------------------------------
         549             :             ! History output (this will be moved to hco_cam_exports soon hopefully)
         550           0 :             exportName = 'HCO_' // trim(HcoConfig%ModelSpc(N)%SpcName)
         551             :
         552             :             !if(masterproc) write(iulog,*) "Exported exportName " // trim(exportName) // " to history"
         553             :
         554             :             ! Physics buffer
         555             :             ! Note that _AddField will prepend HCO_, so do not add it here
         556             :             !
         557             :             ! Update hplin 1/13/23: Verify if part of extfrc_lst. If yes,
         558             :             ! then allocate as 3-D. Otherwise, this field can be allocated
         559             :             ! as 2-D. This scan is somewhat intensive as it uses get_extfrc_ndx
         560             :             ! which loops through extcnt in extfrc_lst.
         561           0 :             IsExtfrc3DEmis = (get_extfrc_ndx(trim(HcoConfig%ModelSpc(N)%SpcName)) .gt. 0)
         562             :
         563           0 :             if(masterproc) write(iulog,*) "Setting up HEMCO exportName " // trim(exportName), IsExtfrc3DEmis
         564           0 :             if(IsExtfrc3DEmis) then
         565             :                 ! 3-D emissions are supported
         566           0 :                 HcoConfig%ModelSpc(N)%DimMax = 3
         567             :
         568           0 :                 exportDesc = "HEMCO 3-D Emissions Species " // trim(HcoConfig%ModelSpc(N)%SpcName)
         569             :                 call addfld(exportName, (/'lev'/), 'I', 'kg/m2/s',          &
         570             :                             trim(exportDesc),                               &
         571           0 :                             gridname='physgrid')
         572           0 :                 call HCO_Export_Pbuf_AddField(HcoConfig%ModelSpc(N)%SpcName, 3, hcoID=N)
         573             :             else
         574             :                 ! 2-D emissions only
         575           0 :                 HcoConfig%ModelSpc(N)%DimMax = 2
         576             :
         577           0 :                 exportDesc = "HEMCO 2-D Emissions Species " // trim(HcoConfig%ModelSpc(N)%SpcName)
         578             :                 call addfld(exportName, horiz_only, 'I', 'kg/m2/s',          &
         579             :                             trim(exportDesc),                               &
         580           0 :                             gridname='physgrid')
         581           0 :                 call HCO_Export_Pbuf_AddField(HcoConfig%ModelSpc(N)%SpcName, 2, hcoID=N)
         582             :             endif
         583             :         enddo
         584             :
         585             :         !-----------------------------------------------------------------------
         586             :         ! Read HEMCO configuration file from HcoConfigFile (location in CAM namelist)
         587             :         !-----------------------------------------------------------------------
         588             :         !if(masterproc) write(iulog,*) "> Reading HEMCO configuration file..."
         589             :
         590             :         ! FIXME: Not implementing "Dry-run" functionality in HEMCO_CESM. (hplin, 3/27/20)
         591             :         ! Phase: 0 = all, 1 = sett and switches only, 2 = fields only
         592           0 :         call Config_ReadFile(HcoConfig%amIRoot, HcoConfig, HcoConfigFile, 1, HMRC, IsDryRun=.false.)
         593           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
         594           0 :             write(iulog,*) "******************************************"
         595           0 :             write(iulog,*) "HEMCO_CESM: Config_ReadFile has failed (1)!    "
         596           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!       "
         597           0 :             write(iulog,*) "HEMCO configuration file could not be read."
         598           0 :             write(iulog,*) "This may be due to misconfiguration of the"
         599           0 :             write(iulog,*) "hemco_config_file namelist variable, or a"
         600           0 :             write(iulog,*) "misformatted HEMCO configuration file."
         601           0 :             write(iulog,*) "Please refer to the HEMCO.log log file in your"
         602           0 :             write(iulog,*) "case run directory or as configured in HEMCO_Config.rc"
         603           0 :             write(iulog,*) "for more information."
         604           0 :             write(iulog,*) "******************************************"
         605             :         endif
         606           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         607             :
         608             :         ! Open the log file
         609           0 :         if(masterproc) then
         610           0 :             call HCO_LOGFILE_OPEN(HcoConfig%Err, RC=HMRC)
         611           0 :             ASSERT_(HMRC==HCO_SUCCESS)
         612             :         endif
         613             :
         614           0 :         call Config_ReadFile(HcoConfig%amIRoot, HcoConfig, HcoConfigFile, 2, HMRC, IsDryRun=.false.)
         615           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
         616           0 :             write(iulog,*) "******************************************"
         617           0 :             write(iulog,*) "HEMCO_CESM: Config_ReadFile has failed (2)!    "
         618           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!       "
         619           0 :             write(iulog,*) "HEMCO configuration file could not be read."
         620           0 :             write(iulog,*) "This may be due to misconfiguration of the"
         621           0 :             write(iulog,*) "hemco_config_file namelist variable, or a"
         622           0 :             write(iulog,*) "misformatted HEMCO configuration file."
         623           0 :             write(iulog,*) "Please refer to the HEMCO.log log file in your"
         624           0 :             write(iulog,*) "case run directory or as configured in HEMCO_Config.rc"
         625           0 :             write(iulog,*) "for more information."
         626           0 :             write(iulog,*) "******************************************"
         627             :         endif
         628           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         629             :
         630             :         !if(masterproc) write(iulog,*) "> Read HEMCO configuration file OK!"
         631             :
         632             :         !-----------------------------------------------------------------------
         633             :         ! Initialize the HEMCO state object
         634             :         !-----------------------------------------------------------------------
         635           0 :         call HcoState_Init(HcoState, HcoConfig, nHcoSpc, HMRC)
         636           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         637             :
         638             :         !if(masterproc) write(iulog,*) "> Initialize HEMCO state obj OK!"
         639             :
         640             :         ! Emissions, chemistry and dynamics timestep [s]
         641             :         ! Assume 0.5h until given actual time in HCO_GC_Run!
         642             :
         643           0 :         stepsize_tmp = get_step_size()
         644           0 :         if(masterproc) write(iulog,*) "> HEMCO_CESM: Step size is ", stepsize_tmp
         645             :
         646           0 :         HcoState%TS_EMIS = stepsize_tmp * 1.0
         647           0 :         HcoState%TS_CHEM = stepsize_tmp * 1.0
         648           0 :         HcoState%TS_DYN  = stepsize_tmp * 1.0
         649             :
         650             :         ! Not a MAPL simulation. isESMF is deceiving.
         651           0 :         HcoState%Options%isESMF = .false.
         652             :
         653             :         ! Deposition length scale. Used for computing dry deposition frequencies
         654             :         ! over the entire PBL or the first model layer. Hardcoded for now,
         655             :         ! should load Input_Opt%PBL_DRYDEP from GEOS-Chem-CESM (hplin, 3/29/20)
         656             :         ! !FIXME
         657           0 :         HcoState%Options%PBL_DRYDEP = .false.
         658             :
         659             :         ! Don't support DryRun option (for now)
         660           0 :         HcoState%Options%IsDryRun = .false.
         661             :
         662             :         !if(masterproc) write(iulog,*) "> Set basic HEMCO state obj OK!"
         663             :
         664             :         !-----------------------------------------------------------------------
         665             :         ! Register HEMCO species information (HEMCO state object)
         666             :         !-----------------------------------------------------------------------
         667           0 :         do N = 1, nHcoSpc
         668           0 :             HcoState%Spc(N)%ModID         = N               ! model id
         669           0 :             HcoState%Spc(N)%SpcName       = trim(cnst_name(N)) ! species name
         670           0 :             HcoState%Spc(N)%MW_g          = cnst_mw(N)     ! mol. weight [g/mol]
         671             :
         672             :             ! !!! We don't set Henry's law coefficients in HEMCO_CESM !!!
         673             :             ! they are mostly used in HCOX_SeaFlux_Mod, but HCOX are unsupported (for now)
         674             :             ! (hplin, 3/29/20)
         675             :
         676             :             ! If is CESM-GC, then set Henry's law constants for SeaFlux
         677             :             ! KLUDGE by hplin: 1/3/21
         678             :             ! For defined species, hard code the Henry* values for now so we can work
         679             :             ! with SeaFlux. This fragmentation will cause issues down the road, FIXME
         680           0 :             if(HcoState%Spc(N)%SpcName .eq. "CH3I") then
         681             :                 ! 101.325_r8
         682           0 :                 HcoState%Spc(N)%HenryK0  = 0.20265_r8 ! [M/atm]
         683           0 :                 HcoState%Spc(N)%HenryCR  = 3.6e+3_r8 ! [K]
         684           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         685             :             endif
         686             :
         687           0 :             if(HcoState%Spc(N)%SpcName .eq. "DMS") then
         688             :                 ! 101.325_r8
         689           0 :                 HcoState%Spc(N)%HenryK0  = 4.80e-1_r8 ! [M/atm]
         690           0 :                 HcoState%Spc(N)%HenryCR  = 3100.0_r8 ! [K]
         691           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         692             :             endif
         693             :
         694           0 :             if(HcoState%Spc(N)%SpcName .eq. "ACET") then
         695             :                 ! 101.325_r8. using new henry constants
         696           0 :                 HcoState%Spc(N)%HenryK0  = 2.74e+1_r8 ! [M/atm]
         697           0 :                 HcoState%Spc(N)%HenryCR  = 5500.0_r8 ! [K]
         698           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         699             :             endif
         700             :
         701           0 :             if(HcoState%Spc(N)%SpcName .eq. "MOH") then
         702             :                 ! 101.325_r8
         703           0 :                 HcoState%Spc(N)%HenryK0  = 2.03e+2_r8 ! [M/atm]
         704           0 :                 HcoState%Spc(N)%HenryCR  = 5600.0_r8 ! [K]
         705           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         706             :             endif
         707             :
         708           0 :             if(HcoState%Spc(N)%SpcName .eq. "ALD2") then
         709             :                 ! 101.325_r8. using new henry constants
         710           0 :                 HcoState%Spc(N)%HenryK0  = 1.30e-01_r8 * 101.325_r8 ! [M/atm]
         711           0 :                 HcoState%Spc(N)%HenryCR  = 5900.0_r8 ! [K]
         712           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         713             :             endif
         714             :
         715           0 :             if(HcoState%Spc(N)%SpcName .eq. "MENO3") then
         716             :                 ! 101.325_r8
         717           0 :                 HcoState%Spc(N)%HenryK0  = 1.1e+1_r8 ! [M/atm]
         718           0 :                 HcoState%Spc(N)%HenryCR  = 4700.0_r8 ! [K]
         719           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         720             :             endif
         721             :
         722           0 :             if(HcoState%Spc(N)%SpcName .eq. "ETNO3") then
         723             :                 ! 101.325_r8
         724           0 :                 HcoState%Spc(N)%HenryK0  = 1.6_r8 ! [M/atm]
         725           0 :                 HcoState%Spc(N)%HenryCR  = 5400.0_r8 ! [K]
         726           0 :                 HcoState%Spc(N)%HenryPKA = -999e+0_r8 ! [1] (missing_r8 from species_mod)
         727             :             endif
         728             :
         729             :             ! HcoState%Spc(N)%HenryK0 ! [M/atm]
         730             :             ! HcoState%Spc(N)%HenryCR ! [K]
         731             :             ! HcoState%Spc(N)%HenryPKA ! [1]
         732             :
         733             :             ! Write to log too
         734           0 :             if(masterproc) then
         735             :                 !write(iulog,*) ">> Spc", N, " = ", cnst_name(N), "MW_g", cnst_mw(N)
         736           0 :                 call HCO_Spec2Log(HcoState, N)
         737             :             endif
         738             :         enddo
         739             :
         740             :         !if(masterproc) write(iulog,*) "> Set HEMCO species info OK!"
         741             :
         742             :         !-----------------------------------------------------------------------
         743             :         ! Register HEMCO Grid information
         744             :         !-----------------------------------------------------------------------
         745             :         ! Note that HEMCO running in the CAM environment is entirely MPI and
         746             :         ! we use the grid dimensions of the local PET. Thus, remember that all
         747             :         ! data and fields are sized my_* and NOT the global indices, although
         748             :         ! all PETs are aware. This is similar to ids, ide, jds, jde ... versus
         749             :         ! its, ite, jts, jte ... in WRF, but here we use my_IS, my_IE, my_JS...
         750             :         !
         751             :         ! The vertical dimension is not decomposed and follows the CAM vertical,
         752             :         ! whatever that is. This information is all abstracted and propagated within
         753             :         ! HCO_ESMF_Grid. (hplin, 3/29/20)
         754             :
         755           0 :         HcoState%NX = my_IM
         756           0 :         HcoState%NY = my_JM
         757           0 :         HcoState%NZ = LM
         758             :
         759             :         ! Pass Ap, Bp values, units [Pa], [unitless]
         760             :         ! later remove masterproc
         761             :         call HCO_VertGrid_Define(HcoState%Config,                &
         762             :                                  zGrid = HcoState%Grid%zGrid,    &
         763             :                                  nz    = HcoState%NZ,            &
         764             :                                  Ap    = Ap,                     &
         765             :                                  Bp    = Bp,                     &
         766           0 :                                  RC    = HMRC)
         767           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         768             :
         769             :         ! Point to grid variables
         770           0 :         HcoState%Grid%XMID%Val         => XMid   (my_IS:my_IE  , my_JS:my_JE  )
         771           0 :         HcoState%Grid%YMID%Val         => YMid   (my_IS:my_IE  , my_JS:my_JE  )
         772           0 :         HcoState%Grid%XEdge%Val        => XEdge  (my_IS:my_IE+1, my_JS:my_JE  )
         773           0 :         HcoState%Grid%YEdge%Val        => YEdge  (my_IS:my_IE  , my_JS:my_JE+1)
         774           0 :         HcoState%Grid%YSin%Val         => YSin   (my_IS:my_IE  , my_JS:my_JE+1)
         775           0 :         HcoState%Grid%AREA_M2%Val      => AREA_M2(my_IS:my_IE  , my_JS:my_JE  )
         776             :
         777             :         ! Debug
         778             :         ! write(6,*) "HCOI_Chunk_Init XMid, YMid(1,1)", HcoState%Grid%XMid%Val(1,1), &
         779             :         !                                               HcoState%Grid%YMid%Val(1,1), &
         780             :         !                                               HcoState%Grid%Area_m2%Val(1,1)
         781             :
         782             :         !if(masterproc) write(iulog,*) "> Set HEMCO PET-local grid info OK!"
         783             :
         784             :         !-----------------------------------------------------------------------
         785             :         ! Override HEMCO diagnostic file and root file paths in CESM environment
         786             :         ! This is so that the configuration file $ROOT and $DiagnFile do not
         787             :         ! have to contain hard-coded paths and can be distributed by cesmdata
         788             :         ! agnostically of the running environment. (hplin, 6/15/23)
         789             :         !-----------------------------------------------------------------------
         790             :         ! ROOT property. This is retrieved in several forms within the HEMCO code:
         791             :         !   hco_extlist_mod::HCO_ROOT(HcoConfig) --> HcoConfig%ROOT (populated by HCO_SetDefaultToken)
         792             :         !   hco_extlist_mod::HCO_GetOpt(ExtList, 'ROOT', -1) --> extension opt linked list
         793             :         ! looks like most of HEMCO convention will use HcoConfig%ROOT which is good.
         794             :         ! the $ROOT token replacement happens in hco_chartools_mod which uses HCO_ROOT().
         795             :         !
         796             :         ! the property has to be updated right after HCO_SetDefaultToken and values
         797             :         ! appropriately updated so that retrieval will use the overridden property.
         798             :         ! This means it has to go right after Config_ReadFile.
         799             :
         800             :         ! This might not be sufficient to update the configuration within the extlist -1.
         801           0 :         HcoConfig%ROOT = HcoRoot
         802             :
         803             :         ! DiagnFile property. This is part of the extension options and we replicate
         804             :         ! some of the functionality in order to override it here. Maybe this work could
         805             :         ! be done upstream.
         806           0 :         OptFound = .false.
         807           0 :         ThisOpt => NULL()
         808           0 :         ThisExt => NULL()
         809           0 :         ThisExt => HcoConfig%ExtList
         810           0 :         do while(associated(ThisExt))
         811           0 :             if(ThisExt%ExtNr /= CoreNr) then    ! Looking for the core extension.
         812           0 :                 ThisExt => ThisExt%NextExt
         813           0 :                 cycle
         814             :             endif
         815             :
         816           0 :             ThisOpt => ThisExt%Opts
         817           0 :             do while(associated(ThisOpt))
         818           0 :                 if(trim(ThisOpt%OptName) == "DiagnFile") then
         819           0 :                     ThisOpt%OptValue = HcoDiagnFile
         820           0 :                     OptFound = .true.
         821           0 :                     exit
         822             :                 endif
         823             :
         824           0 :                 ThisOpt => ThisOpt%NextOpt
         825             :             enddo
         826             :
         827           0 :             if(OptFound) then
         828             :                 ThisExt => NULL()
         829             :             else
         830           0 :                 ThisExt => ThisExt%NextExt
         831             :             endif
         832             :         enddo
         833             :
         834           0 :         ThisOpt => NULL()
         835           0 :         ThisExt => NULL()
         836             :
         837             :         !-----------------------------------------------------------------------
         838             :         ! Initialize HEMCO!
         839             :         ! The following actions happen during initialization:
         840             :         ! 1) time slice pointers (tIDx_Init)
         841             :         ! 2) clock initialization (HcoClock_Init populates HcoState%Clock)
         842             :         ! 3) HEMCO diagnostic containers are initialized (HcoDiagn_Init)
         843             :         ! 4) configuration file initializes ReadList
         844             :         ! 5) universal scale factor for each HEMCO species (Hco_ScaleInit)
         845             :         !-----------------------------------------------------------------------
         846           0 :         call t_startf('HCO_HCOX_Init')
         847           0 :         call HCO_Init(HcoState, HMRC)
         848           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
         849           0 :             write(iulog,*) "******************************************"
         850           0 :             write(iulog,*) "HEMCO_CESM: HCO_Init has failed!"
         851           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!"
         852           0 :             write(iulog,*) "HEMCO could not be initialized."
         853           0 :             write(iulog,*) "This may be due to misconfiguration of the"
         854           0 :             write(iulog,*) "HEMCO configuration file."
         855           0 :             write(iulog,*) "Please refer to the HEMCO.log log file and"
         856           0 :             write(iulog,*) "the cesm.log. log files in your case run directory"
         857           0 :             write(iulog,*) "for more information."
         858           0 :             write(iulog,*) "******************************************"
         859             :         endif
         860           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         861             :
         862           0 :         if(masterproc) write(iulog,*) "> HEMCO initialized successfully!"
         863             :
         864             :         !-----------------------------------------------------------------------
         865             :         ! Initialize HEMCO Extensions!
         866             :         !-----------------------------------------------------------------------
         867           0 :         call HCOX_Init(HcoState, ExtState, HMRC)
         868           0 :         ASSERT_(HMRC==HCO_SUCCESS)
         869             :
         870           0 :         if(masterproc) write(iulog,*) "> HEMCO extensions initialized successfully!"
         871           0 :         call t_stopf('HCO_HCOX_Init')
         872             :
         873             :         !-----------------------------------------------------------------------
         874             :         ! Additional exports: Verify if additional diagnostic quantities
         875             :         ! for HEMCO extensions need to be provisioned.
         876             :         ! (hplin, 3/21/21)
         877             :         !-----------------------------------------------------------------------
         878             :         ! ParaNOx: Ship NO emissions
         879             :         ! Due to the length limit this is a non-standard name, the HEMCO names are
         880             :         ! PARANOX_O3_DEPOSITION_FLUX and PARANOX_HNO3_DEPOSITION_FLUX
         881           0 :         if(ExtState%ParaNOx > 0) then
         882           0 :             write(exportnameTmp, '(a)') 'PAR_O3_DEP'
         883           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         884           0 :             exportDesc = "HEMCO Deposition Flux Name " // trim(exportNameTmp)
         885             :
         886             :             call addfld(exportName, horiz_only, 'I', '1',                &
         887             :                         trim(exportDesc),                                &
         888           0 :                         gridname='physgrid')
         889           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         890             :
         891           0 :             write(exportnameTmp, '(a)') 'PAR_HNO3_DEP'
         892           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         893           0 :             exportDesc = "HEMCO Deposition Flux Name " // trim(exportNameTmp)
         894             :
         895             :             call addfld(exportName, horiz_only, 'I', '1',                &
         896             :                         trim(exportDesc),                                &
         897           0 :                         gridname='physgrid')
         898           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         899             :
         900           0 :             if(masterproc) write(iulog,*) "> HEMCO ParaNOx extension exports (PAR_O3_DEP, PAR_HNO3_DEP) initialized successfully"
         901             :         endif
         902             :
         903             :         !-----------------------------------------------------------------------
         904             :         ! Additional exports: Verify if we need to add additional exports
         905             :         ! for integration with CESM-GC. (hplin, 4/15/20)
         906             :         !-----------------------------------------------------------------------
         907             :
         908             :         ! Do additional exports!
         909             :         ! Removed debug into history output because it does not seem necessary (hplin, 9/23/22)
         910           0 :         if(chem_is('GEOS-Chem')) then
         911           0 :             do N = 0, 72
         912             :                ! LANDTYPExx
         913           0 :                write(exportNameTmp, '(a,i2.2)') 'LANDTYPE', N
         914           0 :                exportName = 'HCO_' // trim(exportNameTmp)
         915           0 :                call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         916             :
         917             :                ! XLAIxx
         918           0 :                write(exportNameTmp, '(a,i2.2)') 'XLAI', N
         919           0 :                exportName = 'HCO_' // trim(exportNameTmp)
         920           0 :                call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         921             :             enddo
         922             :
         923             :             ! VMR_CH3CL
         924           0 :             write(exportnameTmp, '(a)') 'VMR_CH3CL'
         925           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         926           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         927             :
         928             :             ! VMR_CH2CL2
         929           0 :             write(exportnameTmp, '(a)') 'VMR_CH2CL2'
         930           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         931           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         932             :
         933             :             ! VMR_CHCL3
         934           0 :             write(exportnameTmp, '(a)') 'VMR_CHCL3'
         935           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         936           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         937             :
         938             :             ! VMR_CH3BR
         939           0 :             write(exportnameTmp, '(a)') 'VMR_CH3BR'
         940           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         941           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         942             :
         943             :             ! VMR_CCL4
         944           0 :             write(exportnameTmp, '(a)') 'VMR_CCL4'
         945           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         946           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         947             :
         948             :             ! VMR_CFC113
         949           0 :             write(exportnameTmp, '(a)') 'VMR_CFC113'
         950           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         951           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         952             :
         953             :             ! VMR_CFC114
         954           0 :             write(exportnameTmp, '(a)') 'VMR_CFC114'
         955           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         956           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         957             :
         958             :             ! VMR_CFC115
         959           0 :             write(exportnameTmp, '(a)') 'VMR_CFC115'
         960           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         961           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         962             :
         963             :             ! VMR_CFC11
         964           0 :             write(exportnameTmp, '(a)') 'VMR_CFC11'
         965           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         966           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         967             :
         968             :             ! VMR_CFC12
         969           0 :             write(exportnameTmp, '(a)') 'VMR_CFC12'
         970           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         971           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         972             :
         973             :             ! VMR_CH3CCL3
         974           0 :             write(exportnameTmp, '(a)') 'VMR_CH3CCL3'
         975           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         976           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         977             :
         978             :             ! VMR_H1211
         979           0 :             write(exportnameTmp, '(a)') 'VMR_H1211'
         980           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         981           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         982             :
         983             :             ! VMR_H1301
         984           0 :             write(exportnameTmp, '(a)') 'VMR_H1301'
         985           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         986           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         987             :
         988             :             ! VMR_H2402
         989           0 :             write(exportnameTmp, '(a)') 'VMR_H2402'
         990           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         991           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         992             :
         993             :             ! VMR_HCFC141b
         994           0 :             write(exportnameTmp, '(a)') 'VMR_HCFC141B'
         995           0 :             exportName = 'HCO_' // trim(exportNameTmp)
         996           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
         997             :
         998             :             ! VMR_HCFC142B
         999           0 :             write(exportnameTmp, '(a)') 'VMR_HCFC142B'
        1000           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1001           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1002             :
        1003             :             ! VMR_HCFC22
        1004           0 :             write(exportnameTmp, '(a)') 'VMR_HCFC22'
        1005           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1006           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1007             :
        1008             :             ! VMR_N2O
        1009           0 :             write(exportnameTmp, '(a)') 'VMR_N2O'
        1010           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1011           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1012             :
        1013             :             ! VMR_OCS
        1014           0 :             write(exportnameTmp, '(a)') 'VMR_OCS'
        1015           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1016           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1017             :
        1018             :             ! VMR_H2
        1019           0 :             write(exportnameTmp, '(a)') 'VMR_H2'
        1020           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1021           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1022             :
        1023             :             ! UVALBEDO
        1024           0 :             write(exportnameTmp, '(a)') 'UV_ALBEDO'
        1025           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1026           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1027             :
        1028             :             ! SURF_IODIDE
        1029           0 :             write(exportnameTmp, '(a)') 'iodide'
        1030           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1031           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1032             :
        1033             :             ! SURF_SALINITY
        1034           0 :             write(exportnameTmp, '(a)') 'salinity'
        1035           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1036           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1037             :
        1038             :             ! OMOC_DJF
        1039           0 :             write(exportnameTmp, '(a)') 'OMOC_DJF'
        1040           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1041           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1042             :
        1043             :             ! OMOC_MAM
        1044           0 :             write(exportnameTmp, '(a)') 'OMOC_MAM'
        1045           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1046           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1047             :
        1048             :             ! OMOC_JJA
        1049           0 :             write(exportnameTmp, '(a)') 'OMOC_JJA'
        1050           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1051           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1052             :
        1053             :             ! OMOC_SON
        1054           0 :             write(exportnameTmp, '(a)') 'OMOC_SON'
        1055           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1056           0 :             call HCO_Export_Pbuf_AddField(exportNameTmp, 2)
        1057             :
        1058           0 :             if ( masterproc ) then
        1059           0 :                 write(iulog,*) "> HEMCO additional exports for CESM2-GC initialized!"
        1060             :             endif
        1061             :         endif
        1062             :
        1063           0 :         call t_stopf('HCOI_Chunk_Init')
        1064           0 :     end subroutine HCOI_Chunk_Init
        1065             : !EOC
        1066             : !------------------------------------------------------------------------------
        1067             : !                    Harmonized Emissions Component (HEMCO)                   !
        1068             : !------------------------------------------------------------------------------
        1069             : !BOP
        1070             : !
        1071             : ! !IROUTINE: HCOI_Initialize_Pbuf
        1072             : !
        1073             : ! !DESCRIPTION: HCOI\_Initialize\_Pbuf resets the physics buffer.
        1074             : !\\
        1075             : !\\
        1076             : ! !INTERFACE:
        1077             : !
        1078           0 :     subroutine HCOI_Initialize_Pbuf()
        1079             : !
        1080             : ! !USES:
        1081             : !
        1082           0 :         use cam_logfile,      only: iulog
        1083             :         use spmd_utils,       only: masterproc
        1084             : !
        1085             : ! !REVISION HISTORY:
        1086             : !  14 Dec 2020 - H.P. Lin    - Initial version
        1087             : !  16 Jan 2023 - H.P. Lin    - Need to reset this after pbuf fields are now 3-D or 2-D.
        1088             : !                              Approximately 16 hours of debugging stack corruptions
        1089             : !                              were needed to realize I wrote this routine.
        1090             : !EOP
        1091             : !------------------------------------------------------------------------------
        1092             : !BOC
        1093             : !
        1094             : ! !LOCAL VARIABLES:
        1095             : !
        1096             :         character(len=*), parameter  :: subname = 'HCOI_Initialize_Pbuf'
        1097             :         integer                      :: RC                   ! ESMF return code
        1098             :
        1099             :         integer                      :: spcID
        1100           0 :         real(ESMF_KIND_R8)           :: zeroFldCAM_3D(1:LM, 1:my_CE)
        1101           0 :         real(ESMF_KIND_R8)           :: zeroFldCAM_2D(1:my_CE)
        1102             :
        1103             :         ! Zero out quantities first
        1104           0 :         zeroFldCAM_3D(:,:)   = 0.0_r8
        1105           0 :         zeroFldCAM_2D(:  )   = 0.0_r8
        1106             :
        1107             :         ! Reset for each species
        1108           0 :         do spcID = 1, HcoConfig%nModelSpc
        1109             :             ! Write to physics buffer (pass model name)
        1110           0 :             if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1111             :                 call HCO_Export_Pbuf_CAM3D(HcoConfig%ModelSpc(spcID)%SpcName, spcID, zeroFldCAM_3D)
        1112           0 :             elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1113             :                 call HCO_Export_Pbuf_CAM2D(HcoConfig%ModelSpc(spcID)%SpcName, spcID, zeroFldCAM_2D)
        1114             :             else
        1115           0 :                 ASSERT_(.false.)
        1116             :             endif
        1117             :         enddo
        1118             :
        1119           0 :     end subroutine HCOI_Initialize_Pbuf
        1120             : !EOC
        1121             : !------------------------------------------------------------------------------
        1122             : !                    Harmonized Emissions Component (HEMCO)                   !
        1123             : !------------------------------------------------------------------------------
        1124             : !BOP
        1125             : !
        1126             : ! !IROUTINE: HCOI_Chunk_Run
        1127             : !
        1128             : ! !DESCRIPTION: HCOI\_Chunk\_Run is the run method for the CAM interface to HEMCO.
        1129             : !\\
        1130             : !\\
        1131             : ! !INTERFACE:
        1132             : !
        1133           0 :     subroutine HCOI_Chunk_Run(cam_in, phys_state, pbuf2d, phase)
        1134             : !
        1135             : ! !USES:
        1136             : !
        1137             :         ! Type descriptors
        1138             :         use camsrfexch,     only: cam_in_t
        1139             :         use physics_types,  only: physics_state
        1140             :         use physics_buffer, only: physics_buffer_desc
        1141             :
        1142             :         ! Physics grid
        1143             :         use phys_grid,      only: get_ncols_p
        1144             :
        1145             :         ! CAM physics buffer (some fields are here and some are in phys state)
        1146             :         use physics_buffer, only: pbuf_get_chunk, pbuf_get_field
        1147             :         use physics_buffer, only: pbuf_get_index
        1148             :
        1149             :         ! Output and mpi
        1150             :         use cam_logfile,    only: iulog
        1151             :         use spmd_utils,     only: masterproc, mpicom, masterprocid, iam
        1152             :
        1153             :         ! Performance timers
        1154             :         use perf_mod,       only: t_startf, t_stopf
        1155             :
        1156             :         ! ESMF
        1157             :         use ESMF,           only: ESMF_GridCompRun
        1158             :
        1159             : !
        1160             : ! !INPUT PARAMETERS:
        1161             : !
        1162             :         type(cam_in_t),      intent(inout) :: cam_in(begchunk:endchunk)
        1163             :         type(physics_state), intent(inout) :: phys_state(begchunk:endchunk)
        1164             :         type(physics_buffer_desc), pointer :: pbuf2d(:,:)
        1165             :         integer, intent(in)                :: phase               ! 1, 2
        1166             : !
        1167             : ! !REVISION HISTORY:
        1168             : !  06 Feb 2020 - H.P. Lin    - Initial version
        1169             : !EOP
        1170             : !------------------------------------------------------------------------------
        1171             : !BOC
        1172             : !
        1173             : ! !LOCAL VARIABLES:
        1174             : !
        1175             :         character(len=*), parameter  :: subname = 'HCOI_Chunk_Run'
        1176             :         integer                      :: RC                        ! Return code
        1177             :
        1178             :         logical, save                :: FIRST = .true.
        1179             :
        1180           0 :         call t_startf('HCOI_Chunk_Run')
        1181             :
        1182           0 :         if(masterproc) then
        1183           0 :             write(iulog,*) "HEMCO_CESM: Running HCOI_Chunk_Run phase", phase
        1184             :         endif
        1185             :
        1186             :         ! We only run the gridded components on Phase 2 per recommendations
        1187             :         ! from Steve, but this can be easily extended.
        1188             :         !
        1189             :         ! In edyn_grid_comp, the ionosphere interface runs on run1 and run2
        1190             :         ! and uses a global variable to control the gridded component's
        1191             :         ! run stage. This is not needed for HEMCO right now but we can always
        1192             :         ! implement this in the future.
        1193             :         !
        1194             :         ! HEMCO also has two stages, but the distinction is not necessary
        1195             :         ! in the CAM interface. For more information, look at the actual
        1196             :         ! run routine in the gridded component HCO_GC_Run.
        1197             :         ! (hplin, 2/6/20)
        1198           0 :         if(phase == 2) then
        1199             :             ! Only need to do this once to save time.
        1200             :             ! reset all the physics buffer contents
        1201             :             ! to prevent trash data being read by other components.
        1202             :             ! (hplin, 12/15/20)
        1203           0 :             if(FIRST) then
        1204             :
        1205             :                 ! Pass the pbuf to the hco_cam_exports component so she has it...
        1206           0 :                 hco_pbuf2d => pbuf2d
        1207             :
        1208           0 :                 call HCOI_Initialize_Pbuf()
        1209             :
        1210             :                 ! No longer first call
        1211           0 :                 FIRST = .false.
        1212             :
        1213             :             endif
        1214             :
        1215             :             ! Pass the pbuf to the hco_cam_exports component so she has it...
        1216             :             ! hco_pbuf2d => pbuf2d
        1217             :
        1218             :             ! Set fields from CAM state before run
        1219           0 :             call t_startf('HCO_CAM_GetBefore_HCOI')
        1220             :             call CAM_GetBefore_HCOI(cam_in, phys_state, pbuf2d, phase, &
        1221           0 :                                     HcoState, ExtState)
        1222           0 :             call t_stopf('HCO_CAM_GetBefore_HCOI')
        1223             :
        1224             :             ! Run the gridded component.
        1225           0 :             call t_startf('HCO_GridCompRun')
        1226           0 :             call ESMF_GridCompRun(HCO_GridComp, rc=RC)!importState=HCO_GridCompState, &
        1227             :                                                 !exportState=HCO_GridCompState, &
        1228             :                                                 !rc=RC)
        1229           0 :             call t_stopf('HCO_GridCompRun')
        1230             :
        1231           0 :             ASSERT_(RC==ESMF_SUCCESS)
        1232             :         endif
        1233             :
        1234           0 :         if(masterproc) then
        1235           0 :             write(iulog,*) "HEMCO_CESM: Leaving HCOI_Chunk_Run"
        1236             :         endif
        1237             :
        1238           0 :         call t_stopf('HCOI_Chunk_Run')
        1239           0 :     end subroutine HCOI_Chunk_Run
        1240             : !EOC
        1241             : !------------------------------------------------------------------------------
        1242             : !                    Harmonized Emissions Component (HEMCO)                   !
        1243             : !------------------------------------------------------------------------------
        1244             : !BOP
        1245             : !
        1246             : ! !IROUTINE: HCOI_Chunk_Final
        1247             : !
        1248             : ! !DESCRIPTION: HCOI\_Chunk\_Final cleans up the CAM interface to HEMCO.
        1249             : !\\
        1250             : !\\
        1251             : ! !INTERFACE:
        1252             : !
        1253           0 :     subroutine HCOI_Chunk_Final()
        1254             :         ! Stub...
        1255           0 :     end subroutine HCOI_Chunk_Final
        1256             :     !-----------------------------------------------------------------------
        1257             :     !              H E M C O   W R A P P E R   G R I D C O M P             !
        1258             :     !-----------------------------------------------------------------------
        1259             :     !  Below code includes internal routines used to wrap a ESMF gridded   !
        1260             :     !  component around the HEMCO interface, so ESMF can handle all the    !
        1261             :     !  interaction with the physics mesh.                                  !
        1262             :     !                                                                      !
        1263             :     !  This is largely based on edyn_grid_comp.F90 from ionosphere/waccmx  !
        1264             :     !  Thanks to Steve Goldhaber for the example                           !
        1265             :     !                                                                      !
        1266             :     !  (hplin, 1/31/20)                                                    !
        1267             :     !-----------------------------------------------------------------------
        1268             : !EOC
        1269             : !------------------------------------------------------------------------------
        1270             : !                    Harmonized Emissions Component (HEMCO)                   !
        1271             : !------------------------------------------------------------------------------
        1272             : !BOP
        1273             : !
        1274             : ! !IROUTINE: HCO_GC_Run
        1275             : !
        1276             : ! !DESCRIPTION: HCO\_GC\_Run is an internal method in the HEMCO gridded component
        1277             : !  in CAM. It runs the main routines of HEMCO and is called by ESMF.
        1278             : !  The routines inside the GridComp operate on the HEMCO grid and are responsible
        1279             : !  to run regridding routines to return data into the physics mesh.
        1280             : !  In short, code goes here.
        1281             : !\\
        1282             : !\\
        1283             : ! !INTERFACE:
        1284             : !
        1285           0 :     subroutine HCO_GC_Run(GC, IMPORT, EXPORT, Clock, RC)
        1286             : !
        1287             : ! !USES:
        1288             : !
        1289             :         use cam_logfile,               only: iulog
        1290             :         use spmd_utils,                only: masterproc, iam
        1291             :
        1292             :         ! Performance timers
        1293             :         use perf_mod,                  only: t_startf, t_stopf
        1294             :
        1295             :         ! HEMCO
        1296             :         use HCO_Interface_Common,      only: GetHcoVal, GetHcoDiagn
        1297             :         use HCO_Clock_Mod,             only: HcoClock_Set, HcoClock_Get
        1298             :         use HCO_Clock_Mod,             only: HcoClock_EmissionsDone
        1299             :         use HCO_Diagn_Mod,             only: HcoDiagn_AutoUpdate
        1300             :         use HCO_Driver_Mod,            only: HCO_Run
        1301             :         use HCO_EmisList_Mod,          only: Hco_GetPtr
        1302             :         use HCO_Calc_Mod,              only: Hco_EvalFld
        1303             :         use HCO_FluxArr_Mod,           only: HCO_FluxArrReset
        1304             :         use HCO_GeoTools_Mod,          only: HCO_CalcVertGrid, HCO_SetPBLm
        1305             :
        1306             :         use HCO_State_Mod,             only: HCO_GetHcoId
        1307             :
        1308             :         ! HEMCO Extensions
        1309             :         use HCOX_Driver_Mod,           only: HCOX_Run
        1310             :
        1311             :         ! Physical constants
        1312             :         use physconst,                 only: mwdry
        1313             :
        1314             :         ! Necessary imported properties for physics calculations
        1315             :         use hco_cam_convert_state_mod, only: State_HCO_PSFC, State_HCO_TK, State_HCO_PBLH, State_CAM_chmDMS
        1316             :         use hco_cam_convert_state_mod, only: State_CAM_chmACET, State_CAM_chmALD2, State_CAM_chmMOH, State_CAM_chmMENO3, State_CAM_DELP_DRYs, State_CAM_chmETNO3
        1317             :
        1318             : !
        1319             : ! !INPUT/OUTPUT PARAMETERS:
        1320             : !
        1321             :         type(ESMF_GridComp)                   :: GC
        1322             :         type(ESMF_State)                      :: IMPORT
        1323             :         type(ESMF_State)                      :: EXPORT
        1324             :         type(ESMF_Clock)                      :: Clock
        1325             :         integer, intent(out)                  :: RC
        1326             : !
        1327             : ! !REMARKS:
        1328             : !  All the input/output parameters here are dummies.
        1329             : !
        1330             : ! !REVISION HISTORY:
        1331             : !  06 Feb 2020 - H.P. Lin    - Initial version
        1332             : !  09 Mar 2023 - H.P. Lin    - Allow for FixYY in HEMCO clock for climo runs
        1333             : !EOP
        1334             : !------------------------------------------------------------------------------
        1335             : !BOC
        1336             : !
        1337             : ! !LOCAL VARIABLES:
        1338             : !
        1339             :         character(len=*),       parameter     :: subname = 'HCO_GC_Run'
        1340             :
        1341             :         ! Parameters
        1342             :         real(r8), parameter                   :: G0_100 = 100.e+0_r8 / 9.80665e+0_r8
        1343             :
        1344             :         integer                               :: I, J, K
        1345             :         integer                               :: HI, HJ, HL
        1346             :
        1347             :         ! Temporaries for exports
        1348             :         real(ESMF_KIND_R8)                    :: TMP
        1349             :         logical                               :: FND
        1350             :         character(len=128)                    :: exportName, exportNameTmp
        1351             :         integer                               :: spcID, N
        1352             :
        1353             :         ! For grabbing data from HEMCO Ptrs (uses HEMCO single-precision)
        1354           0 :         real(sp), pointer                     :: Ptr2D(:,:)
        1355             :         real(sp), pointer                     :: Ptr3D(:,:,:)
        1356             :
        1357             :         ! Temporaries used for export
        1358           0 :         real(ESMF_KIND_R8)                    :: exportFldHco(my_IS:my_IE, my_JS:my_JE, 1:LM)
        1359           0 :         real(ESMF_KIND_R8)                    :: exportFldCAM(1:LM, 1:my_CE)
        1360             :         real(ESMF_KIND_R8)                    :: scratchFldCAM(1:LM, 1:my_CE)
        1361             :         real(ESMF_KIND_R8)                    :: scratchFldCAM2(1:my_CE)
        1362             :
        1363             :         ! Temporaries used for export (2-D data)
        1364           0 :         real(ESMF_KIND_R8)                    :: exportFldHco2(my_IS:my_IE, my_JS:my_JE)
        1365           0 :         real(ESMF_KIND_R8)                    :: exportFldCAM2(1:my_CE)
        1366           0 :         real(ESMF_KIND_R8)                    :: exportFldHcoDep(my_IS:my_IE, my_JS:my_JE)
        1367           0 :         real(ESMF_KIND_R8)                    :: exportFldCAMDep(1:my_CE)
        1368             :
        1369             :         ! For debug dummies
        1370           0 :         real(ESMF_KIND_R8)                    :: dummy_0_CAM(1:LM, 1:my_CE)
        1371             :         real(ESMF_KIND_R8)                    :: dummy_1(my_IS:my_IE, my_JS:my_JE, 1:LM)
        1372           0 :         real(ESMF_KIND_R8)                    :: dummy_1_CAM(1:LM, 1:my_CE)
        1373             :         real(ESMF_KIND_R8)                    :: dummy_2(my_IS:my_IE, my_JS:my_JE)
        1374             :
        1375             :         ! Timing properties
        1376             :         integer                               :: year, month, day, tod
        1377             :         integer                               :: hour, minute, second
        1378             :         integer                               :: prev_day, prev_s, now_day, now_s
        1379             :         integer                               :: tmp_currTOD
        1380             :
        1381             :         ! HEMCO vertical grid property pointers
        1382             :         ! NOTE: Hco_CalcVertGrid expects pointer-based arguments, so we must
        1383             :         ! make PEDGE be a pointer and allocate/deallocate it on each call.
        1384           0 :         real(hp), pointer            :: BXHEIGHT(:,:,:)    ! Grid box height      [m ]
        1385           0 :         real(hp), pointer            :: PEDGE   (:,:,:)    ! Pressure @ lvl edges [Pa]
        1386           0 :         real(hp), pointer            :: ZSFC    (:,:  )    ! Surface geopotential [m ]
        1387             :
        1388             :
        1389             :         real(hp), pointer            :: PBLM    (:,:  )    ! PBL height           [m ]
        1390           0 :         real(hp), pointer            :: PSFC    (:,:  )    ! Surface pressure     [Pa]
        1391           0 :         real(hp), pointer            :: TK      (:,:,:)    ! Temperature          [K ]
        1392             :
        1393             :         ! HEMCO return code
        1394             :         integer                      :: HMRC
        1395             :
        1396             :         logical, save                :: FIRST = .True.
        1397             :         logical                      :: doExport = .False.
        1398             :         integer, save                :: nCalls = 0
        1399             :
        1400             :         ! Assume success
        1401           0 :         RC = ESMF_SUCCESS
        1402           0 :         HMRC = HCO_SUCCESS
        1403             :
        1404           0 :         nCalls = nCalls + 1
        1405             :
        1406             :         !-----------------------------------------------------------------------
        1407             :         ! Update regridding file handles as necessary
        1408             :         !-----------------------------------------------------------------------
        1409           0 :         call HCO_Grid_UpdateRegrid(RC=RC)
        1410           0 :         ASSERT_(RC==ESMF_SUCCESS)
        1411             :
        1412             :         !if(masterproc) then
        1413             :         !    write(iulog,*) "HEMCO_CESM: Reload (if necessary) of HEMCO Regrid descriptors"
        1414             :         !endif
        1415             :
        1416             :         !-----------------------------------------------------------------------
        1417             :         ! Allow for year forcing in climatological runs. (hplin, 3/9/23)
        1418             :         ! This is set if HcoFixYY is set in this module and is > 0
        1419             :         !
        1420             :         ! This is set in the run routine because HEMCO clock is initialized at
        1421             :         ! HCO_INIT -> HcoClock_Init, so it was not available until very late in
        1422             :         ! the Init phase. But maybe it could be moved up as well.
        1423             :         !-----------------------------------------------------------------------
        1424           0 :         if(HcoFixYY .gt. 0) then
        1425             :             ! Override the HEMCO clock FixYY property
        1426           0 :             HcoState%Clock%FixYY = HcoFixYY
        1427             :         endif
        1428             :
        1429             :         !-----------------------------------------------------------------------
        1430             :         ! Get time properties
        1431             :         !-----------------------------------------------------------------------
        1432           0 :         call get_prev_time(prev_day, prev_s)
        1433           0 :         call get_curr_time(now_day, now_s)
        1434           0 :         call get_curr_date(year, month, day, tod)
        1435             :
        1436             :         !if(masterproc) then
        1437             :         !    write(iulog,*) "hco year,month,day,tod", year, month, day, tod
        1438             :         !    write(iulog,*) "hco prev_day, prev_s", prev_day, prev_s
        1439             :         !    write(iulog,*) "hco now_day, now_s", now_day, now_s
        1440             :         !endif
        1441             :         ! 2005 1 1 1800 | 0 0 | 0 1800
        1442             :         ! 2005 1 1 3600 | 0 1800 | 0 3600
        1443             :         ! 2005 1 1 5400 | 0 3600 | 0 5400
        1444             :         ! ...
        1445             :
        1446             :         ! Check if we have run HEMCO for this time step already. If yes can exit
        1447           0 :         if(last_HCO_day * 86400.0 + last_HCO_second .ge. now_day * 86400.0 + now_s) then
        1448             :             ! The first timestep should not be skipped. A fix is made during initialization (hplin, 6/11/24)
        1449           0 :             if(masterproc) then
        1450           0 :                 write(iulog,*) "HEMCO_CESM: HEMCO already ran for this time, check timestep mgr (now day, s; last day, s)", now_day, now_s, last_HCO_day, last_HCO_second
        1451             :             endif
        1452             :
        1453             :             return
        1454             :         endif
        1455             :
        1456             :         ! Timestep no longer needs to be updated by diff calculation because it can be
        1457             :         ! reliably retrieved from time_manager stepsize. (hplin, 6/11/24)
        1458             :
        1459             :         ! Compute hour, minute, second (borrowed from tfritz)
        1460           0 :         tmp_currTOD = tod
        1461           0 :         hour = 0
        1462           0 :         minute = 0
        1463           0 :         do while(tmp_currTOD >= 3600)
        1464           0 :             tmp_currTOD = tmp_currTOD - 3600
        1465           0 :             hour = hour + 1
        1466             :         enddo
        1467             :
        1468           0 :         do while(tmp_currTOD >= 60)
        1469           0 :             tmp_currTOD = tmp_currTOD - 60
        1470           0 :             minute = minute + 1
        1471             :         enddo
        1472           0 :         second = tmp_currTOD
        1473             :
        1474             :         ! Update HEMCO clock
        1475             :         ! using HcoClock_Set and not common SetHcoTime because we don't have DOY
        1476             :         ! and we want HEMCO to do the math for us. oh well
        1477           0 :         if(masterproc) then
        1478           0 :             write(iulog,'(A,I4,A,I2.2,A,I2.2,A,I4.4)') "HEMCO_CESM: Internally HEMCO was at (Sim H:M:S:nStep) ", HcoState%Clock%SimHour, ":", HcoState%Clock%SimMin, ":", HcoState%Clock%SimSec, " x", HcoState%Clock%nSteps
        1479           0 :             write(iulog,'(A,I4,A,I2.2,A,I2.2,A,I2.2,A,I2.2,A,I2.2)') "HEMCO_CESM: Updating HEMCO clock to set (Y-M-D H:I:S) ", year, "-", month, "-", day, " ", hour, ":", minute, ":", second
        1480             :         endif
        1481             :
        1482             :         call HCOClock_Set(HcoState, year, month, day,  &
        1483           0 :                           hour, minute, second, IsEmisTime=.true., RC=HMRC)
        1484           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1485             :
        1486             :         !-----------------------------------------------------------------------
        1487             :         ! Continue setting up HEMCO
        1488             :         !-----------------------------------------------------------------------
        1489             :
        1490             :         ! Reset all emission and deposition values.
        1491           0 :         call HCO_FluxArrReset(HcoState, HMRC)
        1492           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1493             :
        1494             :         !-----------------------------------------------------------------------
        1495             :         ! Regrid necessary meteorological quantities (Phase 1)
        1496             :         ! Computes the absolute minimum (PSFC and TK) necessary for HEMCO
        1497             :         ! to define its grid.
        1498             :         !-----------------------------------------------------------------------
        1499           0 :         call CAM_RegridSet_HCOI(HcoState, ExtState, Phase=1)
        1500             :
        1501           0 :         if(masterproc .and. nCalls < 10) then
        1502           0 :             write(iulog,*) "HEMCO_CESM: Finished regridding CAM met fields to HEMCO (1)"
        1503             :         endif
        1504             :
        1505             :         !-----------------------------------------------------------------------
        1506             :         ! Get grid properties
        1507             :         !-----------------------------------------------------------------------
        1508             :         ! Calculate HEMCO vertical grid properties, e.g. PEDGE,
        1509             :         ! then PHIS, BXHEIGHT, T, ..., from GridEdge_Set
        1510             :         !
        1511             :         ! The below conversions mostly borrowed from tfritz's CESM2-GC.
        1512             :         ! HEMCO CalcVertGrid can approximate all quantities. We provide them with
        1513             :         ! PSFC (surface pressure), TK (temperature)
        1514             :         ! in the form of allocated pointers. The rest can be inferred from Ap, Bp
        1515           0 :         PSFC => State_HCO_PSFC
        1516           0 :         TK   => State_HCO_TK
        1517             :
        1518           0 :         call HCO_CalcVertGrid(HcoState, PSFC, ZSFC, TK, BXHEIGHT, PEDGE, HMRC)
        1519           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1520             :
        1521             :         ! Pass boundary layer height to HEMCO (PBLm = PBL mixing height) [m]
        1522             :         call HCO_SetPBLm(HcoState, PBLM=State_HCO_PBLH, &
        1523             :                          DefVal=1000.0_hp, & ! default value
        1524           0 :                          RC=HMRC)
        1525           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1526             :
        1527             :         !-----------------------------------------------------------------------
        1528             :         ! Regrid necessary meteorological quantities (Phase 2)
        1529             :         ! Has to be below grid properties because vertical grid needs to be defined
        1530             :         ! for quantities to be computed!
        1531             :         !-----------------------------------------------------------------------
        1532           0 :         call CAM_RegridSet_HCOI(HcoState, ExtState, Phase=2)
        1533             :
        1534           0 :         if(masterproc .and. nCalls < 10) then
        1535           0 :             write(iulog,*) "HEMCO_CESM: Finished regridding CAM met fields to HEMCO (2)"
        1536             :
        1537             :             ! As a test... maybe we also need to flip in the vertical
        1538             :             ! write(iulog,*) State_HCO_TK(1,1,:)
        1539             :             ! write(iulog,*) "PSFC(1:2,:)"
        1540             :             ! write(iulog,*) State_HCO_PSFC(1:2,:)
        1541             :
        1542             :             !write(iulog,*) "cam state%ps dump"
        1543             :             !write(iulog,*) State_CAM_ps
        1544             :
        1545             :             ! TK: 288 283 277 271 266 261 ... 250 251 252
        1546             :             ! Seems like the vertical is OK for now
        1547             :         endif
        1548             :
        1549             :         !-----------------------------------------------------------------------
        1550             :         ! Set HEMCO options
        1551             :         !-----------------------------------------------------------------------
        1552             :         ! Range of species and emission categories.
        1553             :         ! Set Extension number ExtNr to 0, indicating that the core
        1554             :         ! module shall be executed.
        1555           0 :         HcoState%Options%SpcMin = 1
        1556           0 :         HcoState%Options%SpcMax = -1
        1557           0 :         HcoState%Options%CatMin = 1
        1558           0 :         HcoState%Options%CatMax = -1
        1559           0 :         HcoState%Options%ExtNr  = 0
        1560             :
        1561             :         ! Use temporary array?
        1562           0 :         HcoState%Options%FillBuffer = .FALSE.
        1563             :
        1564             :         !-----------------------------------------------------------------------
        1565             :         ! Run HEMCO!
        1566             :         !-----------------------------------------------------------------------
        1567             :
        1568           0 :         call t_startf('HCO_HCOX_Run')
        1569             :
        1570             :         ! Run HCO core module
        1571             :         ! Pass phase as argument. Phase 1 will update the emissions list,
        1572             :         ! phase 2 will calculate the emissions. Emissions will be written into
        1573             :         ! the corresponding flux arrays in HcoState.
        1574             :         !
        1575             :         ! FIXME: hplin - setting false as last timestep of simulation. maybe see
        1576             :         ! if we can figure out from CAM if we are at run end and set to true
        1577           0 :         call HCO_Run( HcoState, 1, HMRC, IsEndStep=.false. )
        1578           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
        1579           0 :             write(iulog,*) "******************************************"
        1580           0 :             write(iulog,*) "HEMCO_CESM: HCO_Run Phase 1 has failed!    "
        1581           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!       "
        1582           0 :             write(iulog,*) "A critical component in HEMCO failed to run."
        1583           0 :             write(iulog,*) "This may be due to misconfiguration, or a bug."
        1584           0 :             write(iulog,*) "Please refer to the HEMCO.log log file in your"
        1585           0 :             write(iulog,*) "case run directory or as configured in HEMCO_Config.rc"
        1586           0 :             write(iulog,*) "for more information."
        1587           0 :             write(iulog,*) "******************************************"
        1588             :         endif
        1589           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1590             :
        1591           0 :         if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: HCO_Run Phase 1"
        1592             :
        1593           0 :         call HCO_Run( HcoState, 2, HMRC, IsEndStep=.false. )
        1594           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
        1595           0 :             write(iulog,*) "******************************************"
        1596           0 :             write(iulog,*) "HEMCO_CESM: HCO_Run Phase 2 has failed!    "
        1597           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!       "
        1598           0 :             write(iulog,*) "A critical component in HEMCO failed to run."
        1599           0 :             write(iulog,*) "This may be due to misconfiguration, or a bug."
        1600           0 :             write(iulog,*) "Please refer to the HEMCO.log log file in your"
        1601           0 :             write(iulog,*) "case run directory or as configured in HEMCO_Config.rc"
        1602           0 :             write(iulog,*) "for more information."
        1603           0 :             write(iulog,*) "******************************************"
        1604             :         endif
        1605           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1606             :
        1607           0 :         if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: HCO_Run Phase 2"
        1608             :
        1609             :         !-----------------------------------------------------------------------
        1610             :         ! Run HEMCO Extensions!
        1611             :         !-----------------------------------------------------------------------
        1612           0 :         call HCOX_Run(HcoState, ExtState, HMRC)
        1613           0 :         if(masterproc .and. HMRC /= HCO_SUCCESS) then
        1614           0 :             write(iulog,*) "******************************************"
        1615           0 :             write(iulog,*) "HEMCO_CESM: HCOX_Run (extensions) has failed!"
        1616           0 :             write(iulog,*) "THIS ERROR ORIGINATED WITHIN HEMCO!"
        1617           0 :             write(iulog,*) "A critical component in HEMCO failed to run."
        1618           0 :             write(iulog,*) "This may be due to misconfiguration, or a bug."
        1619           0 :             write(iulog,*) "Please refer to the HEMCO.log log file in your"
        1620           0 :             write(iulog,*) "case run directory or as configured in HEMCO_Config.rc"
        1621           0 :             write(iulog,*) "for more information."
        1622           0 :             write(iulog,*) "******************************************"
        1623             :         endif
        1624           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1625             :
        1626           0 :         if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: HCOX_Run"
        1627             :
        1628           0 :         call t_stopf('HCO_HCOX_Run')
        1629             :
        1630             :         !-----------------------------------------------------------------------
        1631             :         ! Update "autofill" diagnostics.
        1632             :         ! Update all 'AutoFill' diagnostics. This makes sure that all
        1633             :         ! diagnostics fields with the 'AutoFill' flag are up-to-date. The
        1634             :         ! AutoFill flag is specified when creating a diagnostics container
        1635             :         ! (Diagn_Create).
        1636             :         !-----------------------------------------------------------------------
        1637           0 :         call HcoDiagn_AutoUpdate(HcoState, HMRC)
        1638           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1639             :
        1640             :         !if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: HcoDiagn_AutoUpdate"
        1641             :
        1642             :         !-----------------------------------------------------------------------
        1643             :         ! Tell HEMCO we are done for this timestep...
        1644             :         !-----------------------------------------------------------------------
        1645           0 :         call HcoClock_EmissionsDone(HcoState%Clock, HMRC)
        1646           0 :         ASSERT_(HMRC==HCO_SUCCESS)
        1647             :
        1648             :         !if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: HcoClock_EmissionsDone"
        1649             :
        1650             :         !-----------------------------------------------------------------------
        1651             :         ! Do some testing and write emissions to the tape
        1652             :         !-----------------------------------------------------------------------
        1653             :
        1654             :         ! HCO Index boundaries
        1655           0 :         HI = my_IE - my_IS + 1
        1656           0 :         HJ = my_JE - my_JS + 1
        1657           0 :         HL = LM
        1658             :
        1659             :         ! For each species...
        1660           0 :         do spcID = 1, HcoConfig%nModelSpc
        1661             :
        1662             :             ! TODO: Eventually convert aerosol number emissions from mass fluxes
        1663             :             ! directly rather than using scale factors for num_ax (1/12/23, hplin)
        1664             :
        1665             :             ! Build history / pbuf field name (HCO_NO, HCO_CO, etc.)
        1666           0 :             exportName = 'HCO_' // trim(HcoConfig%ModelSpc(spcID)%SpcName)
        1667           0 :             doExport   = (FIRST .or. associated(HcoState%Spc(spcID)%Emis%Val))
        1668             :             ! if(masterproc) write(iulog,*) "HEMCO_CESM: Begin exporting " // trim(exportName)
        1669             :
        1670             :             ! Get HEMCO emissions flux [kg/m2/s].
        1671             :             ! For performance optimization ... tap into HEMCO structure directly (ugly ugly)
        1672             :             ! No need to flip vertical here. The regridder will do it for us
        1673           0 :             if(associated(HcoState%Spc(spcID)%Emis%Val)) then
        1674           0 :                 if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1675             :                     ! Zero out quantities first
        1676           0 :                     exportFldHco(:,:,:) = 0.0_r8
        1677           0 :                     exportFldCAM(:,:)   = 0.0_r8
        1678             :
        1679             :                     ! Retrieve flux from HEMCO...
        1680           0 :                     exportFldHco(my_IS:my_IE,my_JS:my_JE,1:LM) = HcoState%Spc(spcID)%Emis%Val(1:HI,1:HJ,1:LM)
        1681             :
        1682             :                     ! Regrid exportFldHco to CAM grid...
        1683           0 :                     call HCO_Grid_HCO2CAM_3D(exportFldHco, exportFldCAM)
        1684             :
        1685             :                     ! Debug only: Output data for debug and comparing against logs
        1686             :                     ! if(masterproc) write(iulog, *) "HEMCO_CESM debug ", trim(exportName), " HCO min max sum ", minval(exportFldHco(my_IS:my_IE,my_JS:my_JE,1:LM)), maxval(exportFldHco(my_IS:my_IE,my_JS:my_JE,1:LM)), sum(exportFldHco(my_IS:my_IE,my_JS:my_JE,1:LM))
        1687             :                     ! if(masterproc) write(iulog, *) "HEMCO_CESM debug ", trim(exportName), " CAM min max sum ", minval(exportFldCAM), maxval(exportFldCAM), sum(exportFldCAM)
        1688           0 :                 elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1689             :                     ! Zero out quantities first
        1690           0 :                     exportFldHco2(:,:) = 0.0_r8
        1691           0 :                     exportFldCAM2(:)   = 0.0_r8
        1692             :
        1693             :                     ! Retrieve flux from HEMCO...
        1694             :                     ! Only surface emissions are supported here. Note, HEMCO emissions are with 1 = surface and LM = TOA. Use index 1. (hplin, 1/12/23)
        1695           0 :                     exportFldHco2(my_IS:my_IE,my_JS:my_JE)     = HcoState%Spc(spcID)%Emis%Val(1:HI,1:HJ,1)
        1696             :
        1697             :                     ! Regrid exportFldHco to CAM grid...
        1698           0 :                     call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1699             :
        1700             :                     ! Debug only: Output data for debug and comparing against logs
        1701             :                     ! if(masterproc) write(iulog, *) "HEMCO_CESM debug ", trim(exportName), " HCO min max sum ", minval(exportFldHco2(my_IS:my_IE,my_JS:my_JE)), maxval(exportFldHco2(my_IS:my_IE,my_JS:my_JE)), sum(exportFldHco2(my_IS:my_IE,my_JS:my_JE))
        1702             :                     ! if(masterproc) write(iulog, *) "HEMCO_CESM debug ", trim(exportName), " CAM min max sum ", minval(exportFldCAM2), maxval(exportFldCAM2), sum(exportFldCAM2)
        1703             :                 else
        1704           0 :                     ASSERT_(.false.)
        1705             :                 endif
        1706             :
        1707             :                 !if(masterproc) write(iulog,*) "HEMCO_CESM: Retrieved from HCO " // trim(exportName)
        1708             :             else
        1709             :                 ! No emission value. No need to run regrid, instead populate with zeros as needed
        1710             :                 ! Why not populate at top, you ask? Because zeroing out arrays is expensive, and
        1711             :                 ! we do not want to be doing twice the work.
        1712           0 :                 if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1713           0 :                     exportFldCAM(:,:) = 0.0_r8
        1714           0 :                 elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1715           0 :                     exportFldCAM2(:)  = 0.0_r8
        1716             :                 else
        1717           0 :                     ASSERT_(.false.)
        1718             :                 endif
        1719             :             endif
        1720             :
        1721             :             ! Handle deposition flux from deposition velocity [1/s]
        1722             :             ! This can be performed on the CAM grid. (hplin, 5/7/21)
        1723             :             ! GEOS-Chem: (from v/v dry)
        1724             :             !  Step 1)
        1725             :             !              dflx(I,J,NA) = dflx(I,J,NA)                                     &
        1726             :             !              + ( dep * spc(I,J,NA) / (AIRMW / ThisSpc%MW_g)  )
        1727             :             ! for kg/kg dry, no conversion is needed:
        1728             :             !  Step 1a)    dflx = dflx + dep * spc
        1729             :             !
        1730             :             !  Step 2) Convert to 1/s
        1731             :             !             dflx(I,J,:) = dflx(I,J,:) * State_Met%AD(I,J,1)                        &
        1732             :             !                     / State_Grid%Area_M2(I,J)
        1733             :             !
        1734             :             !  Note that, AD is actually DELP_DRY * G0_100 * AREA_M2, thus the final expression is
        1735             :             !  just multiplied by DELP_DRY * G0_100, unit: kg/m2 (delp_dry is hPa, g0_100 is 100 Pa/hPa * s2/m --> unit = Pa*m/s2 = kg/m/s2*s2/m = kg/m2)
        1736             :             !  Multiplied by 1/s, this gives kg/m2/s
        1737             :             !
        1738             :             ! We retrieve the concentration flux read from the convert state module
        1739             :             ! (on the CAM grid) and loop through it to apply deposition fluxes.
        1740           0 :             if(associated(HcoState%Spc(spcID)%Depv%Val)) then
        1741             :                 ! Check if species is available for deposition (hard-coded)
        1742             :                 ! FIXME: hplin 5/7/21
        1743           0 :                 if(trim(HcoConfig%ModelSpc(spcID)%SpcName) == "DMS" .or.            &
        1744           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ACET" .or.           &
        1745           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3COCH3" .or.       &
        1746           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ALD2" .or.           &
        1747           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3CHO" .or.         &
        1748           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "MENO3" .or.          &
        1749           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ETNO3" .or.          &
        1750           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "MOH" .or.            &
        1751           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3OH") then
        1752             :
        1753             :                     ! Clear data
        1754           0 :                     exportFldCAMDep(:) = 0.0_r8
        1755             :
        1756             :                     ! Regrid deposition flux HCO to CAM
        1757           0 :                     exportFldHcoDep(my_IS:my_IE,my_JS:my_JE) = HcoState%Spc(spcID)%Depv%Val(1:HI,1:HJ)
        1758           0 :                     call HCO_Grid_HCO2CAM_2D(exportFldHcoDep, exportFldCAMDep)
        1759             :
        1760             :                     ! dbg:
        1761             :                     ! if(trim(HcoConfig%ModelSpc(spcID)%SpcName) == "DMS") then
        1762             :                     !     dummy_2(:,:) = exportFldHco2(:,:)
        1763             :                     ! endif
        1764             :                 endif
        1765             :
        1766             :                 ! Perform handling: Note species-specific State_CAM_* data
        1767             :                 ! Note handling is for surface (idx LM for CAM inverted-atm)
        1768           0 :                 if(trim(HcoConfig%ModelSpc(spcID)%SpcName) == "DMS") then
        1769           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1770           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmDMS(:) * State_CAM_DELP_DRYs(:) * G0_100
        1771           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1772           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmDMS(:) * State_CAM_DELP_DRYs(:) * G0_100
        1773             :                     else
        1774           0 :                         ASSERT_(.false.)
        1775             :                     endif
        1776             :                 elseif( &
        1777           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ACET" .or. &
        1778           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3COCH3") then
        1779           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1780           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmACET(:) * State_CAM_DELP_DRYs(:) * G0_100
        1781           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1782           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmACET(:) * State_CAM_DELP_DRYs(:) * G0_100
        1783             :                     else
        1784           0 :                         ASSERT_(.false.)
        1785             :                     endif
        1786             :                 elseif( &
        1787           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ALD2" .or. &
        1788           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3CHO") then
        1789           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1790           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmALD2(:) * State_CAM_DELP_DRYs(:) * G0_100
        1791           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1792           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmALD2(:) * State_CAM_DELP_DRYs(:) * G0_100
        1793             :                     else
        1794           0 :                         ASSERT_(.false.)
        1795             :                     endif
        1796             :                 elseif( &
        1797           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "MOH" .or. &
        1798           0 :                    trim(HcoConfig%ModelSpc(spcID)%SpcName) == "CH3OH") then
        1799           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1800           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmMOH(:) * State_CAM_DELP_DRYs(:) * G0_100
        1801           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1802           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmMOH(:) * State_CAM_DELP_DRYs(:) * G0_100
        1803             :                     else
        1804           0 :                         ASSERT_(.false.)
        1805             :                     endif
        1806           0 :                 elseif(trim(HcoConfig%ModelSpc(spcID)%SpcName) == "MENO3") then
        1807           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1808           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmMENO3(:) * State_CAM_DELP_DRYs(:) * G0_100
        1809           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1810           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmMENO3(:) * State_CAM_DELP_DRYs(:) * G0_100
        1811             :                     else
        1812           0 :                         ASSERT_(.false.)
        1813             :                     endif
        1814           0 :                 elseif(trim(HcoConfig%ModelSpc(spcID)%SpcName) == "ETNO3") then
        1815           0 :                     if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1816           0 :                         exportFldCAM(LM,:) = exportFldCAM(LM,:) - exportFldCAMDep(:) * State_CAM_chmETNO3(:) * State_CAM_DELP_DRYs(:) * G0_100
        1817           0 :                     elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1818           0 :                         exportFldCAM2(:)   = exportFldCAM2(:)   - exportFldCAMDep(:) * State_CAM_chmETNO3(:) * State_CAM_DELP_DRYs(:) * G0_100
        1819             :                     else
        1820           0 :                         ASSERT_(.false.)
        1821             :                     endif
        1822             :                 endif
        1823             :             endif
        1824             :
        1825           0 :             if(doExport) then
        1826           0 :                 if(HcoConfig%ModelSpc(spcID)%DimMax .eq. 3) then
        1827             :                     ! Write to history on CAM mesh
        1828           0 :                     call HCO_Export_History_CAM3D(exportName, exportFldCAM)
        1829             :
        1830             :                     ! Write to physics buffer (pass model name)
        1831           0 :                     call HCO_Export_Pbuf_CAM3D(HcoConfig%ModelSpc(spcID)%SpcName, spcID, exportFldCAM)
        1832           0 :                 elseif(HcoConfig%ModelSpc(spcID)%DimMax .eq. 2) then
        1833             :                     ! Write to history on CAM mesh
        1834           0 :                     call HCO_Export_History_CAM2D(exportName, exportFldCAM2)
        1835             :
        1836             :                     ! Write to physics buffer (pass model name)
        1837           0 :                     call HCO_Export_Pbuf_CAM2D(HcoConfig%ModelSpc(spcID)%SpcName, spcID, exportFldCAM2)
        1838             :                 else
        1839           0 :                     ASSERT_(.false.)
        1840             :                 endif
        1841             :             endif
        1842             :
        1843             :         enddo
        1844             :
        1845             :
        1846             :         !-----------------------------------------------------------------------
        1847             :         ! Update aerosol number emissions with correct parameters
        1848             :         ! for CAM-chem and CESM2-GC
        1849             :         !
        1850             :         ! TODO: Implement later. Now using HEMCO config file method (hplin, 5/7/21)
        1851             :         !-----------------------------------------------------------------------
        1852             :         ! call HCO_Calc_Aero_Emis ( ... )
        1853             :
        1854             :         !-----------------------------------------------------------------------
        1855             :         ! Handle special diagnostics for some extensions
        1856             :         !-----------------------------------------------------------------------
        1857             :
        1858             :         ! Reset pointers first. Always do this beforehand
        1859           0 :         Ptr2D => NULL()
        1860             :
        1861             :         ! Eventually save necessary deposition FLUXES from extensions.
        1862           0 :         if(ExtState%ParaNOx > 0) then
        1863             :             ! PAR_O3_DEP, PAR_HNO3_DEP
        1864           0 :             exportName = 'HCO_PAR_O3_DEP'
        1865           0 :             exportNameTmp = 'PAR_O3_DEP'
        1866             :             call GetHcoDiagn(HcoState, ExtState, DiagnName='PARANOX_O3_DEPOSITION_FLUX', &
        1867           0 :                              StopIfNotFound=.false., Ptr2D=Ptr2D, RC=HMRC)
        1868             :
        1869           0 :             if(.not. associated(Ptr2D)) then
        1870           0 :                 write(6,*) "hplin debug err: cannot find paranox o3 dep flux"
        1871             :             endif
        1872             :
        1873           0 :             exportFldHco2(:,:) = 0.0_r8
        1874           0 :             exportFldCAM2(:)   = 0.0_r8
        1875           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. associated(Ptr2D)))
        1876           0 :             if(HMRC == HCO_SUCCESS .and. associated(Ptr2D)) then
        1877           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        1878           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1879             :             endif
        1880             :
        1881           0 :             if(doExport) then
        1882           0 :                 call HCO_Export_History_CAM2D(exportName, exportFldCAM2)
        1883           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1884             :             endif
        1885           0 :             Ptr2D => NULL()
        1886             :
        1887           0 :             exportName = 'HCO_PAR_HNO3_DEP'
        1888           0 :             exportNameTmp = 'PAR_HNO3_DEP'
        1889             :             call GetHcoDiagn(HcoState, ExtState, DiagnName='PARANOX_HNO3_DEPOSITION_FLUX', &
        1890           0 :                              StopIfNotFound=.false., Ptr2D=Ptr2D, RC=HMRC)
        1891             :
        1892           0 :             exportFldHco2(:,:) = 0.0_r8
        1893           0 :             exportFldCAM2(:)   = 0.0_r8
        1894           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. associated(Ptr2D)))
        1895           0 :             if(HMRC == HCO_SUCCESS .and. associated(Ptr2D)) then
        1896           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        1897           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1898             :             endif
        1899             :
        1900           0 :             if(doExport) then
        1901           0 :                 call HCO_Export_History_CAM2D(exportName, exportFldCAM2)
        1902           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1903             :             endif
        1904           0 :             Ptr2D => NULL()
        1905             :         endif
        1906             :
        1907             :         !-----------------------------------------------------------------------
        1908             :         ! Do we need to do additional exports for CESM-GC?
        1909             :         !-----------------------------------------------------------------------
        1910             :
        1911           0 :         if(chem_is('GEOS-Chem')) then
        1912           0 :             if(masterproc) write(iulog,*) "HEMCO_CESM: starting exports to GEOS-Chem"
        1913           0 :             do N = 0, 72
        1914             :                 ! Assume success
        1915           0 :                 HMRC = HCO_SUCCESS
        1916             :
        1917             :                 ! LANDTYPExx
        1918           0 :                 write(exportNameTmp, '(a,i2.2)') 'LANDTYPE', N
        1919           0 :                 exportName = 'HCO_' // trim(exportNameTmp)
        1920             :
        1921           0 :                 exportFldCAM2(:)   = 0.0_r8
        1922             :
        1923             :                 ! Grab the pointer if available
        1924           0 :                 call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        1925           0 :                 doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        1926           0 :                 if(HMRC == HCO_SUCCESS .and. FND) then
        1927           0 :                     exportFldHco2(:,:) = Ptr2D(:,:) ! Have to promote precision
        1928           0 :                     call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1929             :                 endif
        1930             :
        1931           0 :                 if(doExport) then
        1932           0 :                     call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1933             :                 endif
        1934           0 :                 Ptr2D => NULL()
        1935             :
        1936             :                 ! XLAIxx
        1937           0 :                 write(exportNameTmp, '(a,i2.2)') 'XLAI', N
        1938           0 :                 exportName = 'HCO_' // trim(exportNameTmp)
        1939             :
        1940           0 :                 exportFldCAM2(:)   = 0.0_r8
        1941             :
        1942             :                 ! Grab the pointer if available
        1943           0 :                 call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        1944           0 :                 doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        1945           0 :                 if(HMRC == HCO_SUCCESS .and. FND) then
        1946           0 :                     exportFldHco2(:,:) = Ptr2D(:,:) ! Have to promote precision
        1947           0 :                     call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1948             :                 endif
        1949             :
        1950           0 :                 if(doExport) then
        1951           0 :                     call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1952             :                 endif
        1953           0 :                 Ptr2D => NULL()
        1954             :             enddo
        1955             :
        1956             :             ! VMR_CH3CL
        1957           0 :             write(exportNameTmp, '(a)') 'VMR_CH3CL'
        1958             :
        1959           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1960           0 :             exportFldCAM2(:) = 0.0_r8
        1961             :
        1962           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CH3CL', exportFldHco2, HMRC, FOUND=FND)
        1963           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        1964           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        1965           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1966             :             endif
        1967           0 :             if(doExport) then
        1968           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1969             :             endif
        1970             :
        1971             :             ! VMR_CH2CL2
        1972           0 :             write(exportNameTmp, '(a)') 'VMR_CH2CL2'
        1973             :
        1974           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1975           0 :             exportFldCAM2(:) = 0.0_r8
        1976             :
        1977           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CH2CL2', exportFldHco2, HMRC, FOUND=FND)
        1978           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        1979           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        1980           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1981             :             endif
        1982           0 :             if(doExport) then
        1983           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1984             :             endif
        1985             :
        1986             :             ! VMR_CHCL3
        1987           0 :             write(exportNameTmp, '(a)') 'VMR_CHCL3'
        1988             :
        1989           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        1990           0 :             exportFldCAM2(:) = 0.0_r8
        1991             :
        1992           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CHCL3', exportFldHco2, HMRC, FOUND=FND)
        1993           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        1994           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        1995           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        1996             :             endif
        1997           0 :             if(doExport) then
        1998           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        1999             :             endif
        2000             :
        2001             :             ! VMR_CH3BR
        2002           0 :             write(exportNameTmp, '(a)') 'VMR_CH3BR'
        2003             :
        2004           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2005           0 :             exportFldCAM2(:) = 0.0_r8
        2006             :
        2007           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CH3BR', exportFldHco2, HMRC, FOUND=FND)
        2008           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2009           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2010           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2011             :             endif
        2012           0 :             if(doExport) then
        2013           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2014             :             endif
        2015             :
        2016             :             ! VMR_CCL4
        2017           0 :             write(exportNameTmp, '(a)') 'VMR_CCL4'
        2018             :
        2019           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2020           0 :             exportFldCAM2(:) = 0.0_r8
        2021             :
        2022           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CCL4', exportFldHco2, HMRC, FOUND=FND)
        2023           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2024           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2025           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2026             :             endif
        2027           0 :             if(doExport) then
        2028           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2029             :             endif
        2030             :
        2031             :             ! VMR_CFC113
        2032           0 :             write(exportNameTmp, '(a)') 'VMR_CFC113'
        2033             :
        2034           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2035           0 :             exportFldCAM2(:) = 0.0_r8
        2036             :
        2037           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CFC113', exportFldHco2, HMRC, FOUND=FND)
        2038           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2039           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2040           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2041             :             endif
        2042           0 :             if(doExport) then
        2043           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2044             :             endif
        2045             :
        2046             :             ! VMR_CFC114
        2047           0 :             write(exportNameTmp, '(a)') 'VMR_CFC114'
        2048             :
        2049           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2050           0 :             exportFldCAM2(:) = 0.0_r8
        2051             :
        2052           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CFC114', exportFldHco2, HMRC, FOUND=FND)
        2053           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2054           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2055           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2056             :             endif
        2057           0 :             if(doExport) then
        2058           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2059             :             endif
        2060             :
        2061             :             ! VMR_CFC115
        2062           0 :             write(exportNameTmp, '(a)') 'VMR_CFC115'
        2063             :
        2064           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2065           0 :             exportFldCAM2(:) = 0.0_r8
        2066             :
        2067           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CFC115', exportFldHco2, HMRC, FOUND=FND)
        2068           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2069           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2070           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2071             :             endif
        2072           0 :             if(doExport) then
        2073           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2074             :             endif
        2075             :
        2076             :             ! VMR_CFC11
        2077           0 :             write(exportNameTmp, '(a)') 'VMR_CFC11'
        2078             :
        2079           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2080           0 :             exportFldCAM2(:) = 0.0_r8
        2081             :
        2082           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CFC11', exportFldHco2, HMRC, FOUND=FND)
        2083           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2084           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2085           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2086             :             endif
        2087           0 :             if(doExport) then
        2088           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2089             :             endif
        2090             :
        2091             :             ! VMR_CFC12
        2092           0 :             write(exportNameTmp, '(a)') 'VMR_CFC12'
        2093             :
        2094           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2095           0 :             exportFldCAM2(:) = 0.0_r8
        2096             :
        2097           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CFC12', exportFldHco2, HMRC, FOUND=FND)
        2098           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2099           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2100           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2101             :             endif
        2102           0 :             if(doExport) then
        2103           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2104             :             endif
        2105             :
        2106             :             ! VMR_CH3CCL3
        2107           0 :             write(exportNameTmp, '(a)') 'VMR_CH3CCL3'
        2108             :
        2109           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2110           0 :             exportFldCAM2(:) = 0.0_r8
        2111             :
        2112           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_CH3CCL3', exportFldHco2, HMRC, FOUND=FND)
        2113           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2114           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2115           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2116             :             endif
        2117           0 :             if(doExport) then
        2118           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2119             :             endif
        2120             :
        2121             :             ! VMR_H1211
        2122           0 :             write(exportNameTmp, '(a)') 'VMR_H1211'
        2123             :
        2124           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2125           0 :             exportFldCAM2(:) = 0.0_r8
        2126             :
        2127           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_H1211', exportFldHco2, HMRC, FOUND=FND)
        2128           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2129           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2130           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2131             :             endif
        2132           0 :             if(doExport) then
        2133           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2134             :             endif
        2135             :
        2136             :             ! VMR_H1301
        2137           0 :             write(exportNameTmp, '(a)') 'VMR_H1301'
        2138             :
        2139           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2140           0 :             exportFldCAM2(:) = 0.0_r8
        2141             :
        2142           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_H1301', exportFldHco2, HMRC, FOUND=FND)
        2143           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2144           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2145           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2146             :             endif
        2147           0 :             if(doExport) then
        2148           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2149             :             endif
        2150             :
        2151             :             ! VMR_H2402
        2152           0 :             write(exportNameTmp, '(a)') 'VMR_H2402'
        2153             :
        2154           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2155           0 :             exportFldCAM2(:) = 0.0_r8
        2156             :
        2157           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_H2402', exportFldHco2, HMRC, FOUND=FND)
        2158           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2159           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2160           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2161             :             endif
        2162           0 :             if(doExport) then
        2163           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2164             :             endif
        2165             :
        2166             :             ! VMR_HCFC141B
        2167           0 :             write(exportNameTmp, '(a)') 'VMR_HCFC141B'
        2168             :
        2169           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2170           0 :             exportFldCAM2(:) = 0.0_r8
        2171             :
        2172           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_HCFC141B', exportFldHco2, HMRC, FOUND=FND)
        2173           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2174           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2175           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2176             :             endif
        2177           0 :             if(doExport) then
        2178           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2179             :             endif
        2180             :
        2181             :             ! VMR_HCFC142B
        2182           0 :             write(exportNameTmp, '(a)') 'VMR_HCFC142B'
        2183             :
        2184           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2185           0 :             exportFldCAM2(:) = 0.0_r8
        2186             :
        2187           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_HCFC142B', exportFldHco2, HMRC, FOUND=FND)
        2188           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2189           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2190           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2191             :             endif
        2192           0 :             if(doExport) then
        2193           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2194             :             endif
        2195             :
        2196             :             ! VMR_HCFC22
        2197           0 :             write(exportNameTmp, '(a)') 'VMR_HCFC22'
        2198             :
        2199           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2200           0 :             exportFldCAM2(:) = 0.0_r8
        2201             :
        2202           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_HCFC22', exportFldHco2, HMRC, FOUND=FND)
        2203           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2204           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2205           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2206             :             endif
        2207           0 :             if(doExport) then
        2208           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2209             :             endif
        2210             :
        2211             :             ! VMR_N2O
        2212           0 :             write(exportNameTmp, '(a)') 'VMR_N2O'
        2213             :
        2214           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2215           0 :             exportFldCAM2(:) = 0.0_r8
        2216             :
        2217           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_N2O', exportFldHco2, HMRC, FOUND=FND)
        2218           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2219           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2220           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2221             :             endif
        2222           0 :             if(doExport) then
        2223           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2224             :             endif
        2225             :
        2226             :             ! VMR_OCS
        2227           0 :             write(exportNameTmp, '(a)') 'VMR_OCS'
        2228             :
        2229           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2230           0 :             exportFldCAM2(:) = 0.0_r8
        2231             :
        2232           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_OCS', exportFldHco2, HMRC, FOUND=FND)
        2233           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2234           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2235           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2236             :             endif
        2237           0 :             if(doExport) then
        2238           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2239             :             endif
        2240             :
        2241             :             ! VMR_H2
        2242           0 :             write(exportNameTmp, '(a)') 'VMR_H2'
        2243             :
        2244           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2245           0 :             exportFldCAM2(:) = 0.0_r8
        2246             :
        2247           0 :             call HCO_EvalFld(HcoState, 'SfcVMR_H2', exportFldHco2, HMRC, FOUND=FND)
        2248           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2249           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2250           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2251             :             endif
        2252           0 :             if(doExport) then
        2253           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2254             :             endif
        2255             :
        2256             :             ! UVALBEDO
        2257             :             ! Warning: Keep these exportNameTmp as it allows for reuse of
        2258             :             ! code below. (hplin, 2/28/21)
        2259           0 :             write(exportNameTmp, '(a)') 'UV_ALBEDO'
        2260             :
        2261             :             ! Reusable code templating below.
        2262           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2263             :
        2264             :             ! Reset data for safe export at first time step
        2265           0 :             exportFldCAM2(:) = 0.0_r8
        2266             :
        2267           0 :             call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        2268           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2269           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2270           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2271           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2272             :             endif
        2273           0 :             if(doExport) then
        2274           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2275             :             endif
        2276           0 :             Ptr2D => NULL()
        2277             :
        2278             :             ! SURF_SALINITY
        2279             :             ! Note: the name is too long, reduce to HCO_salinity, HCO_iodide
        2280           0 :             write(exportNameTmp, '(a)') 'salinity'
        2281           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2282             :
        2283             :             ! Reset data for safe export at first time step
        2284           0 :             exportFldCAM2(:) = 0.0_r8
        2285             :
        2286           0 :             call HCO_GetPtr(HcoState, 'surf_salinity', Ptr2D, HMRC, FOUND=FND)
        2287           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2288           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2289           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2290           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2291             :             endif
        2292           0 :             if(doExport) then
        2293           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2294             :             endif
        2295           0 :             Ptr2D => NULL()
        2296             :
        2297             :             ! SURF_IODIDE
        2298           0 :             write(exportNameTmp, '(a)') 'iodide'
        2299           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2300             :
        2301             :             ! Reset data for safe export at first time step
        2302           0 :             exportFldCAM2(:) = 0.0_r8
        2303             :
        2304           0 :             call HCO_GetPtr(HcoState, 'surf_iodide', Ptr2D, HMRC, FOUND=FND)
        2305           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2306           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2307           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2308           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2309             :             endif
        2310           0 :             if(doExport) then
        2311           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2312             :             endif
        2313           0 :             Ptr2D => NULL()
        2314             :
        2315             :             ! OMOC_DJF
        2316           0 :             write(exportNameTmp, '(a)') 'OMOC_DJF'
        2317           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2318             :
        2319             :             ! Reset data for safe export at first time step
        2320           0 :             exportFldCAM2(:) = 0.0_r8
        2321             :
        2322           0 :             call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        2323           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2324           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2325           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2326           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2327             :             endif
        2328           0 :             if(doExport) then
        2329           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2330             :             endif
        2331           0 :             Ptr2D => NULL()
        2332             :
        2333             :             ! OMOC_MAM
        2334           0 :             write(exportNameTmp, '(a)') 'OMOC_MAM'
        2335           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2336             :
        2337             :             ! Reset data for safe export at first time step
        2338           0 :             exportFldCAM2(:) = 0.0_r8
        2339             :
        2340           0 :             call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        2341           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2342           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2343           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2344           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2345             :             endif
        2346           0 :             if(doExport) then
        2347           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2348             :             endif
        2349           0 :             Ptr2D => NULL()
        2350             :
        2351             :             ! OMOC_JJA
        2352           0 :             write(exportNameTmp, '(a)') 'OMOC_JJA'
        2353           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2354             :
        2355             :             ! Reset data for safe export at first time step
        2356           0 :             exportFldCAM2(:) = 0.0_r8
        2357             :
        2358           0 :             call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        2359           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2360           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2361           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2362           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2363             :             endif
        2364           0 :             if(doExport) then
        2365           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2366             :             endif
        2367           0 :             Ptr2D => NULL()
        2368             :
        2369             :             ! OMOC_SON
        2370           0 :             write(exportNameTmp, '(a)') 'OMOC_SON'
        2371           0 :             exportName = 'HCO_' // trim(exportNameTmp)
        2372             :
        2373             :             ! Reset data for safe export at first time step
        2374           0 :             exportFldCAM2(:) = 0.0_r8
        2375             :
        2376           0 :             call HCO_GetPtr(HcoState, exportNameTmp, Ptr2D, HMRC, FOUND=FND)
        2377           0 :             doExport = (FIRST .or. (HMRC == HCO_SUCCESS .and. FND))
        2378           0 :             if(HMRC == HCO_SUCCESS .and. FND) then
        2379           0 :                 exportFldHco2(:,:) = Ptr2D(:,:)
        2380           0 :                 call HCO_Grid_HCO2CAM_2D(exportFldHco2, exportFldCAM2)
        2381             :             endif
        2382           0 :             if(doExport) then
        2383           0 :                 call HCO_Export_Pbuf_CAM2D(exportNameTmp, -1, exportFldCAM2)
        2384             :             endif
        2385           0 :             Ptr2D => NULL()
        2386             :
        2387           0 :             if(masterproc .and. nCalls < 10) write(iulog,*) "HEMCO_CESM: done with exports to GEOS-Chem"
        2388             :         endif
        2389             :
        2390             :         ! dummy_0_CAM(:,:) = iam * 1.0_r8
        2391             :
        2392             :         ! dummy_1(:,:,:) = iam * 1.0_r8
        2393             :
        2394             :         ! test data, but on the CAM grid... note vertical is inverted
        2395             :         ! dummy_0_CAM sizes 16384x512. remember dummy_CAM is K, I idx
        2396             :         ! my_CE: 512, pver: 32
        2397             :         ! write(6,*) "hplin debug: sizes dummy", size(dummy_0_CAM, 1), size(dummy_0_CAM, 2), &
        2398             :         !            size(State_CAM_ps, 1), my_CE, pver
        2399             :
        2400           0 :         dummy_0_CAM(:,:) = 0.0_r8
        2401             :         ! dummy_0_CAM(1,:) = State_CAM_TS
        2402             :         ! dummy_0_CAM(2,:) = State_CAM_U10M
        2403             :         ! dummy_0_CAM(3,:) = State_CAM_V10M
        2404             :         ! dummy_0_CAM(4,:) = State_CAM_ALBD
        2405             :         ! dummy_0_CAM(5,:) = State_CAM_LWI
        2406             :         ! dummy_0_CAM(6,:) = State_CAM_ps
        2407             :         ! dummy_0_CAM(7,:) = State_CAM_pblh
        2408             :         ! dummy_0_CAM(8,:) = State_CAM_CSZA
        2409             :         ! dummy_0_CAM(9,:) = State_CAM_psdry
        2410             :         ! dummy_0_CAM(10,:) = State_CAM_chmO3(LM,:)
        2411             :         ! dummy_0_CAM(11,:) = State_CAM_JNO2
        2412             :         ! dummy_0_CAM(12,:) = State_CAM_JOH
        2413             :         ! dummy_0_CAM(13,:) = scratchFldCAM2
        2414             :
        2415             :         ! fill with some test data, but clean the data first!
        2416             :         !dummy_1(:,:,:) = 0.0_r8
        2417           0 :         dummy_1_CAM(:,:) = 0.0_r8
        2418             :         ! dummy_1(:,:,1) = State_HCO_TS
        2419             :         ! dummy_1(:,:,2) = State_HCO_U10M
        2420             :         ! dummy_1(:,:,3) = State_HCO_V10M
        2421             :         ! dummy_1(:,:,4) = State_HCO_ALBD
        2422             :         ! dummy_1(:,:,5) = State_HCO_WLI
        2423             :         ! dummy_1(:,:,6) = State_HCO_PSFC
        2424             :         ! dummy_1(:,:,7) = State_HCO_PBLH
        2425             :         ! dummy_1(:,:,8) = State_HCO_CSZA
        2426             :         ! dummy_1(:,:,9) = State_HCO_AIR(:,:,1)
        2427             :         ! dummy_1(:,:,10) = State_HCO_AIR(:,:,2)
        2428             :         ! dummy_1(:,:,11) = Area_M2(my_IS:my_IE,my_JS:my_JE)
        2429             :         ! dummy_1(:,:,12) = State_HCO_chmO3(:,:,1)
        2430             :         ! dummy_1(:,:,13) = State_HCO_chmNO(:,:,1)
        2431             :
        2432             :         ! dummy_1(:,:,14) = HcoState%Grid%BXHEIGHT_M%Val(:,:,1)
        2433             :         ! dummy_1(:,:,15) = HcoState%Grid%BXHEIGHT_M%Val(:,:,2)
        2434             :         ! dummy_1(:,:,16) = State_HCO_F_OF_PBL(:,:,1)
        2435             :         ! dummy_1(:,:,17) = State_HCO_F_OF_PBL(:,:,2)
        2436             :         ! dummy_1(:,:,18) = dummy_2(:,:)
        2437             :
        2438             :         ! Regrid to CAM physics mesh!
        2439             :         !call HCO_Grid_HCO2CAM_3D(dummy_1, dummy_1_CAM)
        2440             :
        2441             :         ! Write to history on CAM mesh
        2442             :         !call HCO_Export_History_CAM3D("DIAG_HCO_TEST", dummy_1_CAM)
        2443             :         !call HCO_Export_History_CAM3D("DIAG_CAM_TEST", dummy_0_CAM)
        2444             :
        2445           0 :         if(masterproc .and. nCalls < 10) then
        2446           0 :             write(iulog,*) "HEMCO_CESM: Exports completed for this timestep!"
        2447             :         endif
        2448             :
        2449             :         !-----------------------------------------------------------------------
        2450             :         ! Finished!
        2451             :         !-----------------------------------------------------------------------
        2452             :         ! Update last execution time
        2453           0 :         last_HCO_day    = now_day
        2454           0 :         last_HCO_second = now_s
        2455             :
        2456           0 :         IF ( FIRST ) FIRST = .False.
        2457             :
        2458           0 :         RC = ESMF_SUCCESS
        2459             :
        2460           0 :     end subroutine HCO_GC_Run
        2461             :
        2462             :     !---------------------------------------------------------------------
        2463             :     ! Every HEMCO GridComp routine below likely will be just boilerplate
        2464             :     ! that does not need extensive maintenance
        2465             :     !---------------------------------------------------------------------
        2466             :
        2467             :     ! Init routine for the Gridded Component
        2468             :     ! Largely based off edyn_grid_comp::edyn_gcomp_init
        2469           0 :     subroutine HCO_GC_Init(GC, IMPORT, EXPORT, Clock, RC)
        2470           0 :         use spmd_utils,     only: masterproc
        2471             :         use cam_logfile,    only: iulog
        2472             :
        2473             :         ! Dummy arguments
        2474             :         type(ESMF_GridComp)                   :: GC
        2475             :         type(ESMF_State)                      :: IMPORT
        2476             :         type(ESMF_State)                      :: EXPORT
        2477             :         type(ESMF_Clock)                      :: Clock
        2478             :         integer, intent(out)                  :: RC
        2479             :
        2480             :         ! Local variables
        2481             :         character(len=*),       parameter     :: subname = 'HCO_GC_Init'
        2482             :
        2483             :         ! Note hplin 2/17/20: It seems like the physics mesh is re-created in
        2484             :         ! edyn_esmf through edyn_create_physmesh. It may be redundant to do
        2485             :         ! the CAM_DistGrid and CAM_PhysMesh maneuvers here and do this in
        2486             :         ! HCO_ESMF_Grid::HCO_Grid_ESMF_CreateCAM instead.
        2487             :
        2488           0 :         RC = ESMF_SUCCESS
        2489             :
        2490           0 :     end subroutine HCO_GC_Init
        2491             :
        2492             :     ! Finalize Gridded Component
        2493           0 :     subroutine HCO_GC_Final(GC, IMPORT, EXPORT, Clock, RC)
        2494             :         ! use ESMF,         only: ESMF_MeshDestroy
        2495             :
        2496             :         ! Dummy arguments
        2497             :         type(ESMF_GridComp)                   :: GC
        2498             :         type(ESMF_State)                      :: IMPORT
        2499             :         type(ESMF_State)                      :: EXPORT
        2500             :         type(ESMF_Clock)                      :: Clock
        2501             :         integer, intent(out)                  :: RC
        2502             :
        2503             :         ! Local variables
        2504             :         character(len=*),       parameter     :: subname = 'HCO_GC_Final'
        2505             :
        2506             :         ! call ESMF_MeshDestroy(CAM_PhysMesh, rc=RC)
        2507             :         ! ASSERT_(RC==ESMF_SUCCESS)
        2508             :
        2509           0 :         RC = ESMF_SUCCESS
        2510             :
        2511           0 :     end subroutine HCO_GC_Final
        2512             :
        2513           0 :     subroutine HCO_GC_SetServices(GC, RC)
        2514             :         use ESMF,         only: ESMF_GridCompSetEntryPoint
        2515             :         use ESMF,         only: ESMF_METHOD_INITIALIZE
        2516             :         use ESMF,         only: ESMF_METHOD_RUN
        2517             :         use ESMF,         only: ESMF_METHOD_FINALIZE
        2518             :
        2519             :         type(ESMF_GridComp)                   :: GC
        2520             :         integer, intent(out)                  :: RC
        2521             :         character(len=*),       parameter     :: subname = 'HCO_GC_SetServices'
        2522             :
        2523             :         ! Set the IRF methods as follows:
        2524             :         ! HEMCO Gridded Component dummy
        2525             :         !   > Init:     hemco_interface::HCO_GC_Init
        2526             :         !   > Run:      hemco_interface::HCO_GC_Run
        2527             :         !   > Final:    hemco_interface::HCO_GC_Final
        2528             :         !
        2529             :         ! Note from Steve: " all the actual regridding will have to happen inside the gridded component's run method."
        2530             :
        2531           0 :         call ESMF_GridCompSetEntryPoint(GC, ESMF_METHOD_INITIALIZE, userRoutine=HCO_GC_Init,  rc=RC)
        2532           0 :         ASSERT_(RC==ESMF_SUCCESS)
        2533             :
        2534           0 :         call ESMF_GridCompSetEntryPoint(GC, ESMF_METHOD_RUN,        userRoutine=HCO_GC_Run,   rc=RC)
        2535           0 :         ASSERT_(RC==ESMF_SUCCESS)
        2536             :
        2537           0 :         call ESMF_GridCompSetEntryPoint(GC, ESMF_METHOD_FINALIZE,   userRoutine=HCO_GC_Final, rc=RC)
        2538           0 :         ASSERT_(RC==ESMF_SUCCESS)
        2539           0 :     end subroutine HCO_GC_SetServices
        2540             : !EOC
        2541             : end module hemco_interface

Generated by: LCOV version 1.14