LCOV - code coverage report
Current view: | top level - hemco/HEMCO/src/Core - hcoio_write_std_mod.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 0 | 285 | 0.0 %
Date: | 2024-12-17 22:39:59 |  | Functions: | 0 | 2 | 0.0 %

              Line data    Source code
           1             : !BOC
           2             : #if defined ( MODEL_GCCLASSIC ) || defined( MODEL_WRF ) || defined( MODEL_CESM ) || defined( HEMCO_STANDALONE )
           3             : ! The 'standard' HEMCO I/O module is used for:
           4             : ! - HEMCO Standalone (HEMCO_STANDALONE)
           5             : ! - GEOS-Chem 'Classic' (MODEL_GCCLASSIC)
           6             : ! - WRF-GC (MODEL_WRF)
           7             : ! - CESM-GC and CAM-Chem / HEMCO-CESM (MODEL_CESM)
           8             : !EOC
           9             : !------------------------------------------------------------------------------
          10             : !                   Harmonized Emissions Component (HEMCO)                    !
          11             : !------------------------------------------------------------------------------
          12             : !BOP
          13             : !
          14             : ! !MODULE: hcoio_write_mod.F90
          15             : !
          16             : ! !DESCRIPTION: Module HCOIO\_write\_mod.F90 is the HEMCO data output
          17             : ! interface for the 'standard' model environment. It contains routines to
          18             : ! write out diagnostics into a netCDF file.
          19             : !\\
          20             : !\\
          21             : ! !INTERFACE:
          22             : !
          23             : MODULE HCOIO_Write_Mod
          24             : !
          25             : ! !USES:
          26             : !
          27             :   USE HCO_ERROR_MOD
          28             :   USE HCO_DIAGN_MOD
          29             :
          30             :   IMPLICIT NONE
          31             :   PRIVATE
          32             : !
          33             : ! !PUBLIC MEMBER FUNCTIONS:
          34             : !
          35             :   PUBLIC :: HCOIO_Write
          36             : !
          37             : ! !PRIVATE MEMBER FUNCTIONS:
          38             : !
          39             :   PRIVATE :: ConstructTimeStamp
          40             : !
          41             : ! !REMARKS:
          42             : !  HEMCO diagnostics are still in testing mode. We will fully activate them
          43             : !  at a later time.  They will be turned on when debugging & unit testing.
          44             : !
          45             : ! !REVISION HISTORY:
          46             : !  04 May 2014 - C. Keller   - Initial version
          47             : !  See https://github.com/geoschem/hemco for complete history
          48             : !EOP
          49             : !------------------------------------------------------------------------------
          50             : !BOC
          51             : !
          52             : ! !DEFINED PARAMETERS:
          53             : !
          54             :   ! Fill value used in HEMCO diagnostics netCDF files.
          55             : !  REAL(hp), PARAMETER :: FillValue = 1.e-31_hp
          56             :   REAL(sp), PARAMETER :: FillValue = HCO_MISSVAL
          57             :
          58             : CONTAINS
          59             : !EOC
          60             : !------------------------------------------------------------------------------
          61             : !                   Harmonized Emissions Component (HEMCO)                    !
          62             : !------------------------------------------------------------------------------
          63             : !BOP
          64             : !
          65             : ! !IROUTINE: HCOIO_write_std
          66             : !
          67             : ! !DESCRIPTION: Subroutine HCOIO\_write\_std writes diagnostics to
          68             : ! netCDF file. If the ForceWrite flag is set to TRUE, all diagnostics are
          69             : ! written out except they have already been written out during this time
          70             : ! step. This option is usually only used at the end of a simulation run.
          71             : ! If ForceWrite is False, only the diagnostics that are at the end of their
          72             : ! time averaging interval are written. For example, if the current month
          73             : ! is different from the previous (emissions) month, all diagnostics with
          74             : ! hourly, daily and monthly time averaging intervals are written out.
          75             : ! If the optional argument OnlyIfFirst is set to TRUE, diagnostics will
          76             : ! only be written out if its nnGetCalls is 1. This can be used to avoid
          77             : ! that diagnostics will be written out twice. The nnGetCalls is reset to
          78             : ! zero the first time a diagnostics is updated. For diagnostics that
          79             : ! point to data stored somewhere else (i.e. that simply contain a data
          80             : ! pointer, nnGetCalls is never reset and keeps counting.
          81             : !\\
          82             : !\\
          83             : ! !INTERFACE:
          84             : !
          85           0 :   SUBROUTINE HCOIO_Write( HcoState,    ForceWrite,                           &
          86             :                           RC,          PREFIX,      UsePrevTime,             &
          87             :                           OnlyIfFirst, COL                                  )
          88             : !
          89             : ! !USES:
          90             : !
          91             :     USE HCO_m_netCDF_io_define
          92             :     USE HCO_m_netcdf_io_read
          93             :     USE HCO_m_netcdf_io_open
          94             :     USE HCO_Ncdf_Mod,        ONLY : NC_Open
          95             :     USE HCO_Ncdf_Mod,        ONLY : NC_Read_Time
          96             :     USE HCO_Ncdf_Mod,        ONLY : NC_Read_Arr
          97             :     USE HCO_Ncdf_Mod,        ONLY : NC_Create
          98             :     USE HCO_Ncdf_Mod,        ONLY : NC_Close
          99             :     USE HCO_Ncdf_Mod,        ONLY : NC_Var_Def
         100             :     USE HCO_Ncdf_Mod,        ONLY : NC_Var_Write
         101             :     USE HCO_Ncdf_Mod,        ONLY : NC_Get_RefDateTime
         102             :     USE HCO_CHARPAK_Mod,     ONLY : TRANLC
         103             :     USE HCO_Chartools_Mod,   ONLY : HCO_CharParse
         104             :     USE HCO_State_Mod,       ONLY : HCO_State
         105             :     USE HCO_JulDay_Mod,      ONLY : JulDay
         106             :     USE HCO_EXTLIST_MOD,     ONLY : GetExtOpt, CoreNr
         107             :     USE HCO_Types_Mod,       ONLY : DiagnCont
         108             :     USE HCO_Clock_Mod
         109             :
         110             :     ! Parameters for netCDF routines
         111             :     include "netcdf.inc"
         112             : !
         113             : ! !INPUT PARAMETERS:
         114             : !
         115             :     TYPE(HCO_State),  POINTER                 :: HcoState    ! HEMCO state object
         116             :     LOGICAL,                    INTENT(IN   ) :: ForceWrite  ! Write all diagnostics?
         117             :     CHARACTER(LEN=*), OPTIONAL, INTENT(IN   ) :: PREFIX      ! File prefix
         118             :     LOGICAL,          OPTIONAL, INTENT(IN   ) :: UsePrevTime ! Use previous time
         119             :     LOGICAL,          OPTIONAL, INTENT(IN   ) :: OnlyIfFirst ! Only write if nnDiagn is 1
         120             :     INTEGER,          OPTIONAL, INTENT(IN   ) :: COL         ! Collection Nr.
         121             : !
         122             : ! !INPUT/OUTPUT PARAMETERS:
         123             : !
         124             :
         125             :     INTEGER,          INTENT(INOUT) :: RC          ! Failure or success
         126             : !
         127             : ! !REVISION HISTORY:
         128             : !  12 Sep 2013 - C. Keller   - Initial version
         129             : !  See https://github.com/geoschem/hemco for complete history
         130             : !EOP
         131             : !------------------------------------------------------------------------------
         132             : !BOC
         133             : !
         134             : ! !LOCAL VARIABLES:
         135             : !
         136             :     INTEGER                   :: I, PS, CNT, levIdTmp, indexL, indexR
         137             :     REAL(dp)                  :: GMT, JD1, JD1985, JD_DELTA, THISDAY, P0
         138             :     REAL(sp)                  :: TMP, JD_DELTA_RND
         139             :     INTEGER                   :: YYYY, MM, DD, h, m, s
         140           0 :     REAL(sp), POINTER         :: nctime(:)
         141           0 :     REAL(dp), POINTER         :: Arr1D(:)
         142           0 :     INTEGER,  POINTER         :: Int1D(:)
         143           0 :     REAL(sp), POINTER         :: Arr3D(:,:,:)
         144           0 :     REAL(sp), POINTER         :: Arr4D(:,:,:,:)
         145           0 :     REAL(sp), POINTER         :: Arr4DOld(:,:,:,:)
         146           0 :     REAL*8,   POINTER         :: timeVec(:)
         147           0 :     REAL(hp), POINTER         :: hyam(:)
         148           0 :     REAL(hp), POINTER         :: hybm(:)
         149             :     TYPE(DiagnCont), POINTER  :: ThisDiagn
         150             :     INTEGER                   :: FLAG
         151             :     CHARACTER(LEN=255)        :: ncFile
         152             :     CHARACTER(LEN=255)        :: Pfx, title, Reference, Contact
         153             :     CHARACTER(LEN=255)        :: myLName, mySName, myFterm
         154             :     CHARACTER(LEN=255)        :: MSG
         155             :     CHARACTER(LEN=255)        :: RefTime
         156             :     CHARACTER(LEN=4 )         :: Yrs
         157             :     CHARACTER(LEN=2 )         :: Mts, Dys, hrs, mns
         158             :     CHARACTER(LEN=31)         :: myName, myUnit, OutOper
         159             :     CHARACTER(LEN=63)         :: timeunit
         160             :     INTEGER                   :: fId, lonId, latId, levId, TimeId
         161             :     INTEGER                   :: VarCt
         162             :     INTEGER                   :: nLon, nLat, nLev, nLevTmp, nTime
         163             :     INTEGER                   :: Prc,  L
         164             :     INTEGER                   :: lymd, lhms
         165             :     INTEGER                   :: refYYYY, refMM, refDD, refh, refm, refs
         166             :     LOGICAL                   :: EOI, DoWrite, PrevTime, FOUND
         167             :     LOGICAL                   :: NoLevDim, DefMode
         168             :     LOGICAL                   :: IsOldFile
         169             :
         170             :     CHARACTER(LEN=255), PARAMETER :: LOC = 'HCOIO_WRITE_STD (hcoio_write_std_mod.F90)'
         171             :
         172             :     !=================================================================
         173             :     ! HCOIO_WRITE_STD begins here!
         174             :     !=================================================================
         175             :
         176             :     ! Init
         177           0 :     RC        =  HCO_SUCCESS
         178           0 :     CNT       =  0
         179           0 :     Arr1D     => NULL()
         180           0 :     Int1D     => NULL()
         181           0 :     Arr3D     => NULL()
         182           0 :     Arr4D     => NULL()
         183           0 :     Arr4DOld  => NULL()
         184           0 :     timeVec   => NULL()
         185           0 :     nctime    => NULL()
         186           0 :     ThisDiagn => NULL()
         187             :
         188             :     ! Collection number
         189           0 :     PS = HcoState%Diagn%HcoDiagnIDDefault
         190           0 :     IF ( PRESENT(COL) ) PS = COL
         191             :
         192             :     ! Check if it's time to write out this collection. Also set the
         193             :     ! end-of-interval EOI flag accordingly. This will be used lateron
         194             :     ! when calling Diagn_Get. Since all diagnostic containers in a
         195             :     ! given collection have the same output frequency, this is somewhat
         196             :     ! redundant (because we already check here if it is time to write
         197             :     ! out this particular collection). Keep it here for backwards
         198             :     ! consistency (ckeller, 8/6/2015).
         199           0 :     IF ( ForceWrite ) THEN
         200           0 :        DoWrite = .TRUE.
         201           0 :        EOI     = .FALSE.
         202             :     ELSE
         203           0 :        DoWrite = DiagnCollection_IsTimeToWrite( HcoState, PS )
         204           0 :        EOI     = .TRUE.
         205             :     ENDIF
         206             :
         207             :     ! Create current time stamps (to be used to archive time stamps)
         208             :     CALL HcoClock_Get( HcoState%Clock,sYYYY=YYYY,sMM=MM,&
         209           0 :                        sDD=DD,sH=h,sM=m,sS=s,RC=RC)
         210           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         211           0 :         CALL HCO_ERROR( 'ERROR 0', RC, THISLOC=LOC )
         212           0 :         RETURN
         213             :     ENDIF
         214           0 :     lymd = YYYY*10000 + MM*100 + DD
         215           0 :     lhms = h   *10000 + m *100 + s
         216             :
         217             :     ! Leave here if it's not time to write diagnostics. On the first
         218             :     ! time step, set lastYMD and LastHMS to current dates.
         219           0 :     IF ( .NOT. DoWrite ) THEN
         220           0 :        IF ( .NOT. DiagnCollection_LastTimesSet(HcoState%Diagn,PS) ) THEN
         221             :           CALL DiagnCollection_Set ( HcoState%Diagn, COL=PS, &
         222           0 :                                      LastYMD=lymd, LastHMS=lhms, RC=RC )
         223             :        ENDIF
         224           0 :        RETURN
         225             :     ENDIF
         226             :
         227             :     ! Inherit precision from HEMCO
         228           0 :     Prc = HP
         229             :
         230             :     ! Get PrevTime flag from input argument or set to default (=> TRUE)
         231           0 :     IF ( PRESENT(UsePrevTime) ) THEN
         232           0 :        PrevTime = UsePrevTime
         233             :     ELSE
         234           0 :        PrevTime = .TRUE.
         235             :     ENDIF
         236             :
         237             :     !-----------------------------------------------------------------
         238             :     ! Don't define level dimension if there are no 3D fields to write
         239             :     ! This is an optional feature. By default, all diagnostics have
         240             :     ! the full dimension definitions (lon,lat,lev,time) even if all
         241             :     ! output fields are only 2D. If the flag DiagnNoLevDim is
         242             :     ! enabled, the lev dimension is not defined if there are no 3D
         243             :     ! fields on the file.
         244             :     !-----------------------------------------------------------------
         245           0 :     NoLevDim = .FALSE.
         246             :     CALL GetExtOpt ( HcoState%Config, CoreNr, 'DiagnNoLevDim', &
         247           0 :                      OptValBool=NoLevDim, Found=Found, RC=RC )
         248           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         249           0 :         CALL HCO_ERROR( 'ERROR 1', RC, THISLOC=LOC )
         250           0 :         RETURN
         251             :     ENDIF
         252           0 :     IF ( Found ) THEN
         253           0 :        IF ( NoLevDim ) THEN
         254             :
         255             :           ! Loop over all diagnostics to see if any is 3D
         256           0 :           ThisDiagn => NULL()
         257             :           DO WHILE ( .TRUE. )
         258             :
         259             :              ! Get next diagnostics in list. This will return the next
         260             :              ! diagnostics container that contains content.
         261             :              CALL Diagn_Get ( HcoState, EOI, &
         262           0 :                               ThisDiagn, FLAG, RC, COL=PS )
         263           0 :              IF ( RC /= HCO_SUCCESS ) THEN
         264           0 :                  CALL HCO_ERROR( 'ERROR 2', RC, THISLOC=LOC )
         265           0 :                  RETURN
         266             :              ENDIF
         267           0 :              IF ( FLAG /= HCO_SUCCESS ) EXIT
         268             :
         269             :              ! If this is a 3D diagnostics, we must write the level
         270             :              ! coordinate
         271           0 :              IF ( ThisDiagn%SpaceDim == 3 ) THEN
         272           0 :                 NoLevDim = .FALSE.
         273           0 :                 EXIT
         274             :              ENDIF
         275             :           ENDDO
         276             :        ENDIF
         277             :     ENDIF
         278             :
         279             :     !-----------------------------------------------------------------
         280             :     ! Create output file
         281             :     !-----------------------------------------------------------------
         282             :
         283             :     ! Define grid dimensions
         284           0 :     nLon  = HcoState%NX
         285           0 :     nLat  = HcoState%NY
         286           0 :     nLev  = HcoState%NZ
         287           0 :     nTime = 1
         288             :
         289             :     ! Initialize mirror variables
         290           0 :     allocate(Arr4D(nlon,nlat,nlev,ntime))
         291           0 :     allocate(Arr3D(nlon,nlat,ntime))
         292           0 :     Arr3D = 0.0_sp
         293           0 :     Arr4D = 0.0_sp
         294             :
         295             :     ! Construct filename: diagnostics will be written into file
         296             :     ! PREFIX.YYYYMMDDhm.nc, where PREFIX is the input argument or
         297             :     ! (if not present) obtained from the HEMCO configuration file.
         298             :     CALL ConstructTimeStamp ( HcoState, PS, PrevTime, &
         299           0 :                               YYYY, MM, DD, h, m, RC )
         300           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         301           0 :         CALL HCO_ERROR( 'ERROR 3', RC, THISLOC=LOC )
         302           0 :         RETURN
         303             :     ENDIF
         304             :
         305             :     ! Write datetime
         306           0 :     WRITE( Yrs, '(i4.4)' ) YYYY
         307           0 :     WRITE( Mts, '(i2.2)' ) MM
         308           0 :     WRITE( Dys, '(i2.2)' ) DD
         309           0 :     WRITE( hrs, '(i2.2)' ) h
         310           0 :     WRITE( mns, '(i2.2)' ) m
         311             :
         312             :     ! Get prefix
         313           0 :     IF ( PRESENT(PREFIX) ) THEN
         314           0 :        Pfx = PREFIX
         315             :     ELSE
         316           0 :        CALL DiagnCollection_Get( HcoState%Diagn, PS, PREFIX=Pfx, RC=RC )
         317           0 :        IF ( RC /= HCO_SUCCESS ) THEN
         318           0 :            CALL HCO_ERROR( 'ERROR 4', RC, THISLOC=LOC )
         319           0 :            RETURN
         320             :        ENDIF
         321             :     ENDIF
         322           0 :     ncFile = TRIM(Pfx)//'.'//Yrs//Mts//Dys//hrs//mns//'.nc'
         323             :
         324             :     ! Place HEMCO restart files in the Restarts folder of the run directory
         325           0 :     IF ( PS == HcoState%Diagn%HcoDiagnIDRestart ) THEN
         326           0 :        ncFile = 'Restarts/' // TRIM( ncFile )
         327             :     ENDIF
         328             :
         329             :     ! Multiple time slice update. Comment out for now since it causes
         330             :     ! timestamping the filename twice (ewl, 10/19/18)
         331             :     ! Add default time stamp if no time tokens are in the file template.
         332             :     ! This also ensures backward compatibility.
         333             :     !IF ( INDEX(TRIM(ncFile),'$') <= 0 ) THEN
         334             :     !   ncFile = TRIM(ncFile)//'.$YYYY$MM$DD$HH$MN.nc'
         335             :     !ENDIF
         336             :     !CALL HCO_CharParse ( HcoState%Config, ncFile, YYYY, MM, DD, h, m, RC )
         337             :     !IF ( RC /= HCO_SUCCESS ) RETURN
         338             :
         339             :     ! Use filename prefix for title, replacing '_' with spaces
         340             :     ! NOTE: Prefix can only contain up to two underscores
         341           0 :     indexL = SCAN( Pfx, '_', .FALSE. ) ! Return left-most position
         342           0 :     indexR = SCAN( Pfx, '_', .TRUE.  ) ! Return right-most position
         343           0 :     IF ( indexL > 0 .AND. indexR > 0 ) THEN
         344             :        title = Pfx(1:indexL-1)        // ' ' //  &
         345             :                Pfx(indexL+1:indexR-1) // ' ' //  &
         346           0 :                Pfx(indexR+1:)
         347           0 :     ELSE IF ( indexL > 0 .AND. indexR == 0 ) THEN
         348           0 :        title = Pfx(1:indexL-1) // ' ' // Pfx(indexL+1:)
         349             :     ELSE
         350           0 :        title = Pfx
         351             :     ENDIF
         352             :
         353             :     ! verbose
         354           0 :     IF ( HCO_IsVerb( HcoState%Config%Err ) .AND. PS==1 ) THEN
         355           0 :        MSG = 'Write diagnostics into file '//TRIM(ncFile)
         356           0 :        CALL HCO_MSG( HcoState%Config%Err, MSG )
         357             :     ENDIF
         358           0 :     IF ( HCO_IsVerb( HcoState%Config%Err ) .AND. PS==1 ) THEN
         359           0 :        WRITE(MSG,*) '--> write level dimension: ', .NOT.NoLevDim
         360           0 :        CALL HCO_MSG( HcoState%Config%Err, MSG )
         361             :     ENDIF
         362             :
         363             :     ! Check if file already exists. If so, add new diagnostics to this file
         364             :     ! (instead of creating a new one)
         365           0 :     INQUIRE( FILE=ncFile, EXIST=IsOldFile )
         366             :
         367             :     ! Disable multiple time slice update since causes an issue writing
         368             :     ! restart files. Re-enable when restart files are written via HISTORY
         369             :     ! rather than HEMCO by deleting the forcing of IsOldFile below.
         370             :     ! (ewl, 10/19/18)
         371           0 :     IsOldFile = .FALSE.
         372             :
         373             :     ! If file exists, open file and get time dimension
         374             :     IF ( IsOldFile ) THEN
         375             :        CALL Ncop_Wr( fID, ncFile )
         376             :        CALL NC_READ_TIME( fID, ntime, timeunit, timeVec, RC=RC )
         377             :
         378             :        ! new file will have one more time dimension
         379             :        ntime = ntime + 1
         380             :
         381             :     ! Create output file
         382             :     ELSE
         383             :
         384             :        ! Define a variable for the number of levels, which will either be -1
         385             :        ! (if all 2D data) or the number of levels in the grid (for 3D data).
         386           0 :        IF ( NoLevDim ) THEN
         387           0 :           nLevTmp = -1
         388             :        ELSE
         389           0 :           nLevTmp = nLev
         390             :        ENDIF
         391             :
         392             :        ! Define extra metadata for global attributes
         393           0 :        Reference = 'http://wiki.geos-chem.org/The_HEMCO_Users_Guide'
         394           0 :        Contact   = 'GEOS-Chem Support Team (geos-chem-support@as.harvard.edu)'
         395             :
         396             :        ! Create output file
         397             :        ! Pass CREATE_NC4 to make file format netCDF-4 (mps, 3/3/16)
         398             :        ! Now create netCDF file with time dimension as UNLIMITED (bmy, 3/8/17)
         399             :        CALL NC_Create( NcFile       = NcFile,                            &
         400             :                        Title        = Title,                             &
         401             :                        Reference    = Reference,                         &
         402             :                        Contact      = Contact,                           &
         403             :                        nLon         = nLon,                              &
         404             :                        nLat         = nLat,                              &
         405             :                        nLev         = nLevTmp,                           &
         406             :                        nTime        = NF_UNLIMITED,                      &
         407             :                        fId          = fId,                               &
         408             :                        lonId        = lonId,                             &
         409             :                        latId        = latId,                             &
         410             :                        levId        = levId,                             &
         411             :                        timeId       = timeId,                            &
         412             :                        VarCt        = VarCt,                             &
         413           0 :                        CREATE_NC4   =.TRUE.                             )
         414             :
         415             :     ENDIF
         416             :
         417             :     !-----------------------------------------------------------------
         418             :     ! Write grid dimensions (incl. time)
         419             :     !-----------------------------------------------------------------
         420           0 :     IF ( .NOT. IsOldFile ) THEN
         421             :
         422             :        ! Write longitude axis variable ("lon") to file
         423             :        CALL NC_Var_Def( fId         = fId,                                &
         424             :                         lonId       = lonId,                              &
         425             :                         latId       = -1,                                 &
         426             :                         levId       = -1,                                 &
         427             :                         timeId      = -1,                                 &
         428             :                         VarName     = 'lon',                              &
         429             :                         VarLongName = 'Longitude',                        &
         430             :                         VarUnit     = 'degrees_east',                     &
         431             :                         Axis        = 'X',                                &
         432             :                         DataType    = dp,                                 &
         433             :                         VarCt       = VarCt,                              &
         434           0 :                         Compress    = .TRUE.                             )
         435           0 :        ALLOCATE( Arr1D( nLon ) )
         436           0 :        Arr1D = HcoState%Grid%XMID%Val(:,1)
         437           0 :        CALL NC_Var_Write( fId, 'lon', Arr1D=Arr1D )
         438           0 :        DEALLOCATE( Arr1D )
         439             :
         440             :        ! Write latitude axis variable ("lat") to file
         441             :        CALL NC_Var_Def( fId         = fId,                              &
         442             :                         lonId       = -1,                               &
         443             :                         latId       = latId,                            &
         444             :                         levId       = -1,                               &
         445             :                         timeId      = -1,                               &
         446             :                         VarName     = 'lat',                            &
         447             :                         VarLongName = 'Latitude',                       &
         448             :                         VarUnit     = 'degrees_north',                  &
         449             :                         Axis        = 'Y',                              &
         450             :                         DataType    = dp,                               &
         451             :                         VarCt       = VarCt,                            &
         452           0 :                         Compress    = .TRUE.                           )
         453           0 :        ALLOCATE( Arr1D( nLat ) )
         454           0 :        Arr1D = HcoState%Grid%YMID%Val(1,:)
         455           0 :        CALL NC_Var_Write( fId, 'lat', Arr1D=Arr1D )
         456           0 :        DEALLOCATE( Arr1D )
         457             :
         458             :        ! Write vertical grid parameters to file (if necessary)
         459           0 :        IF ( .NOT. NoLevDim ) THEN
         460             :
         461             :           ! Reference pressure [Pa]
         462           0 :           P0 = 1.0e+05_dp
         463             :
         464             :           ! Allocate vertical coordinate arrays
         465           0 :           ALLOCATE( Arr1D( nLev ) )
         466           0 :           ALLOCATE( hyam ( nLev ) )
         467           0 :           ALLOCATE( hybm ( nLev ) )
         468             :
         469             :           ! Construct vertical level coordinates
         470           0 :           DO L = 1, nLev
         471             :
         472             :              ! A parameter at grid midpoints
         473           0 :              hyam(L)  = ( HcoState%Grid%zGrid%Ap(L)                         &
         474           0 :                       +   HcoState%Grid%zGrid%Ap(L+1) ) * 0.5_dp
         475             :
         476             :              ! B parameter at grid midpoints
         477           0 :              hybm(L)  = ( HcoState%Grid%zGrid%Bp(L)                         &
         478           0 :                       +   HcoState%Grid%zGrid%Bp(L+1) ) * 0.5_dp
         479             :
         480             :              ! Vertical level coordinate
         481           0 :              Arr1d(L) = ( hyam(L) / P0 ) + hybm(L)
         482             :
         483             :           ENDDO
         484             :
         485             :           ! Write level axis variable ("lev") to file
         486             :           ! Define extra metadata for calls to NC_Var_Def
         487           0 :           myLName = 'hybrid level at midpoints ((A/P0)+B)'
         488           0 :           mySName = 'atmosphere_hybrid_sigma_pressure_coordinate'
         489           0 :           myFTerm = 'a: hyai b: hybi p0: P0 ps: PS'
         490             :           CALL NC_Var_Def( fId          = fId,                            &
         491             :                            lonId        = -1,                             &
         492             :                            latId        = -1,                             &
         493             :                            levId        = levId,                          &
         494             :                            timeId       = -1,                             &
         495             :                            VarName      = 'lev',                          &
         496             :                            VarLongName  = MyLName,                        &
         497             :                            StandardName = MySName,                        &
         498             :                            FormulaTerms = myFTerm,                        &
         499             :                            VarUnit      = 'level',                        &
         500             :                            Axis         = 'Z',                            &
         501             :                            Positive     = 'up',                           &
         502             :                            DataType     = dp,                             &
         503             :                            VarCt        = VarCt,                          &
         504           0 :                            Compress     = .TRUE.                         )
         505           0 :           CALL NC_Var_Write( fId, 'lev', Arr1D=Arr1D )
         506             :
         507             :           ! Write hybrid A coordinate ("hyam") to file
         508             :           ! Define extra metadata for calls to NC_Var_Def
         509           0 :           myLName = 'hybrid A coefficient at layer midpoints'
         510             :           CALL NC_Var_Def( fId          = fId,                            &
         511             :                            lonId        = -1,                             &
         512             :                            latId        = -1,                             &
         513             :                            levId        = levId,                          &
         514             :                            timeId       = -1,                             &
         515             :                            VarName      = 'hyam',                         &
         516             :                            VarLongName  = MyLName,                        &
         517             :                            VarUnit      = 'Pa',                           &
         518             :                            DataType     = dp,                             &
         519             :                            VarCt        = VarCt,                          &
         520           0 :                            Compress     = .TRUE.                         )
         521           0 :           CALL NC_Var_Write ( fId, 'hyam', Arr1D=hyam )
         522             :
         523             :           ! Write hybrid B coordinate ("hybm") to file
         524             :           ! Define extra metadata for calls to NC_Var_Def
         525           0 :           myLName = 'hybrid B coefficient at layer midpoints'
         526             :           CALL NC_Var_Def( fId          = fId,                           &
         527             :                            lonId        = -1,                            &
         528             :                            latId        = -1,                            &
         529             :                            levId        = levId,                         &
         530             :                            timeId       = -1,                            &
         531             :                            VarName      = 'hybm',                        &
         532             :                            VarLongName  = MyLName,                       &
         533             :                            VarUnit      = '1',                           &
         534             :                            DataType     = dp,                            &
         535             :                            VarCt        = VarCt,                         &
         536           0 :                            Compress     = .TRUE.                        )
         537           0 :           CALL NC_Var_Write( fId, 'hybm', Arr1D=hybm )
         538             :
         539             :           ! Write out reference pressure (P0) to file
         540             :           CALL NC_Var_Def( fId         = fId,                             &
         541             :                            lonId       = -1,                              &
         542             :                            latId       = -1,                              &
         543             :                            levId       = -1,                              &
         544             :                            timeId      = -1,                              &
         545             :                            VarName     = 'P0',                            &
         546             :                            VarLongName = 'Reference pressure',            &
         547             :                            VarUnit     = 'Pa',                            &
         548             :                            DataType    = dp,                              &
         549             :                            VarCt       = VarCt,                           &
         550           0 :                            Compress    = .FALSE.                         )
         551           0 :           CALL NC_Var_Write( fId, 'P0', P0 )
         552             :
         553             :           ! Deallocate arrays
         554           0 :           DEALLOCATE( Arr1d )
         555           0 :           DEALLOCATE( hyam  )
         556           0 :           DEALLOCATE( hybm  )
         557             :
         558             :        ENDIF
         559             :     ENDIF
         560             :
         561             :     !------------------------------------------------------------------------
         562             :     ! Write time axis variable ("time") to file
         563             :     !------------------------------------------------------------------------
         564             :
         565             :     ! JD1 is the julian day of the data slice
         566           0 :     GMT     = REAL(h,dp) + (REAL(m,dp)/60.0_dp) + (REAL(s,dp)/3600.0_dp)
         567           0 :     THISDAY = DD + ( GMT / 24.0_dp )
         568           0 :     JD1     = JULDAY ( YYYY, MM, THISDAY )
         569             :
         570             :     ! Check if reference time is given in HEMCO configuration file
         571             :     CALL GetExtOpt ( HcoState%Config, CoreNr, 'DiagnRefTime', &
         572           0 :                      OptValChar=RefTime, Found=Found, RC=RC )
         573           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         574           0 :         CALL HCO_ERROR( 'ERROR 5', RC, THISLOC=LOC )
         575           0 :         RETURN
         576             :     ENDIF
         577             :
         578             :     ! Use specified reference time (if available)
         579           0 :     IF ( Found ) THEN
         580           0 :        timeunit = ADJUSTL(TRIM(RefTime))
         581           0 :        CALL TRANLC( timeunit )
         582             :        CALL NC_GET_REFDATETIME( timeunit, refYYYY, refMM, refDD, refh, &
         583           0 :                                 refm, refs, RC )
         584           0 :        refs = 0
         585           0 :        IF ( RC /= HCO_SUCCESS ) THEN
         586           0 :            CALL HCO_ERROR( 'ERROR 6', RC, THISLOC=LOC )
         587           0 :            RETURN
         588             :        ENDIF
         589             :        GMT      = REAL(MAX(refh,0),dp) + (REAL(MAX(refm,0),dp)/60.0_dp) + &
         590           0 :                   (REAL(MAX(refs,0),dp)/3600.0_dp)
         591           0 :        THISDAY  = refDD + ( GMT / 24.0_dp )
         592           0 :        JD1985   = JULDAY ( refYYYY, refMM, THISDAY )
         593             :
         594             :     ! Use current time if not found
         595             :     ELSE
         596           0 :        WRITE(timeunit,100) YYYY,MM,DD,h,m,s
         597           0 :        JD1985 = JD1
         598             :     ENDIF
         599             : 100 FORMAT ( 'hours since ',i4.4,'-',i2.2,'-',i2.2,' ',i2.2,':',i2.2,':',i2.2,' GMT' )
         600             :
         601             :     ! Calculate time value
         602           0 :     JD_DELTA = (JD1 - JD1985 )
         603             :
         604             :     ! Default is 'days since'. Adjust for 'hours since', 'minutes since',
         605             :     ! 'seconds since'.
         606           0 :     IF ( timeunit(1:4) == 'days' ) THEN
         607             :        ! all ok
         608           0 :     ELSEIF ( timeunit(1:5) == 'hours' ) THEN
         609           0 :        JD_DELTA = JD_DELTA * 24.0_dp
         610           0 :     ELSEIF ( timeunit(1:7) == 'minutes' ) THEN
         611           0 :        JD_DELTA = JD_DELTA * 24.0_dp * 60.0_dp
         612           0 :     ELSEIF ( timeunit(1:7) == 'seconds' ) THEN
         613           0 :        JD_DELTA = JD_DELTA * 24.0_dp * 3600.0_dp
         614             :     ELSE
         615             :        MSG = 'Unrecognized output reference time, will ' // &
         616           0 :              'assume `days since`: '//TRIM(timeunit)
         617           0 :        CALL HCO_WARNING( HcoState%Config%Err, MSG, RC, THISLOC=LOC )
         618             :     ENDIF
         619             :
         620             :     ! Special case where we have an old file but it has the same time stamp: in
         621             :     ! that case simply overwrite the current values
         622             :     ! Comment out code for single precision rounded time (ewl, 10/18/18)
         623             :     !IF ( IsOldFile .AND. ntime == 2 .AND. timeVec(1) == JD_DELTA_RND ) THEN
         624           0 :     IF ( IsOldFile .AND. ntime == 2 ) THEN
         625           0 :        IF ( timeVec(1) == JD_DELTA ) THEN
         626           0 :           ntime = 1
         627             :        ENDIF
         628             :     ENDIF
         629           0 :     ALLOCATE( nctime(ntime) )
         630           0 :     IF ( IsOldFile .AND. ntime > 1 ) THEN
         631           0 :        nctime(1:ntime-1) = timeVec(:)
         632             :     ENDIF
         633           0 :     nctime(ntime) = JD_DELTA
         634             :
         635           0 :     IF ( .NOT. IsOldFile ) THEN
         636             :        CALL NC_Var_Def( fId         = fId,                                &
         637             :                         lonId       = -1,                                 &
         638             :                         latId       = -1,                                 &
         639             :                         levId       = -1,                                 &
         640             :                         timeId      = timeId,                             &
         641             :                         VarName     = 'time',                             &
         642             :                         VarLongName = 'Time',                             &
         643             :                         VarUnit     = TimeUnit,                           &
         644             :                         Axis        = 'T',                                &
         645             :                         Calendar    = 'gregorian',                        &
         646             :                         DataType    = 8,                                  &
         647             :                         VarCt       = VarCt,                              &
         648           0 :                         Compress    = .TRUE.                             )
         649             :     ENDIF
         650           0 :     CALL NC_VAR_WRITE( fId, 'time', Arr1D=nctime )
         651           0 :     DEALLOCATE( nctime )
         652           0 :     IF ( ASSOCIATED(timeVec) ) DEALLOCATE( timeVec )
         653             :
         654             :     !-----------------------------------------------------------------
         655             :     ! Write out grid box areas
         656             :     !-----------------------------------------------------------------
         657             :
         658           0 :     IF ( .NOT. IsOldFile ) THEN
         659             :        CALL NC_Var_Def( fId         = fId,                                &
         660             :                         lonId       = lonId,                              &
         661             :                         latId       = latId,                              &
         662             :                         levId       = -1,                                 &
         663             :                         timeId      = -1,                                 &
         664             :                         VarName     = 'AREA',                             &
         665             :                         VarLongName = 'Grid box area',                    &
         666             :                         VarUnit     = 'm2',                               &
         667             :                         DataType    = Prc,                                &
         668             :                         VarCt       = VarCt,                              &
         669           0 :                         Compress    = .TRUE.                             )
         670           0 :        CALL NC_Var_Write ( fId, 'AREA', Arr2D=HcoState%Grid%Area_M2%Val )
         671             :     ENDIF
         672             :
         673             :     !-----------------------------------------------------------------
         674             :     ! Write diagnostics
         675             :     !-----------------------------------------------------------------
         676             :
         677             :     ! Run this section twice, first in define mode for metadata, then in
         678             :     ! data mode to write variables
         679           0 :     DO I=1,2
         680             :
         681             :     ! Skip definition mode for existing file
         682           0 :     IF ( I==1 .AND. IsOldFile ) CYCLE
         683             :
         684           0 :     IF (I==1) THEN
         685             :        ! Open netCDF define mode
         686           0 :        CALL NcBegin_Def( fID )
         687           0 :        DefMode=.TRUE.
         688             :     ELSE
         689             : !       IF ( .NOT. IsOldFile ) THEN
         690             :           ! Close netCDF define mode
         691           0 :           CALL NcEnd_Def( fID )
         692             : !       ENDIF
         693           0 :        DefMode=.False.
         694             :     ENDIF
         695             :
         696             :     ! Loop over all diagnostics in diagnostics list
         697           0 :     ThisDiagn => NULL()
         698           0 :     DO WHILE ( .TRUE. )
         699             :
         700             :        ! Get next diagnostics in list. This will return the next
         701             :        ! diagnostics container that contains content.
         702           0 :        CALL Diagn_Get ( HcoState, EOI, ThisDiagn, FLAG, RC, COL=PS )
         703           0 :        IF ( RC /= HCO_SUCCESS ) THEN
         704           0 :            CALL HCO_ERROR( 'ERROR 7', RC, THISLOC=LOC )
         705           0 :            RETURN
         706             :        ENDIF
         707           0 :        IF ( FLAG /= HCO_SUCCESS ) EXIT
         708             :
         709             :        ! Only write diagnostics if this is the first Diagn_Get call for
         710             :        ! this container and time step.
         711           0 :        IF ( PRESENT( OnlyIfFirst ) ) THEN
         712           0 :           IF ( OnlyIfFirst .AND. ThisDiagn%nnGetCalls > 1 ) CYCLE
         713             :        ENDIF
         714             :
         715             :        ! Define variable
         716           0 :        myName = ThisDiagn%cName
         717           0 :        myUnit = ThisDiagn%OutUnit
         718           0 :        IF ( ThisDiagn%SpaceDim == 3 ) THEN
         719           0 :           levIdTmp = levId
         720             :        ELSE
         721           0 :           levIdTmp = -1
         722             :        ENDIF
         723             :
         724             :        ! Error check: this should never happen!
         725           0 :        IF ( levIdTmp > 0 .AND. NoLevDim ) THEN
         726             :           MSG = 'Level dimension undefined but 3D container found: ' &
         727           0 :                 // TRIM(myName)
         728           0 :           CALL HCO_ERROR(MSG,RC,THISLOC=LOC)
         729           0 :           RETURN
         730             :        ENDIF
         731             :
         732           0 :        IF (DefMode) THEN
         733             :
         734             :           !------------------------------------
         735             :           ! Define variables in define mode
         736             :           !------------------------------------
         737             :
         738             :           ! Define variable as single precision
         739             :           CALL NC_Var_Def( fId          = fId,                               &
         740             :                            lonId        = lonId,                             &
         741             :                            latId        = latId,                             &
         742             :                            levId        = levIdTmp,                          &
         743             :                            timeId       = timeId,                            &
         744             :                            VarName      = TRIM(myName),                      &
         745             :                            VarLongName  = ThisDiagn%long_name,               &
         746             :                            VarUnit      = TRIM(myUnit),                      &
         747             :                            AvgMethod    = ThisDiagn%AvgName,                 &
         748             :                            MissingValue = FillValue,                         &
         749             :                            DataType     = sp,                                &
         750             :                            VarCt        = VarCt,                             &
         751             :                            DefMode      = DefMode,                           &
         752           0 :                            Compress     = .True.                            )
         753             :
         754             :        ELSE
         755             :
         756             :           !------------------------------------
         757             :           ! Write variables in data mode
         758             :           !------------------------------------
         759             :
         760           0 :           IF ( IsOldFile .AND. ntime > 1 ) THEN
         761           0 :              IF ( ThisDiagn%SpaceDim == 3 ) THEN
         762             :                 CALL NC_READ_ARR( fID, TRIM(myName), 1, nlon, 1, nlat, &
         763           0 :                                   1, nlev, 1, ntime-1, ncArr=Arr4DOld, RC=RC )
         764           0 :                 Arr4D(:,:,:,1:ntime-1) = Arr4DOld(:,:,:,:)
         765             :              ELSE
         766             :                 CALL NC_READ_ARR( fID, TRIM(myName), 1, nlon, 1, nlat, &
         767           0 :                                   -1, -1, 1, ntime-1, ncArr=Arr4DOld, RC=RC )
         768           0 :                 Arr3D(:,:,1:ntime-1) = Arr4DOld(:,:,1,:)
         769             :              ENDIF
         770           0 :              IF ( ASSOCIATED(Arr4DOld) ) DEALLOCATE(Arr4DOld)
         771             :           ENDIF
         772             :
         773             :           ! Mirror data and write to file. The mirroring is required in
         774             :           ! order to add the time dimension. Otherwise, the data would
         775             :           ! have no time information!
         776           0 :           IF ( ThisDiagn%SpaceDim == 3 ) THEN
         777           0 :              IF ( ASSOCIATED(ThisDiagn%Arr3D) ) THEN
         778           0 :                 Arr4D(:,:,:,ntime) = ThisDiagn%Arr3D%Val
         779           0 :                 Arr4D(:,:,:,1) = ThisDiagn%Arr3D%Val
         780             :              ENDIF
         781           0 :              CALL NC_VAR_WRITE ( fId, TRIM(myName), Arr4D=Arr4D )
         782             :           ELSE
         783           0 :              IF ( ASSOCIATED(ThisDiagn%Arr2D) ) THEN
         784           0 :                 Arr3D(:,:,ntime) = ThisDiagn%Arr2D%Val
         785           0 :                 Arr3D(:,:,1) = ThisDiagn%Arr2D%Val
         786             :              ENDIF
         787           0 :              CALL NC_VAR_WRITE ( fId, TRIM(myName), Arr3D=Arr3D )
         788             :           ENDIF
         789             :
         790             :           ! verbose
         791           0 :           IF ( HCO_IsVerb(HcoState%Config%Err ) .AND. PS==1 ) THEN
         792           0 :              MSG = '--- Added diagnostics: '//TRIM(myName)
         793           0 :              CALL HCO_MSG(HcoState%Config%Err,MSG)
         794             :           ENDIF
         795             :        ENDIF
         796             :     ENDDO
         797             :     ENDDO
         798             :
         799             :     !-----------------------------------------------------------------
         800             :     ! Cleanup
         801             :     !-----------------------------------------------------------------
         802             :
         803             :     ! Close file
         804           0 :     CALL NC_CLOSE ( fId )
         805             :
         806             :     ! Cleanup local variables
         807           0 :     Deallocate(Arr3D,Arr4D)
         808           0 :     ThisDiagn => NULL()
         809             :
         810             :     ! Archive time stamp
         811             :     CALL DiagnCollection_Set ( HcoState%Diagn, COL=PS, &
         812           0 :                                LastYMD=lymd, LastHMS=lhms, RC=RC )
         813             :
         814             :     ! Return
         815           0 :     RC = HCO_SUCCESS
         816             :
         817           0 :   END SUBROUTINE HCOIO_Write
         818             : !EOC
         819             : !------------------------------------------------------------------------------
         820             : !                   Harmonized Emissions Component (HEMCO)                    !
         821             : !------------------------------------------------------------------------------
         822             : !BOP
         823             : !
         824             : ! !IROUTINE: ConstructTimeStamp
         825             : !
         826             : ! !DESCRIPTION: Subroutine ConstructTimeStamp is a helper routine to construct
         827             : ! the time stamp of a given diagnostics collection.
         828             : !\\
         829             : !\\
         830             : ! !INTERFACE:
         831             : !
         832           0 :   SUBROUTINE ConstructTimeStamp ( HcoState, PS, PrevTime, Yr, Mt, Dy, hr, mn, RC )
         833             : !
         834             : ! !USES:
         835             : !
         836             :     USE HCO_State_Mod,       ONLY : HCO_State
         837             :     USE HCO_Clock_Mod
         838             :     USE HCO_JULDAY_MOD
         839             : !
         840             : ! !INPUT/OUTPUT PARAMETERS:
         841             : !
         842             :     TYPE(HCO_State), POINTER          :: HcoState     ! HEMCO state obj
         843             :     INTEGER,         INTENT(IN   )    :: PS           ! collecion ID
         844             :     LOGICAL,         INTENT(IN   )    :: PrevTime     ! Use previous time?
         845             : !
         846             : ! !INPUT/OUTPUT PARAMETERS:
         847             : !
         848             :     INTEGER,         INTENT(INOUT)    :: RC           ! Return code
         849             : !
         850             : ! !OUTPUT PARAMETERS:
         851             : !
         852             :     INTEGER,         INTENT(  OUT)    :: Yr
         853             :     INTEGER,         INTENT(  OUT)    :: Mt
         854             :     INTEGER,         INTENT(  OUT)    :: Dy
         855             :     INTEGER,         INTENT(  OUT)    :: hr
         856             :     INTEGER,         INTENT(  OUT)    :: mn
         857             : !
         858             : ! !REVISION HISTORY:
         859             : !  06 Nov 2015 - C. Keller   - Initial version
         860             : !  See https://github.com/geoschem/hemco for complete history
         861             : !EOP
         862             : !------------------------------------------------------------------------------
         863             : !BOC
         864             : !
         865             : ! !LOCAL VARIABLES:
         866             : !
         867             :     INTEGER            :: Y2, M2, D2, h2, n2, s2
         868             :     INTEGER            :: Y1, M1, D1, h1, n1, s1
         869             :     INTEGER            :: LastYMD, LastHMS
         870             :     INTEGER            :: YYYYMMDD, HHMMSS
         871             :     INTEGER            :: OutTimeStamp
         872             :     REAL(dp)           :: DAY, UTC, JD1, JD2, JDMID
         873             :     CHARACTER(LEN=255) :: MSG
         874             :     CHARACTER(LEN=255) :: LOC = 'ConstuctTimeStamp (hcoi_diagn_mod.F90)'
         875             :
         876             :     !=================================================================
         877             :     ! ConstructTimeStamp begins here!
         878             :     !=================================================================
         879             :
         880             :     ! Use HEMCO clock to create timestamp used in filename. Use previous
         881             :     ! time step if this option is selected.
         882           0 :     IF ( .NOT. PrevTime ) THEN
         883             :        CALL HcoClock_Get(HcoState%Clock,sYYYY=Y2,sMM=M2,&
         884           0 :                          sDD=D2,sH=h2,sM=n2,sS=s2,RC=RC)
         885           0 :        IF ( RC /= HCO_SUCCESS ) THEN
         886           0 :            CALL HCO_ERROR( 'ERROR 8', RC, THISLOC=LOC )
         887           0 :            RETURN
         888             :        ENDIF
         889             :     ELSE
         890             :        CALL HcoClock_Get(HcoState%Clock,pYYYY=Y2,pMM=M2,&
         891           0 :                          pDD=D2,pH=h2,pM=n2,pS=s2,RC=RC)
         892           0 :        IF ( RC /= HCO_SUCCESS ) THEN
         893           0 :            CALL HCO_ERROR( 'ERROR 9', RC, THISLOC=LOC )
         894           0 :            RETURN
         895             :        ENDIF
         896             :     ENDIF
         897             :
         898             :     ! Get timestamp location for this collection
         899             :     CALL DiagnCollection_Get( HcoState%Diagn, PS, OutTimeStamp=OutTimeStamp, &
         900           0 :                               LastYMD=LastYMD, LastHMS=LastHMS, RC=RC )
         901           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         902           0 :         CALL HCO_ERROR( 'ERROR 10', RC, THISLOC=LOC )
         903           0 :         RETURN
         904             :     ENDIF
         905             :
         906             :     ! Determine dates to be used:
         907             :
         908             :     ! To use start date
         909           0 :     IF ( OutTimeStamp == HcoDiagnStart ) THEN
         910           0 :        Yr = FLOOR( MOD(LastYMD*1.d0, 100000000.d0 ) / 1.0d4 )
         911           0 :        Mt = FLOOR( MOD(LastYMD*1.d0, 10000.d0     ) / 1.0d2 )
         912           0 :        Dy = FLOOR( MOD(LastYMD*1.d0, 100.d0       ) / 1.0d0 )
         913           0 :        Hr = FLOOR( MOD(LastHMS*1.d0, 1000000.d0   ) / 1.0d4 )
         914           0 :        Mn = FLOOR( MOD(LastHMS*1.d0, 10000.d0     ) / 1.0d2 )
         915             :
         916             :     ! Use mid point
         917           0 :     ELSEIF ( OutTimeStamp == HcoDiagnMid ) THEN
         918             :
         919             :        ! Julian day of start interval:
         920           0 :        Y1 = FLOOR( MOD(LastYMD*1.d0, 100000000.d0 ) / 1.0d4 )
         921           0 :        M1 = FLOOR( MOD(LastYMD*1.d0, 10000.d0     ) / 1.0d2 )
         922           0 :        D1 = FLOOR( MOD(LastYMD*1.d0, 100.d0       ) / 1.0d0 )
         923           0 :        h1 = FLOOR( MOD(LastHMS*1.d0, 1000000.d0   ) / 1.0d4 )
         924           0 :        n1 = FLOOR( MOD(LastHMS*1.d0, 10000.d0     ) / 1.0d2 )
         925           0 :        s1 = FLOOR( MOD(LastHMS*1.d0, 100.d0       ) / 1.0d0 )
         926             :
         927             :        UTC = ( REAL(h1,dp) / 24.0_dp    ) + &
         928             :              ( REAL(n1,dp) / 1440.0_dp  ) + &
         929           0 :              ( REAL(s1,dp) / 86400.0_dp )
         930           0 :        DAY = REAL(D1,dp) + UTC
         931           0 :        JD1 = JULDAY( Y1, M1, DAY )
         932             :
         933             :        ! Julian day of end interval:
         934             :        UTC = ( REAL(h2,dp) / 24.0_dp    ) + &
         935             :              ( REAL(n2,dp) / 1440.0_dp  ) + &
         936           0 :              ( REAL(s2,dp) / 86400.0_dp )
         937           0 :        DAY = REAL(D2,dp) + UTC
         938           0 :        JD2 = JULDAY( Y2, M2, DAY )
         939             :
         940             :        ! Julian day in the middle
         941           0 :        JDMID = ( JD1 + JD2 ) / 2.0_dp
         942             :
         943             :        ! Tranlate back into dates
         944           0 :        CALL CALDATE( JDMID, YYYYMMDD, HHMMSS )
         945           0 :        Yr = FLOOR ( MOD( YYYYMMDD, 100000000) / 1.0e4_dp )
         946           0 :        Mt = FLOOR ( MOD( YYYYMMDD, 10000    ) / 1.0e2_dp )
         947           0 :        Dy = FLOOR ( MOD( YYYYMMDD, 100      ) / 1.0e0_dp )
         948           0 :        Hr = FLOOR ( MOD(   HHMMSS, 1000000  ) / 1.0e4_dp )
         949           0 :        Mn = FLOOR ( MOD(   HHMMSS, 10000    ) / 1.0e2_dp )
         950             :
         951             :     ! Otherwise, use end date
         952             :     ELSE
         953           0 :        Yr = Y2
         954           0 :        Mt = M2
         955           0 :        Dy = D2
         956           0 :        Hr = h2
         957           0 :        Mn = n2
         958             :     ENDIF
         959             :
         960             :     ! Return w/ success
         961           0 :     RC = HCO_SUCCESS
         962             :
         963             :   END SUBROUTINE ConstructTimeStamp
         964             : !EOC
         965             : END MODULE HCOIO_WRITE_MOD
         966             : #endif

Generated by: LCOV version 1.14