LCOV - code coverage report
Current view: | top level - physics/clubb/src/CLUBB_core - parameters_model.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 5 | 5 | 100.0 %
Date: | 2024-12-17 22:39:59 |  | Functions: | 1 | 1 | 100.0 %

              Line data    Source code
           1             : !-------------------------------------------------------------------------------
           2             : ! $Id$
           3             : !===============================================================================
           4             : module parameters_model
           5             :
           6             : ! Description:
           7             : !   Contains model parameters that are determined at run time rather than
           8             : !   compile time.
           9             : !
          10             : ! References:
          11             : !   None
          12             : !-------------------------------------------------------------------------------
          13             :
          14             :   use clubb_precision, only: &
          15             :     core_rknd
          16             :
          17             :   implicit none
          18             :
          19             :   private ! Default scope
          20             :
          21             :   ! Maximum magnitude of PDF parameter 'mixt_frac'.
          22             :   real( kind = core_rknd ), public :: &
          23             :     mixt_frac_max_mag
          24             :
          25             :   ! Model parameters and constraints setup in the namelists
          26             :   real( kind = core_rknd ), public ::  &
          27             :     T0       = 300._core_rknd, & ! Reference temperature (usually 300)  [K]
          28             :     ts_nudge = 0._core_rknd      ! Timescale of u/v nudging             [s]
          29             :
          30             :   real( kind = core_rknd), public :: &
          31             :     rtm_min                = epsilon( rtm_min ), & ! Value below which rtm will be nudged [kg/kg]
          32             :     rtm_nudge_max_altitude = 10000._core_rknd      ! Highest altitude at which to nudge rtm [m]
          33             :
          34             :   public :: setup_parameters_model
          35             :
          36             :   contains
          37             :
          38             : !-------------------------------------------------------------------------------
          39        1536 :   subroutine setup_parameters_model ( T0_in, ts_nudge_in, Skw_max_mag )
          40             :
          41             : ! Description:
          42             : !   Sets parameters to their initial values
          43             : !
          44             : ! References:
          45             : !   None
          46             : !-------------------------------------------------------------------------------
          47             :
          48             :     use clubb_precision, only: &
          49             :         core_rknd ! Variable(s)
          50             :
          51             :     implicit none
          52             :
          53             :     !------------------------ Input Variables ------------------------
          54             :     real( kind = core_rknd ), intent(in) ::  &
          55             :       T0_in,       & ! Ref. temperature                         [K]
          56             :       ts_nudge_in, & ! Timescale for u/v nudging                [s]
          57             :       Skw_max_mag    ! Maximum allowable magnitude of Skewness  [-]
          58             :
          59             :     !------------------------ Begin Code ------------------------
          60             :
          61             :     ! Formula from subroutine pdf_closure, where sigma_sqd_w = 0.4 and Skw =
          62             :     ! Skw_max_mag in this formula.  Note that this is constant, but can't appear
          63             :     ! with a Fortran parameter attribute, so we define it here.
          64             :     mixt_frac_max_mag = 1.0_core_rknd &
          65             :       - ( 0.5_core_rknd * ( 1.0_core_rknd - Skw_max_mag / &
          66             :       sqrt( 4.0_core_rknd * ( 1.0_core_rknd - 0.4_core_rknd )**3 &
          67        1536 :       + Skw_max_mag**2 ) ) ) ! Known magic number
          68             :
          69        1536 :     T0       = T0_in
          70        1536 :     ts_nudge = ts_nudge_in
          71             :
          72        1536 :     return
          73             :   end subroutine setup_parameters_model
          74             : !-------------------------------------------------------------------------------
          75             :
          76             : end module parameters_model

Generated by: LCOV version 1.14