LCOV - code coverage report
Current view: | top level - infrastructure - phys_grid.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 200 | 386 | 51.8 %
Date: | 2025-01-13 21:54:50 |  | Functions: | 13 | 31 | 41.9 %

Function Name | Hit count
__phys_grid_MOD___copy_phys_grid_Chunk | 0
__phys_grid_MOD___final_phys_grid_Chunk | 0
__phys_grid_MOD_dyn_decomp_to_phys | 0
__phys_grid_MOD_get_area_all_p | 0
__phys_grid_MOD_get_area_p | 0
__phys_grid_MOD_get_dyn_col_p_chunk | 0
__phys_grid_MOD_get_grid_dims | 0
__phys_grid_MOD_get_lat_all_p_int | 0
__phys_grid_MOD_get_lat_all_p_r8 | 0
__phys_grid_MOD_get_lat_p | 0
__phys_grid_MOD_get_lon_all_p_int | 0
__phys_grid_MOD_get_lon_all_p_r8 | 0
__phys_grid_MOD_get_lon_p | 0
__phys_grid_MOD_get_rlat_p | 0
__phys_grid_MOD_get_rlon_p | 0
__phys_grid_MOD_get_wght_p | 0
__phys_grid_MOD_phys_decomp_to_dyn | 0
__phys_grid_MOD_scatter_field_to_chunk | 0
__phys_grid_MOD_phys_grid_init | 1536
__phys_grid_MOD_phys_grid_readnl | 1536
__phys_grid_MOD_get_gcol_all_p | 6192
__phys_grid_MOD_chunk_info_to_index_p | 194400
__phys_grid_MOD_get_gcol_p | 194400
__phys_grid_MOD_get_nlcols_p | 370944
__phys_grid_MOD_get_rlon_all_p | 6012432
__phys_grid_MOD_get_wght_all_p | 7470648
__phys_grid_MOD_get_chunk_info_p | 46850400
__phys_grid_MOD_get_dyn_col_p_index | 46850400
__phys_grid_MOD_get_rlat_all_p | 83771568
__phys_grid_MOD_get_ncols_p | 139362696
__phys_grid_MOD_phys_grid_initialized | 233268696

Generated by: LCOV version 1.14