LCOV - code coverage report
Current view: | top level - physics/cam - cam_diagnostics.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 791 | 1086 | 72.8 %
Date: | 2025-01-13 21:54:50 |  | Functions: | 27 | 30 | 90.0 %

              Line data    Source code
           1             : module cam_diagnostics
           2             :
           3             : !---------------------------------------------------------------------------------
           4             : ! Module to compute a variety of diagnostics quantities for history files
           5             : !---------------------------------------------------------------------------------
           6             :
           7             : use shr_kind_mod,    only: r8 => shr_kind_r8
           8             : use camsrfexch,      only: cam_in_t, cam_out_t
           9             : use cam_control_mod, only: moist_physics
          10             : use physics_types,   only: physics_state, physics_tend, physics_ptend
          11             : use ppgrid,          only: pcols, pver, begchunk, endchunk
          12             : use physics_buffer,  only: physics_buffer_desc, pbuf_add_field, dtype_r8
          13             : use physics_buffer,  only: dyn_time_lvls, pbuf_get_field, pbuf_get_index, pbuf_old_tim_idx
          14             :
          15             : use cam_history,     only: outfld, write_inithist, hist_fld_active, inithist_all, write_camiop
          16             : use cam_history_support, only: max_fieldname_len
          17             : use constituents,    only: pcnst, cnst_name, cnst_longname, cnst_cam_outfld
          18             : use constituents,    only: ptendnam, apcnst, bpcnst, cnst_get_ind
          19             : use dycore,          only: dycore_is
          20             : use phys_control,    only: phys_getopts
          21             : use wv_saturation,   only: qsat, qsat_water, svp_ice_vect
          22             : use time_manager,    only: is_first_step
          23             :
          24             : use scamMod,         only: single_column, wfld
          25             : use cam_abortutils,  only: endrun
          26             :
          27             : implicit none
          28             : private
          29             : save
          30             :
          31             : ! Public interfaces
          32             :
          33             : public :: &
          34             :    diag_readnl,              &! read namelist options
          35             :    diag_register,            &! register pbuf space
          36             :    diag_init,                &! initialization
          37             :    diag_allocate,            &! allocate memory for module variables
          38             :    diag_deallocate,          &! deallocate memory for module variables
          39             :    diag_conv_tend_ini,       &! initialize convective tendency calcs
          40             :    diag_phys_writeout,       &! output diagnostics of the dynamics
          41             :    diag_clip_tend_writeout,  &! output diagnostics for clipping
          42             :    diag_phys_tend_writeout,  &! output physics tendencies
          43             :    diag_state_b4_phys_write, &! output state before physics execution
          44             :    diag_conv,                &! output diagnostics of convective processes
          45             :    diag_surf,                &! output diagnostics of the surface
          46             :    diag_export,              &! output export state
          47             :    diag_physvar_ic,          &
          48             :    nsurf
          49             :
          50             : integer, public, parameter                                 :: num_stages = 8
          51             : character (len = max_fieldname_len), dimension(num_stages) :: stage = (/"phBF","phBP","phAP","phAM","dyBF","dyBP","dyAP","dyAM"/)
          52             : character (len = 45),dimension(num_stages) :: stage_txt = (/&
          53             :      " before energy fixer                     ",& !phBF - physics energy
          54             :      " before parameterizations                ",& !phBF - physics energy
          55             :      " after parameterizations                 ",& !phAP - physics energy
          56             :      " after dry mass correction               ",& !phAM - physics energy
          57             :      " before energy fixer (dycore)            ",& !dyBF - dynamics energy
          58             :      " before parameterizations (dycore)       ",& !dyBF - dynamics energy
          59             :      " after parameterizations (dycore)        ",& !dyAP - dynamics energy
          60             :      " after dry mass correction (dycore)      " & !dyAM - dynamics energy
          61             :      /)
          62             :
          63             : ! Private data
          64             :
          65             : integer :: dqcond_num                     ! number of constituents to compute convective
          66             : character(len=16) :: dcconnam(pcnst)      ! names of convection tendencies
          67             :                                           ! tendencies for
          68             : real(r8), allocatable :: dtcond(:,:,:)    ! temperature tendency due to convection
          69             : type dqcond_t
          70             :    real(r8), allocatable :: cnst(:,:,:)   ! constituent tendency due to convection
          71             : end type dqcond_t
          72             : type(dqcond_t), allocatable :: dqcond(:)
          73             :
          74             : character(len=8) :: diag_cnst_conv_tend = 'q_only' ! output constituent tendencies due to convection
          75             :                                                    ! 'none', 'q_only' or 'all'
          76             :
          77             : integer, parameter :: surf_100000 = 1
          78             : integer, parameter :: surf_092500 = 2
          79             : integer, parameter :: surf_085000 = 3
          80             : integer, parameter :: surf_070000 = 4
          81             : integer, parameter :: nsurf = 4
          82             :
          83             : logical          :: history_amwg                   ! output the variables used by the AMWG diag package
          84             : logical          :: history_vdiag                  ! output the variables used by the AMWG variability diag package
          85             : logical          :: history_eddy                   ! output the eddy variables
          86             : logical          :: history_budget                 ! output tendencies and state variables for CAM4
          87             :                                                    ! temperature, water vapor, cloud ice and cloud
          88             :                                                    ! liquid budgets.
          89             : integer          :: history_budget_histfile_num    ! output history file number for budget fields
          90             : logical          :: history_waccm                  ! outputs typically used for WACCM
          91             :
          92             : ! Physics buffer indices
          93             :
          94             : integer  ::      psl_idx    = 0
          95             : integer  ::      relhum_idx = 0
          96             : integer  ::      qcwat_idx  = 0
          97             : integer  ::      tcwat_idx  = 0
          98             : integer  ::      lcwat_idx  = 0
          99             : integer  ::      cld_idx    = 0
         100             : integer  ::      concld_idx = 0
         101             : integer  ::      tke_idx    = 0
         102             : integer  ::      kvm_idx    = 0
         103             : integer  ::      kvh_idx    = 0
         104             : integer  ::      cush_idx   = 0
         105             : integer  ::      t_ttend_idx = 0
         106             : integer  ::      t_utend_idx = 0
         107             : integer  ::      t_vtend_idx = 0
         108             :
         109             : integer  ::      prec_dp_idx  = 0
         110             : integer  ::      snow_dp_idx  = 0
         111             : integer  ::      prec_sh_idx  = 0
         112             : integer  ::      snow_sh_idx  = 0
         113             : integer  ::      prec_sed_idx = 0
         114             : integer  ::      snow_sed_idx = 0
         115             : integer  ::      prec_pcw_idx = 0
         116             : integer  ::      snow_pcw_idx = 0
         117             :
         118             :
         119             : integer :: tpert_idx=-1, qpert_idx=-1, pblh_idx=-1
         120             :
         121             : integer :: trefmxav_idx = -1, trefmnav_idx = -1
         122             :
         123             : contains
         124             :
         125             : !==============================================================================
         126             :
         127        1536 :   subroutine diag_readnl(nlfile)
         128             :     use namelist_utils,  only: find_group_name
         129             :     use units,           only: getunit, freeunit
         130             :     use spmd_utils,      only: masterproc, masterprocid, mpi_character, mpicom
         131             :
         132             :     character(len=*), intent(in) :: nlfile  ! filepath for file containing namelist input
         133             :
         134             :     ! Local variables
         135             :     integer :: unitn, ierr
         136             :     character(len=*), parameter :: subname = 'diag_readnl'
         137             :
         138             :     namelist /cam_diag_opts/ diag_cnst_conv_tend
         139             :     !--------------------------------------------------------------------------
         140             :
         141        1536 :     if (masterproc) then
         142           2 :       unitn = getunit()
         143           2 :       open( unitn, file=trim(nlfile), status='old' )
         144           2 :       call find_group_name(unitn, 'cam_diag_opts', status=ierr)
         145           2 :       if (ierr == 0) then
         146           0 :         read(unitn, cam_diag_opts, iostat=ierr)
         147           0 :         if (ierr /= 0) then
         148           0 :           call endrun(subname // ':: ERROR reading namelist')
         149             :         end if
         150             :       end if
         151           2 :       close(unitn)
         152           2 :       call freeunit(unitn)
         153             :     end if
         154             :
         155             :     ! Broadcast namelist variables
         156        1536 :     call mpi_bcast(diag_cnst_conv_tend, len(diag_cnst_conv_tend), mpi_character, masterprocid, mpicom, ierr)
         157             :
         158        1536 :   end subroutine diag_readnl
         159             :
         160             : !==============================================================================
         161             :
         162        1536 :   subroutine diag_register_dry()
         163             :
         164        1536 :     call pbuf_add_field('PSL', 'physpkg', dtype_r8, (/pcols/), psl_idx)
         165             :
         166             :     ! Request physics buffer space for fields that persist across timesteps.
         167        6144 :     call pbuf_add_field('T_TTEND', 'global', dtype_r8, (/pcols,pver,dyn_time_lvls/), t_ttend_idx)
         168        6144 :     call pbuf_add_field('T_UTEND', 'global', dtype_r8, (/pcols,pver,dyn_time_lvls/), t_utend_idx)
         169        6144 :     call pbuf_add_field('T_VTEND', 'global', dtype_r8, (/pcols,pver,dyn_time_lvls/), t_vtend_idx)
         170        1536 :   end subroutine diag_register_dry
         171             :
         172        1536 :   subroutine diag_register_moist()
         173             :     ! Request physics buffer space for fields that persist across timesteps.
         174        1536 :     call pbuf_add_field('TREFMXAV', 'global', dtype_r8, (/pcols/), trefmxav_idx)
         175        1536 :     call pbuf_add_field('TREFMNAV', 'global', dtype_r8, (/pcols/), trefmnav_idx)
         176        1536 :   end subroutine diag_register_moist
         177             :
         178        1536 :   subroutine diag_register()
         179        1536 :     call diag_register_dry()
         180        1536 :     if (moist_physics) then
         181        1536 :       call diag_register_moist()
         182             :     end if
         183        1536 :   end subroutine diag_register
         184             :
         185             : !==============================================================================
         186             :
         187        1536 :   subroutine diag_init_dry(pbuf2d)
         188             :     ! Declare the history fields for which this module contains outfld calls.
         189             :
         190             :     use cam_history,        only: addfld, add_default, horiz_only
         191             :     use cam_history,        only: register_vector_field
         192             :     use tidal_diag,         only: tidal_diag_init
         193             :     use cam_budget,         only: cam_budget_em_snapshot, cam_budget_em_register, thermo_budget_history
         194             :
         195             :     type(physics_buffer_desc), pointer, intent(in) :: pbuf2d(:,:)
         196             :
         197             :     integer :: istage
         198             :     ! outfld calls in diag_phys_writeout
         199        3072 :     call addfld (cnst_name(1), (/ 'lev' /), 'A', 'kg/kg',    cnst_longname(1))
         200        1536 :     call addfld ('NSTEP',      horiz_only,  'A', 'timestep', 'Model timestep')
         201        1536 :     call addfld ('PHIS',       horiz_only,  'I', 'm2/s2',    'Surface geopotential')
         202             :
         203        1536 :     call addfld ('PS',         horiz_only,  'A', 'Pa',       'Surface pressure')
         204        3072 :     call addfld ('T',          (/ 'lev' /), 'A', 'K',        'Temperature')
         205        3072 :     call addfld ('U',          (/ 'lev' /), 'A', 'm/s',      'Zonal wind')
         206        3072 :     call addfld ('V',          (/ 'lev' /), 'A', 'm/s',      'Meridional wind')
         207             :
         208        1536 :     call register_vector_field('U','V')
         209             :
         210             :     ! State before physics
         211        3072 :     call addfld ('TBP',     (/ 'lev' /), 'A','K',             'Temperature (before physics)')
         212        3072 :     call addfld ('UBP',     (/ 'lev' /), 'A','m/s',           'Zonal wind (before physics)')
         213        3072 :     call addfld ('VBP',     (/ 'lev' /), 'A','m/s',           'Meridional Wind (before physics)')
         214        1536 :     call register_vector_field('UBP','VBP')
         215        3072 :     call addfld (bpcnst(1), (/ 'lev' /), 'A','kg/kg',         trim(cnst_longname(1))//' (before physics)')
         216             :     ! State after physics
         217        3072 :     call addfld ('TAP',     (/ 'lev' /), 'A','K',             'Temperature (after physics)'       )
         218        3072 :     call addfld ('UAP',     (/ 'lev' /), 'A','m/s',           'Zonal wind (after physics)'        )
         219        3072 :     call addfld ('VAP',     (/ 'lev' /), 'A','m/s',           'Meridional wind (after physics)'   )
         220             :
         221        1536 :     call register_vector_field('UAP','VAP')
         222             :
         223        3072 :     call addfld (apcnst(1), (/ 'lev' /), 'A','kg/kg',         trim(cnst_longname(1))//' (after physics)')
         224        1536 :     if (.not.dycore_is('EUL')) then
         225        1536 :       call addfld ('TFIX',    horiz_only,  'A', 'K/s',        'T fixer (T equivalent of Energy correction)')
         226             :     end if
         227        3072 :     call addfld ('TTEND_TOT', (/ 'lev' /), 'A', 'K/s',        'Total temperature tendency')
         228             :
         229             :     ! outfld calls in diag_phys_tend_writeout
         230        3072 :     call addfld ('UTEND_TOT', (/ 'lev' /), 'A', 'm/s2',       'Total zonal wind tendency')
         231        3072 :     call addfld ('VTEND_TOT', (/ 'lev' /), 'A', 'm/s2',       'Total meridional wind tendency')
         232        1536 :     call register_vector_field('UTEND_TOT','VTEND_TOT')
         233             :
         234             :     ! Debugging negative water output fields
         235        3072 :     call addfld ('INEGCLPTEND ', (/ 'lev' /), 'A', 'kg/kg/s', 'Cloud ice tendency due to clipping neg values after microp')
         236        3072 :     call addfld ('LNEGCLPTEND ', (/ 'lev' /), 'A', 'kg/kg/s', 'Cloud liq tendency due to clipping neg values after microp')
         237        3072 :     call addfld ('VNEGCLPTEND ', (/ 'lev' /), 'A', 'kg/kg/s', 'Vapor tendency due to clipping neg values after microp')
         238             :
         239        3072 :     call addfld ('Z3',         (/ 'lev' /), 'A', 'm',         'Geopotential Height (above sea level)')
         240        1536 :     call addfld ('Z1000',      horiz_only,  'A', 'm',         'Geopotential Z at 1000 mbar pressure surface')
         241        1536 :     call addfld ('Z700',       horiz_only,  'A', 'm',         'Geopotential Z at 700 mbar pressure surface')
         242        1536 :     call addfld ('Z500',       horiz_only,  'A', 'm',         'Geopotential Z at 500 mbar pressure surface')
         243        1536 :     call addfld ('Z300',       horiz_only,  'A', 'm',         'Geopotential Z at 300 mbar pressure surface')
         244        1536 :     call addfld ('Z200',       horiz_only,  'A', 'm',         'Geopotential Z at 200 mbar pressure surface')
         245        1536 :     call addfld ('Z100',       horiz_only,  'A', 'm',         'Geopotential Z at 100 mbar pressure surface')
         246        1536 :     call addfld ('Z050',       horiz_only,  'A', 'm',         'Geopotential Z at 50 mbar pressure surface')
         247             :
         248        3072 :     call addfld ('ZZ',         (/ 'lev' /), 'A', 'm2',        'Eddy height variance' )
         249        3072 :     call addfld ('VZ',         (/ 'lev' /), 'A', 'm2/s',      'Meridional transport of geopotential height')
         250        3072 :     call addfld ('VT',         (/ 'lev' /), 'A', 'K m/s   ',  'Meridional heat transport')
         251        3072 :     call addfld ('VU',         (/ 'lev' /), 'A', 'm2/s2',     'Meridional flux of zonal momentum' )
         252        3072 :     call addfld ('VV',         (/ 'lev' /), 'A', 'm2/s2',     'Meridional velocity squared' )
         253        3072 :     call addfld ('OMEGAV',     (/ 'lev' /), 'A', 'm Pa/s2 ',  'Vertical flux of meridional momentum' )
         254        3072 :     call addfld ('OMGAOMGA',   (/ 'lev' /), 'A', 'Pa2/s2',    'Vertical flux of vertical momentum' )
         255             :
         256        3072 :     call addfld ('UU',         (/ 'lev' /), 'A', 'm2/s2',     'Zonal velocity squared' )
         257        3072 :     call addfld ('WSPEED',     (/ 'lev' /), 'X', 'm/s',       'Horizontal total wind speed maximum' )
         258        1536 :     call addfld ('WSPDSRFMX',  horiz_only,  'X', 'm/s',       'Horizontal total wind speed maximum at surface layer midpoint' )
         259        1536 :     call addfld ('WSPDSRFAV',  horiz_only,  'A', 'm/s',       'Horizontal total wind speed average at surface layer midpoint' )
         260             :
         261        3072 :     call addfld ('OMEGA',      (/ 'lev' /), 'A', 'Pa/s',      'Vertical velocity (pressure)')
         262        3072 :     call addfld ('OMEGAT',     (/ 'lev' /), 'A', 'K Pa/s  ',  'Vertical heat flux' )
         263        3072 :     call addfld ('OMEGAU',     (/ 'lev' /), 'A', 'm Pa/s2 ',  'Vertical flux of zonal momentum' )
         264        1536 :     call addfld ('OMEGA850',   horiz_only,  'A', 'Pa/s',      'Vertical velocity at 850 mbar pressure surface')
         265        1536 :     call addfld ('OMEGA500',   horiz_only,  'A', 'Pa/s',      'Vertical velocity at 500 mbar pressure surface')
         266             :
         267        1536 :     call addfld ('PSL',        horiz_only,  'A', 'Pa','Sea level pressure')
         268             :
         269        1536 :     call addfld ('T1000',      horiz_only,  'A', 'K','Temperature at 1000 mbar pressure surface')
         270        1536 :     call addfld ('T925',       horiz_only,  'A', 'K','Temperature at 925 mbar pressure surface')
         271        1536 :     call addfld ('T850',       horiz_only,  'A', 'K','Temperature at 850 mbar pressure surface')
         272        1536 :     call addfld ('T700',       horiz_only,  'A', 'K','Temperature at 700 mbar pressure surface')
         273        1536 :     call addfld ('T500',       horiz_only,  'A', 'K','Temperature at 500 mbar pressure surface')
         274        1536 :     call addfld ('T400',       horiz_only,  'A', 'K','Temperature at 400 mbar pressure surface')
         275        1536 :     call addfld ('T300',       horiz_only,  'A', 'K','Temperature at 300 mbar pressure surface')
         276        1536 :     call addfld ('T200',       horiz_only,  'A', 'K','Temperature at 200 mbar pressure surface')
         277        1536 :     call addfld ('T010',       horiz_only,  'A', 'K','Temperature at 10 mbar pressure surface')
         278             :
         279        1536 :     call addfld ('T7001000',   horiz_only,  'A', 'K','Temperature difference 700 mb - 1000 mb')
         280        1536 :     call addfld ('TH7001000',  horiz_only,  'A', 'K','Theta difference 700 mb - 1000 mb')
         281        1536 :     call addfld ('THE7001000', horiz_only,  'A', 'K','ThetaE difference 700 mb - 1000 mb')
         282             :
         283        1536 :     call addfld ('T8501000',   horiz_only,  'A', 'K','Temperature difference 850 mb - 1000 mb')
         284        1536 :     call addfld ('TH8501000',  horiz_only,  'A', 'K','Theta difference 850 mb - 1000 mb')
         285        1536 :     call addfld ('T9251000',   horiz_only,  'A', 'K','Temperature difference 925 mb - 1000 mb')
         286        1536 :     call addfld ('TH9251000',  horiz_only,  'A', 'K','Theta difference 925 mb - 1000 mb')
         287             :
         288        3072 :     call addfld ('TT',         (/ 'lev' /), 'A', 'K2','Eddy temperature variance' )
         289             :
         290        1536 :     call addfld ('U850',       horiz_only,  'A', 'm/s','Zonal wind at 850 mbar pressure surface')
         291        1536 :     call addfld ('U500',       horiz_only,  'A', 'm/s','Zonal wind at 500 mbar pressure surface')
         292        1536 :     call addfld ('U250',       horiz_only,  'A', 'm/s','Zonal wind at 250 mbar pressure surface')
         293        1536 :     call addfld ('U200',       horiz_only,  'A', 'm/s','Zonal wind at 200 mbar pressure surface')
         294        1536 :     call addfld ('U010',       horiz_only,  'A', 'm/s','Zonal wind at  10 mbar pressure surface')
         295        1536 :     call addfld ('V850',       horiz_only,  'A', 'm/s','Meridional wind at 850 mbar pressure surface')
         296        1536 :     call addfld ('V500',       horiz_only,  'A', 'm/s','Meridional wind at 500 mbar pressure surface')
         297        1536 :     call addfld ('V250',       horiz_only,  'A', 'm/s','Meridional wind at 250 mbar pressure surface')
         298        1536 :     call addfld ('V200',       horiz_only,  'A', 'm/s','Meridional wind at 200 mbar pressure surface')
         299             :
         300        1536 :     call register_vector_field('U850', 'V850')
         301        1536 :     call register_vector_field('U500', 'V500')
         302        1536 :     call register_vector_field('U250', 'V250')
         303        1536 :     call register_vector_field('U200', 'V200')
         304             :
         305        1536 :     call addfld ('UBOT',       horiz_only,  'A', 'm/s','Lowest model level zonal wind')
         306        1536 :     call addfld ('VBOT',       horiz_only,  'A', 'm/s','Lowest model level meridional wind')
         307        1536 :     call register_vector_field('UBOT', 'VBOT')
         308             :
         309        1536 :     call addfld ('ZBOT',       horiz_only,  'A', 'm','Lowest model level height')
         310             :
         311        1536 :     call addfld ('ATMEINT',    horiz_only,  'A', 'J/m2','Vertically integrated total atmospheric energy ')
         312             :
         313        1536 :     if (history_amwg) then
         314        1536 :       call add_default ('PHIS    '  , 1, ' ')
         315        1536 :       call add_default ('PS      '  , 1, ' ')
         316        1536 :       call add_default ('T       '  , 1, ' ')
         317        1536 :       call add_default ('U       '  , 1, ' ')
         318        1536 :       call add_default ('V       '  , 1, ' ')
         319        1536 :       call add_default ('Z3      '  , 1, ' ')
         320        1536 :       call add_default ('OMEGA   '  , 1, ' ')
         321        1536 :       call add_default ('VT      ', 1, ' ')
         322        1536 :       call add_default ('VU      ', 1, ' ')
         323        1536 :       call add_default ('VV      ', 1, ' ')
         324        1536 :       call add_default ('UU      ', 1, ' ')
         325        1536 :       call add_default ('OMEGAT  ', 1, ' ')
         326        1536 :       call add_default ('PSL     ', 1, ' ')
         327             :     end if
         328             :
         329        1536 :     if (history_vdiag) then
         330           0 :       call add_default ('U200', 2, ' ')
         331           0 :       call add_default ('V200', 2, ' ')
         332           0 :       call add_default ('U850', 2, ' ')
         333           0 :       call add_default ('U200', 3, ' ')
         334           0 :       call add_default ('U850', 3, ' ')
         335           0 :       call add_default ('OMEGA500', 3, ' ')
         336             :     end if
         337             :
         338        1536 :     if (history_eddy) then
         339           0 :       call add_default ('VT      ', 1, ' ')
         340           0 :       call add_default ('VU      ', 1, ' ')
         341           0 :       call add_default ('VV      ', 1, ' ')
         342           0 :       call add_default ('UU      ', 1, ' ')
         343           0 :       call add_default ('OMEGAT  ', 1, ' ')
         344           0 :       call add_default ('OMEGAU  ', 1, ' ')
         345           0 :       call add_default ('OMEGAV  ', 1, ' ')
         346             :     endif
         347             :
         348        1536 :     if ( history_budget ) then
         349           0 :       call add_default ('PHIS    '  , history_budget_histfile_num, ' ')
         350           0 :       call add_default ('PS      '  , history_budget_histfile_num, ' ')
         351           0 :       call add_default ('T       '  , history_budget_histfile_num, ' ')
         352           0 :       call add_default ('U       '  , history_budget_histfile_num, ' ')
         353           0 :       call add_default ('V       '  , history_budget_histfile_num, ' ')
         354           0 :       call add_default ('TTEND_TOT' , history_budget_histfile_num, ' ')
         355           0 :       call add_default ('UTEND_TOT' , history_budget_histfile_num, ' ')
         356           0 :       call add_default ('VTEND_TOT' , history_budget_histfile_num, ' ')
         357             :
         358             :       ! State before physics (FV)
         359           0 :       call add_default ('TBP     '  , history_budget_histfile_num, ' ')
         360           0 :       call add_default ('UBP     '  , history_budget_histfile_num, ' ')
         361           0 :       call add_default ('VBP     '  , history_budget_histfile_num, ' ')
         362           0 :       call add_default (bpcnst(1)   , history_budget_histfile_num, ' ')
         363             :       ! State after physics (FV)
         364           0 :       call add_default ('TAP     '  , history_budget_histfile_num, ' ')
         365           0 :       call add_default ('UAP     '  , history_budget_histfile_num, ' ')
         366           0 :       call add_default ('VAP     '  , history_budget_histfile_num, ' ')
         367           0 :       call add_default (apcnst(1)   , history_budget_histfile_num, ' ')
         368           0 :       if (.not.dycore_is('EUL')) then
         369           0 :         call add_default ('TFIX    '    , history_budget_histfile_num, ' ')
         370             :       end if
         371             :     end if
         372             :
         373        1536 :     if (history_waccm) then
         374           0 :       call add_default ('PHIS', 7, ' ')
         375           0 :       call add_default ('PS', 7, ' ')
         376           0 :       call add_default ('PSL', 7, ' ')
         377             :     end if
         378             :
         379             :     ! outfld calls in diag_phys_tend_writeout
         380        3072 :     call addfld ('PTTEND',          (/ 'lev' /), 'A', 'K/s','T total physics tendency')
         381        3072 :     call addfld ('UTEND_PHYSTOT',   (/ 'lev' /), 'A', 'm/s2','U total physics tendency')
         382        3072 :     call addfld ('VTEND_PHYSTOT',   (/ 'lev' /), 'A', 'm/s2','V total physics tendency')
         383        1536 :     call register_vector_field('UTEND_PHYSTOT','VTEND_PHYSTOT')
         384        1536 :     if ( history_budget ) then
         385           0 :       call add_default ('PTTEND'          , history_budget_histfile_num, ' ')
         386           0 :       call add_default ('UTEND_PHYSTOT'   , history_budget_histfile_num, ' ')
         387           0 :       call add_default ('VTEND_PHYSTOT'   , history_budget_histfile_num, ' ')
         388             :     end if
         389             :
         390             :     ! create history variables for fourier coefficients of the diurnal
         391             :     ! and semidiurnal tide in T, U, V, and Z3
         392        1536 :     call tidal_diag_init()
         393             :
         394        3072 :     call addfld( 'CPAIRV', (/ 'lev' /), 'I', 'J/K/kg', 'Variable specific heat cap air' )
         395        3072 :     call addfld( 'RAIRV', (/ 'lev' /), 'I', 'J/K/kg', 'Variable dry air gas constant' )
         396             :
         397        1536 :     if (thermo_budget_history) then
         398             :        !
         399             :        ! energy diagnostics addflds for vars_stage combinations plus e_m_snapshots
         400             :        !
         401           0 :        do istage = 1, num_stages
         402           0 :           call cam_budget_em_snapshot(TRIM(ADJUSTL(stage(istage))),'phy',longname=TRIM(ADJUSTL(stage_txt(istage))))
         403             :        end do
         404             :
         405             :        ! Create budgets that are a sum/dif of 2 stages
         406             :
         407           0 :        call cam_budget_em_register('dEdt_param_efix_physE','phAP','phBF','phy','dif',longname='dE/dt CAM physics + energy fixer using physics E formula (phAP-phBF)')
         408           0 :        call cam_budget_em_register('dEdt_param_efix_dynE' ,'dyAP','dyBF','phy','dif',longname='dE/dt CAM physics + energy fixer using dycore E formula (dyAP-dyBF)')
         409           0 :        call cam_budget_em_register('dEdt_param_physE'     ,'phAP','phBP','phy','dif',longname='dE/dt CAM physics using physics E formula (phAP-phBP)')
         410           0 :        call cam_budget_em_register('dEdt_param_dynE'      ,'dyAP','dyBP','phy','dif',longname='dE/dt CAM physics using dycore E (dyAP-dyBP)')
         411           0 :        call cam_budget_em_register('dEdt_dme_adjust_physE','phAM','phAP','phy','dif',longname='dE/dt dry mass adjustment using physics E formula (phAM-phAP)')
         412           0 :        call cam_budget_em_register('dEdt_dme_adjust_dynE' ,'dyAM','dyAP','phy','dif',longname='dE/dt dry mass adjustment using dycore E (dyAM-dyAP)')
         413           0 :        call cam_budget_em_register('dEdt_efix_physE'      ,'phBP','phBF','phy','dif',longname='dE/dt energy fixer using physics E formula (phBP-phBF)')
         414           0 :        call cam_budget_em_register('dEdt_efix_dynE'       ,'dyBP','dyBF','phy','dif',longname='dE/dt energy fixer using dycore E formula (dyBP-dyBF)')
         415           0 :        call cam_budget_em_register('dEdt_phys_tot_physE'  ,'phAM','phBF','phy','dif',longname='dE/dt physics total using physics E formula (phAM-phBF)')
         416           0 :        call cam_budget_em_register('dEdt_phys_tot_dynE'   ,'dyAM','dyBF','phy','dif',longname='dE/dt physics total using dycore E (dyAM-dyBF)')
         417             :     endif
         418        1536 :   end subroutine diag_init_dry
         419             :
         420        1536 :   subroutine diag_init_moist(pbuf2d)
         421             :
         422             :     ! Declare the history fields for which this module contains outfld calls.
         423             :
         424        1536 :     use cam_history,        only: addfld, add_default, horiz_only
         425             :     use constituent_burden, only: constituent_burden_init
         426             :     use physics_buffer,     only: pbuf_set_field
         427             :
         428             :     type(physics_buffer_desc), pointer, intent(in) :: pbuf2d(:,:)
         429             :
         430             :     integer :: m
         431             :     integer :: ixcldice, ixcldliq ! constituent indices for cloud liquid and ice water.
         432             :     integer :: ierr
         433             :     ! column burdens for all constituents except water vapor
         434        1536 :     call constituent_burden_init
         435             :
         436        1536 :     call cnst_get_ind('CLDLIQ', ixcldliq, abort=.false.)
         437        1536 :     call cnst_get_ind('CLDICE', ixcldice, abort=.false.)
         438             :
         439             :     ! outfld calls in diag_phys_writeout
         440        3072 :     call addfld ('OMEGAQ',     (/ 'lev' /), 'A', 'kgPa/kgs', 'Vertical water transport' )
         441        3072 :     call addfld ('VQ',         (/ 'lev' /), 'A', 'm/skg/kg',  'Meridional water transport')
         442        3072 :     call addfld ('QQ',         (/ 'lev' /), 'A', 'kg2/kg2',   'Eddy moisture variance')
         443             :
         444        3072 :     call addfld ('MQ',         (/ 'lev' /), 'A', 'kg/m2','Water vapor mass in layer')
         445        1536 :     call addfld ('TMQ',        horiz_only,  'A', 'kg/m2','Total (vertically integrated) precipitable water')
         446        3072 :     call addfld ('RELHUM',     (/ 'lev' /), 'A', 'percent','Relative humidity')
         447        3072 :     call addfld ('RHW',        (/ 'lev' /), 'A', 'percent','Relative humidity with respect to liquid')
         448        3072 :     call addfld ('RHI',        (/ 'lev' /), 'A', 'percent','Relative humidity with respect to ice')
         449        3072 :     call addfld ('RHCFMIP',    (/ 'lev' /), 'A', 'percent','Relative humidity with respect to water above 273 K, ice below 273 K')
         450             :
         451        1536 :     call addfld ('IVT',        horiz_only,  'A', 'kg/m/s','Total (vertically integrated) vapor transport')
         452        1536 :     call addfld ('uIVT',       horiz_only,  'A', 'kg/m/s','u-component (vertically integrated) vapor transport')
         453        1536 :     call addfld ('vIVT',       horiz_only,  'A', 'kg/m/s','v-component (vertically integrated) vapor transport')
         454             :
         455        1536 :     call addfld ('THE8501000', horiz_only,  'A', 'K','ThetaE difference 850 mb - 1000 mb')
         456        1536 :     call addfld ('THE9251000', horiz_only,  'A', 'K','ThetaE difference 925 mb - 1000 mb')
         457             :
         458        1536 :     call addfld ('Q1000',      horiz_only,  'A', 'kg/kg','Specific Humidity at 1000 mbar pressure surface')
         459        1536 :     call addfld ('Q925',       horiz_only,  'A', 'kg/kg','Specific Humidity at 925 mbar pressure surface')
         460        1536 :     call addfld ('Q850',       horiz_only,  'A', 'kg/kg','Specific Humidity at 850 mbar pressure surface')
         461        1536 :     call addfld ('Q200',       horiz_only,  'A', 'kg/kg','Specific Humidity at 200 mbar pressure surface')
         462        1536 :     call addfld ('QBOT',       horiz_only,  'A', 'kg/kg','Lowest model level water vapor mixing ratio')
         463             :
         464        1536 :     call addfld ('PSDRY',      horiz_only,  'A', 'Pa', 'Dry surface pressure')
         465        3072 :     call addfld ('PMID',       (/ 'lev' /), 'A', 'Pa', 'Pressure at layer midpoints')
         466        3072 :     call addfld ('PINT',       (/ 'ilev' /), 'A', 'Pa', 'Pressure at layer interfaces')
         467        3072 :     call addfld ('PDELDRY',    (/ 'lev' /), 'A', 'Pa', 'Dry pressure difference between levels')
         468        3072 :     call addfld ('PDEL',       (/ 'lev' /), 'A', 'Pa', 'Pressure difference between levels')
         469             :
         470             :     ! outfld calls in diag_conv
         471             :
         472        3072 :     call addfld ('DTCOND',       (/ 'lev' /), 'A','K/s','T tendency - moist processes')
         473        3072 :     call addfld ('DTCOND_24_COS',(/ 'lev' /), 'A','K/s','T tendency - moist processes 24hr. cos coeff.')
         474        3072 :     call addfld ('DTCOND_24_SIN',(/ 'lev' /), 'A','K/s','T tendency - moist processes 24hr. sin coeff.')
         475        3072 :     call addfld ('DTCOND_12_COS',(/ 'lev' /), 'A','K/s','T tendency - moist processes 12hr. cos coeff.')
         476        3072 :     call addfld ('DTCOND_12_SIN',(/ 'lev' /), 'A','K/s','T tendency - moist processes 12hr. sin coeff.')
         477        3072 :     call addfld ('DTCOND_08_COS',(/ 'lev' /), 'A','K/s','T tendency - moist processes  8hr. cos coeff.')
         478        3072 :     call addfld ('DTCOND_08_SIN',(/ 'lev' /), 'A','K/s','T tendency - moist processes  8hr. sin coeff.')
         479             :
         480        1536 :     call addfld ('PRECL',    horiz_only, 'A', 'm/s','Large-scale (stable) precipitation rate (liq + ice)'                )
         481        1536 :     call addfld ('PRECC',    horiz_only, 'A', 'm/s','Convective precipitation rate (liq + ice)'                          )
         482        1536 :     call addfld ('PRECT',    horiz_only, 'A', 'm/s','Total (convective and large-scale) precipitation rate (liq + ice)'  )
         483        1536 :     call addfld ('PREC_PCW', horiz_only, 'A', 'm/s','LS_pcw precipitation rate')
         484        1536 :     call addfld ('PREC_zmc', horiz_only, 'A', 'm/s','CV_zmc precipitation rate')
         485        1536 :     call addfld ('PRECTMX',  horiz_only, 'X','m/s','Maximum (convective and large-scale) precipitation rate (liq+ice)'   )
         486        1536 :     call addfld ('PRECSL',   horiz_only, 'A', 'm/s','Large-scale (stable) snow rate (water equivalent)'                  )
         487        1536 :     call addfld ('PRECSC',   horiz_only, 'A', 'm/s','Convective snow rate (water equivalent)'                            )
         488        1536 :     call addfld ('PRECCav',  horiz_only, 'A', 'm/s','Average large-scale precipitation (liq + ice)'                      )
         489        1536 :     call addfld ('PRECLav',  horiz_only, 'A', 'm/s','Average convective precipitation  (liq + ice)'                      )
         490             :
         491             :     ! outfld calls in diag_surf
         492             :
         493        1536 :     call addfld ('SHFLX',    horiz_only, 'A', 'W/m2','Surface sensible heat flux')
         494        1536 :     call addfld ('LHFLX',    horiz_only, 'A', 'W/m2','Surface latent heat flux')
         495        1536 :     call addfld ('QFLX',     horiz_only, 'A', 'kg/m2/s','Surface water flux')
         496             :
         497        1536 :     call addfld ('TAUX',     horiz_only, 'A', 'N/m2','Zonal surface stress')
         498        1536 :     call addfld ('TAUY',     horiz_only, 'A', 'N/m2','Meridional surface stress')
         499        1536 :     call addfld ('TREFHT',   horiz_only, 'A', 'K','Reference height temperature')
         500        1536 :     call addfld ('TREFHTMN', horiz_only, 'M','K','Minimum reference height temperature over output period')
         501        1536 :     call addfld ('TREFHTMX', horiz_only, 'X','K','Maximum reference height temperature over output period')
         502        1536 :     call addfld ('QREFHT',   horiz_only, 'A', 'kg/kg','Reference height humidity')
         503        1536 :     call addfld ('U10',      horiz_only, 'A', 'm/s','10m wind speed')
         504        1536 :     call addfld ('UGUST',    horiz_only, 'A', 'm/s','Gustiness term added to U10')
         505        1536 :     call addfld ('U10WITHGUSTS',horiz_only, 'A', 'm/s','10m wind speed with gustiness added')
         506        1536 :     call addfld ('RHREFHT',  horiz_only, 'A', 'fraction','Reference height relative humidity')
         507             :
         508        1536 :     call addfld ('LANDFRAC', horiz_only, 'A', 'fraction','Fraction of sfc area covered by land')
         509        1536 :     call addfld ('ICEFRAC',  horiz_only, 'A', 'fraction','Fraction of sfc area covered by sea-ice')
         510        1536 :     call addfld ('OCNFRAC',  horiz_only, 'A', 'fraction','Fraction of sfc area covered by ocean')
         511             :
         512        1536 :     call addfld ('TREFMNAV', horiz_only, 'A', 'K','Average of TREFHT daily minimum')
         513        1536 :     call addfld ('TREFMXAV', horiz_only, 'A', 'K','Average of TREFHT daily maximum')
         514             :
         515        1536 :     call addfld ('TS',       horiz_only, 'A', 'K','Surface temperature (radiative)')
         516        1536 :     call addfld ('TSMN',     horiz_only, 'M','K','Minimum surface temperature over output period')
         517        1536 :     call addfld ('TSMX',     horiz_only, 'X','K','Maximum surface temperature over output period')
         518        1536 :     call addfld ('SNOWHLND', horiz_only, 'A', 'm','Water equivalent snow depth')
         519        1536 :     call addfld ('SNOWHICE', horiz_only, 'A', 'm','Snow depth over ice', fill_value = 1.e30_r8)
         520        1536 :     call addfld ('TBOT',     horiz_only, 'A', 'K','Lowest model level temperature')
         521             :
         522        1536 :     call addfld ('ASDIR',    horiz_only, 'A', '1','albedo: shortwave, direct')
         523        1536 :     call addfld ('ASDIF',    horiz_only, 'A', '1','albedo: shortwave, diffuse')
         524        1536 :     call addfld ('ALDIR',    horiz_only, 'A', '1','albedo: longwave, direct')
         525        1536 :     call addfld ('ALDIF',    horiz_only, 'A', '1','albedo: longwave, diffuse')
         526        1536 :     call addfld ('SST',      horiz_only, 'A', 'K','sea surface temperature')
         527             :
         528             :
         529             :     ! outfld calls in diag_phys_tend_writeout
         530             :
         531        3072 :     call addfld (ptendnam(       1),(/ 'lev' /), 'A', 'kg/kg/s',trim(cnst_name(       1))//' total physics tendency '      )
         532             :
         533        1536 :     if (ixcldliq > 0) then
         534        3072 :        call addfld (ptendnam(ixcldliq),(/ 'lev' /), 'A', 'kg/kg/s',trim(cnst_name(ixcldliq))//' total physics tendency '      )
         535             :     end if
         536        1536 :     if (ixcldice > 0) then
         537        3072 :       call addfld (ptendnam(ixcldice),(/ 'lev' /), 'A', 'kg/kg/s',trim(cnst_name(ixcldice))//' total physics tendency ')
         538             :     end if
         539             :
         540             :     ! outfld calls in diag_physvar_ic
         541             :
         542        3072 :     call addfld ('QCWAT&IC',  (/ 'lev' /),  'I','kg/kg','q associated with cloud water'                   )
         543        3072 :     call addfld ('TCWAT&IC',  (/ 'lev' /),  'I','kg/kg','T associated with cloud water'                   )
         544        3072 :     call addfld ('LCWAT&IC',  (/ 'lev' /),  'I','kg/kg','Cloud water (ice + liq'                          )
         545        3072 :     call addfld ('CLOUD&IC',  (/ 'lev' /),  'I','fraction','Cloud fraction'                               )
         546        3072 :     call addfld ('CONCLD&IC', (/ 'lev' /),  'I','fraction','Convective cloud fraction'                    )
         547        3072 :     call addfld ('TKE&IC',    (/ 'ilev' /), 'I','m2/s2','Turbulent Kinetic Energy'                        )
         548        1536 :     call addfld ('CUSH&IC',   horiz_only,   'I','m','Convective Scale Height'                             )
         549        3072 :     call addfld ('KVH&IC',    (/ 'ilev' /), 'I','m2/s','Vertical diffusion diffusivities (heat/moisture)' )
         550        3072 :     call addfld ('KVM&IC',    (/ 'ilev' /), 'I','m2/s','Vertical diffusion diffusivities (momentum)'      )
         551        1536 :     call addfld ('PBLH&IC',   horiz_only,   'I','m','PBL height'                                          )
         552        1536 :     call addfld ('TPERT&IC',  horiz_only,   'I','K','Perturbation temperature (eddies in PBL)'            )
         553        1536 :     call addfld ('QPERT&IC',  horiz_only,   'I','kg/kg','Perturbation specific humidity (eddies in PBL)'  )
         554             :
         555             :     ! CAM export state
         556        1536 :     call addfld('a2x_BCPHIWET', horiz_only, 'A', 'kg/m2/s', 'wetdep of hydrophilic black carbon')
         557        1536 :     call addfld('a2x_BCPHIDRY', horiz_only, 'A', 'kg/m2/s', 'drydep of hydrophilic black carbon')
         558        1536 :     call addfld('a2x_BCPHODRY', horiz_only, 'A', 'kg/m2/s', 'drydep of hydrophobic black carbon')
         559        1536 :     call addfld('a2x_OCPHIWET', horiz_only, 'A', 'kg/m2/s', 'wetdep of hydrophilic organic carbon')
         560        1536 :     call addfld('a2x_OCPHIDRY', horiz_only, 'A', 'kg/m2/s', 'drydep of hydrophilic organic carbon')
         561        1536 :     call addfld('a2x_OCPHODRY', horiz_only, 'A', 'kg/m2/s', 'drydep of hydrophobic organic carbon')
         562        1536 :     call addfld('a2x_DSTWET1',  horiz_only, 'A',  'kg/m2/s', 'wetdep of dust (bin1)')
         563        1536 :     call addfld('a2x_DSTDRY1',  horiz_only, 'A',  'kg/m2/s', 'drydep of dust (bin1)')
         564        1536 :     call addfld('a2x_DSTWET2',  horiz_only, 'A',  'kg/m2/s', 'wetdep of dust (bin2)')
         565        1536 :     call addfld('a2x_DSTDRY2',  horiz_only, 'A',  'kg/m2/s', 'drydep of dust (bin2)')
         566        1536 :     call addfld('a2x_DSTWET3',  horiz_only, 'A',  'kg/m2/s', 'wetdep of dust (bin3)')
         567        1536 :     call addfld('a2x_DSTDRY3',  horiz_only, 'A',  'kg/m2/s', 'drydep of dust (bin3)')
         568        1536 :     call addfld('a2x_DSTWET4',  horiz_only, 'A',  'kg/m2/s', 'wetdep of dust (bin4)')
         569        1536 :     call addfld('a2x_DSTDRY4',  horiz_only, 'A',  'kg/m2/s', 'drydep of dust (bin4)')
         570             :
         571             :     ! defaults
         572        1536 :     if (history_amwg) then
         573        1536 :       call add_default (cnst_name(1), 1, ' ')
         574        1536 :       call add_default ('VQ      ', 1, ' ')
         575        1536 :       call add_default ('TMQ     ', 1, ' ')
         576        1536 :       call add_default ('PSL     ', 1, ' ')
         577        1536 :       call add_default ('RELHUM  ', 1, ' ')
         578             :
         579        1536 :       call add_default ('DTCOND  ', 1, ' ')
         580        1536 :       call add_default ('PRECL   ', 1, ' ')
         581        1536 :       call add_default ('PRECC   ', 1, ' ')
         582        1536 :       call add_default ('PRECSL  ', 1, ' ')
         583        1536 :       call add_default ('PRECSC  ', 1, ' ')
         584        1536 :       call add_default ('SHFLX   ', 1, ' ')
         585        1536 :       call add_default ('LHFLX   ', 1, ' ')
         586        1536 :       call add_default ('QFLX    ', 1, ' ')
         587        1536 :       call add_default ('TAUX    ', 1, ' ')
         588        1536 :       call add_default ('TAUY    ', 1, ' ')
         589        1536 :       call add_default ('TREFHT  ', 1, ' ')
         590        1536 :       call add_default ('LANDFRAC', 1, ' ')
         591        1536 :       call add_default ('OCNFRAC ', 1, ' ')
         592        1536 :       call add_default ('QREFHT  ', 1, ' ')
         593        1536 :       call add_default ('U10     ', 1, ' ')
         594        1536 :       call add_default ('ICEFRAC ', 1, ' ')
         595        1536 :       call add_default ('TS      ', 1, ' ')
         596        1536 :       call add_default ('TSMN    ', 1, ' ')
         597        1536 :       call add_default ('TSMX    ', 1, ' ')
         598        1536 :       call add_default ('SNOWHLND', 1, ' ')
         599        1536 :       call add_default ('SNOWHICE', 1, ' ')
         600             :     end if
         601             :
         602        1536 :     if (dycore_is('SE')) then
         603        1536 :       call add_default ('PSDRY', 1, ' ')
         604        1536 :       call add_default ('PMID',  1, ' ')
         605             :    end if
         606             :
         607        1536 :     if (dycore_is('MPAS')) then
         608           0 :       call add_default ('PINT', 1, ' ')
         609           0 :       call add_default ('PMID',  1, ' ')
         610           0 :       call add_default ('PDEL',  1, ' ')
         611             :    end if
         612             :
         613        1536 :     if (history_eddy) then
         614           0 :       call add_default ('VQ      ', 1, ' ')
         615             :     endif
         616             :
         617        1536 :     if ( history_budget ) then
         618           0 :       call add_default (cnst_name(1), history_budget_histfile_num, ' ')
         619           0 :       call add_default ('PTTEND'          , history_budget_histfile_num, ' ')
         620           0 :       call add_default ('UTEND_PHYSTOT'   , history_budget_histfile_num, ' ')
         621           0 :       call add_default ('VTEND_PHYSTOT'   , history_budget_histfile_num, ' ')
         622           0 :       call add_default (ptendnam(       1), history_budget_histfile_num, ' ')
         623           0 :       if (ixcldliq > 0) then
         624           0 :          call add_default (ptendnam(ixcldliq), history_budget_histfile_num, ' ')
         625             :       end if
         626           0 :       if (ixcldice > 0) then
         627           0 :         call add_default (ptendnam(ixcldice), history_budget_histfile_num, ' ')
         628             :       end if
         629           0 :       if( history_budget_histfile_num > 1 ) then
         630           0 :         call add_default ('DTCOND  '         , history_budget_histfile_num, ' ')
         631             :       end if
         632             :     end if
         633             :
         634        1536 :     if (history_vdiag) then
         635           0 :       call add_default ('PRECT   ', 2, ' ')
         636           0 :       call add_default ('PRECT   ', 3, ' ')
         637           0 :       call add_default ('PRECT   ', 4, ' ')
         638             :     end if
         639             :
         640             :     ! Initial file - Optional fields
         641        1536 :     if (inithist_all.or.single_column) then
         642           0 :       call add_default ('CONCLD&IC  ',0, 'I')
         643           0 :       call add_default ('QCWAT&IC   ',0, 'I')
         644           0 :       call add_default ('TCWAT&IC   ',0, 'I')
         645           0 :       call add_default ('LCWAT&IC   ',0, 'I')
         646           0 :       call add_default ('PBLH&IC    ',0, 'I')
         647           0 :       call add_default ('TPERT&IC   ',0, 'I')
         648           0 :       call add_default ('QPERT&IC   ',0, 'I')
         649           0 :       call add_default ('CLOUD&IC   ',0, 'I')
         650           0 :       call add_default ('TKE&IC     ',0, 'I')
         651           0 :       call add_default ('CUSH&IC    ',0, 'I')
         652           0 :       call add_default ('KVH&IC     ',0, 'I')
         653           0 :       call add_default ('KVM&IC     ',0, 'I')
         654             :     end if
         655             :
         656             :     ! determine number of constituents for which convective tendencies must be computed
         657        1536 :     if (history_budget) then
         658           0 :       dqcond_num = pcnst
         659             :     else
         660        1536 :       if (diag_cnst_conv_tend == 'none')   dqcond_num = 0
         661        1536 :       if (diag_cnst_conv_tend == 'q_only') dqcond_num = 1
         662        1536 :       if (diag_cnst_conv_tend == 'all')    dqcond_num = pcnst
         663             :     end if
         664             :
         665        3072 :     do m = 1, dqcond_num
         666        3072 :       dcconnam(m) = 'DC'//cnst_name(m)
         667             :     end do
         668             :
         669        1536 :     if ((diag_cnst_conv_tend == 'q_only') .or. (diag_cnst_conv_tend == 'all') .or. history_budget) then
         670        3072 :       call addfld (dcconnam(1),(/ 'lev' /),'A', 'kg/kg/s',trim(cnst_name(1))//' tendency due to moist processes')
         671        1536 :       if ( diag_cnst_conv_tend == 'q_only' .or. diag_cnst_conv_tend == 'all' ) then
         672        1536 :         call add_default (dcconnam(1),                           1, ' ')
         673             :       end if
         674        1536 :       if( history_budget ) then
         675           0 :         call add_default (dcconnam(1), history_budget_histfile_num, ' ')
         676             :       end if
         677        1536 :       if (diag_cnst_conv_tend == 'all' .or. history_budget) then
         678           0 :         do m = 2, pcnst
         679           0 :           call addfld (dcconnam(m),(/ 'lev' /),'A', 'kg/kg/s',trim(cnst_name(m))//' tendency due to moist processes')
         680           0 :           if( diag_cnst_conv_tend == 'all' ) then
         681           0 :             call add_default (dcconnam(m),                           1, ' ')
         682             :           end if
         683           0 :           if( history_budget .and. (m == ixcldliq .or. m == ixcldice) ) then
         684             :             call add_default (dcconnam(m), history_budget_histfile_num, ' ')
         685             :           end if
         686             :         end do
         687             :       end if
         688             :     end if
         689             :
         690             :     ! Pbuf field indices for collecting output data
         691        1536 :     relhum_idx = pbuf_get_index('RELHUM',  errcode=ierr)
         692        1536 :     qcwat_idx  = pbuf_get_index('QCWAT',  errcode=ierr)
         693        1536 :     tcwat_idx  = pbuf_get_index('TCWAT',  errcode=ierr)
         694        1536 :     lcwat_idx  = pbuf_get_index('LCWAT',  errcode=ierr)
         695        1536 :     cld_idx    = pbuf_get_index('CLD',    errcode=ierr)
         696        1536 :     concld_idx = pbuf_get_index('CONCLD', errcode=ierr)
         697             :
         698        1536 :     tke_idx  = pbuf_get_index('tke',  errcode=ierr)
         699        1536 :     kvm_idx  = pbuf_get_index('kvm',  errcode=ierr)
         700        1536 :     kvh_idx  = pbuf_get_index('kvh',  errcode=ierr)
         701        1536 :     cush_idx = pbuf_get_index('cush', errcode=ierr)
         702             :
         703        1536 :     pblh_idx  = pbuf_get_index('pblh',  errcode=ierr)
         704        1536 :     tpert_idx = pbuf_get_index('tpert', errcode=ierr)
         705        1536 :     qpert_idx = pbuf_get_index('qpert', errcode=ierr)
         706             :
         707        1536 :     prec_dp_idx  = pbuf_get_index('PREC_DP',  errcode=ierr)
         708        1536 :     snow_dp_idx  = pbuf_get_index('SNOW_DP',  errcode=ierr)
         709        1536 :     prec_sh_idx  = pbuf_get_index('PREC_SH',  errcode=ierr)
         710        1536 :     snow_sh_idx  = pbuf_get_index('SNOW_SH',  errcode=ierr)
         711        1536 :     prec_sed_idx = pbuf_get_index('PREC_SED', errcode=ierr)
         712        1536 :     snow_sed_idx = pbuf_get_index('SNOW_SED', errcode=ierr)
         713        1536 :     prec_pcw_idx = pbuf_get_index('PREC_PCW', errcode=ierr)
         714        1536 :     snow_pcw_idx = pbuf_get_index('SNOW_PCW', errcode=ierr)
         715             :
         716        1536 :     if (is_first_step()) then
         717         768 :       call pbuf_set_field(pbuf2d, trefmxav_idx, -1.0e36_r8)
         718         768 :       call pbuf_set_field(pbuf2d, trefmnav_idx,  1.0e36_r8)
         719             :     end if
         720             :
         721        1536 :   end subroutine diag_init_moist
         722             :
         723        1536 :   subroutine diag_init(pbuf2d)
         724             :
         725             :     ! Declare the history fields for which this module contains outfld calls.
         726             :
         727             :     type(physics_buffer_desc), pointer, intent(in) :: pbuf2d(:,:)
         728             :
         729             :     ! ----------------------------
         730             :     ! determine default variables
         731             :     ! ----------------------------
         732             :     call phys_getopts(history_amwg_out   = history_amwg    , &
         733             :          history_vdiag_out  = history_vdiag   , &
         734             :          history_eddy_out   = history_eddy    , &
         735             :          history_budget_out = history_budget  , &
         736             :          history_budget_histfile_num_out = history_budget_histfile_num, &
         737        1536 :          history_waccm_out  = history_waccm)
         738             :
         739        1536 :     call diag_init_dry(pbuf2d)
         740        1536 :     if (moist_physics) then
         741        1536 :       call diag_init_moist(pbuf2d)
         742             :     end if
         743             :
         744        1536 :   end subroutine diag_init
         745             :
         746             : !===============================================================================
         747             :
         748      370944 :   subroutine diag_allocate_dry()
         749             :     use infnan, only: nan, assignment(=)
         750             :
         751             :     ! Allocate memory for module variables.
         752             :     ! Done at the begining of a physics step at same point as the pbuf allocate
         753             :     ! for variables with "physpkg" scope.
         754             :
         755             :     ! Local variables
         756             :     character(len=*), parameter :: sub = 'diag_allocate_dry'
         757             :     character(len=128)          :: errmsg
         758             :     integer                     :: istat
         759             :
         760     1112832 :     allocate(dtcond(pcols,pver,begchunk:endchunk), stat=istat)
         761      370944 :     if ( istat /= 0 ) then
         762           0 :       write(errmsg, '(2a,i0)') sub, ': allocate failed, stat = ',istat
         763           0 :       call endrun (errmsg)
         764             :     end if
         765      370944 :     dtcond = nan
         766      370944 :   end subroutine diag_allocate_dry
         767             :
         768      370944 :   subroutine diag_allocate_moist()
         769             :     use infnan, only: nan, assignment(=)
         770             :
         771             :     ! Allocate memory for module variables.
         772             :     ! Done at the begining of a physics step at same point as the pbuf allocate
         773             :     ! for variables with "physpkg" scope.
         774             :
         775             :     ! Local variables
         776             :     character(len=*), parameter :: sub = 'diag_allocate_moist'
         777             :     character(len=128)          :: errmsg
         778             :     integer                     :: i, istat
         779             :
         780      370944 :     if (dqcond_num > 0) then
         781     1483776 :       allocate(dqcond(dqcond_num))
         782      741888 :       do i = 1, dqcond_num
         783     1112832 :         allocate(dqcond(i)%cnst(pcols,pver,begchunk:endchunk), stat=istat)
         784      370944 :         if ( istat /= 0 ) then
         785           0 :           write(errmsg, '(2a,i0)') sub, ': allocate failed, stat = ',istat
         786           0 :           call endrun (errmsg)
         787             :         end if
         788      741888 :         dqcond(i)%cnst = nan
         789             :       end do
         790             :     end if
         791             :
         792      370944 :   end subroutine diag_allocate_moist
         793             :
         794      370944 :   subroutine diag_allocate()
         795             :
         796      370944 :     call diag_allocate_dry()
         797      370944 :     if (moist_physics) then
         798      370944 :       call diag_allocate_moist()
         799             :     end if
         800             :
         801      370944 :   end subroutine diag_allocate
         802             :
         803             : !===============================================================================
         804             :
         805      369408 :   subroutine diag_deallocate_dry()
         806             :     ! Deallocate memory for module variables.
         807             :     ! Done at the end of a physics step at same point as the pbuf deallocate for
         808             :     ! variables with "physpkg" scope.
         809             :
         810             :     ! Local variables
         811             :     character(len=*), parameter :: sub = 'diag_deallocate_dry'
         812             :     integer :: istat
         813             :
         814      369408 :     deallocate(dtcond, stat=istat)
         815           0 :     if ( istat /= 0 ) call endrun (sub//': ERROR: deallocate failed')
         816      369408 :   end subroutine diag_deallocate_dry
         817             :
         818      369408 :   subroutine diag_deallocate_moist()
         819             :
         820             :     ! Deallocate memory for module variables.
         821             :     ! Done at the end of a physics step at same point as the pbuf deallocate for
         822             :     ! variables with "physpkg" scope.
         823             :
         824             :     ! Local variables
         825             :     character(len=*), parameter :: sub = 'diag_deallocate_moist'
         826             :     integer :: i, istat
         827             :
         828      369408 :     if (dqcond_num > 0) then
         829      738816 :       do i = 1, dqcond_num
         830      369408 :         deallocate(dqcond(i)%cnst, stat=istat)
         831      369408 :         if ( istat /= 0 ) call endrun (sub//': ERROR: deallocate failed')
         832             :       end do
         833      738816 :       deallocate(dqcond, stat=istat)
         834           0 :       if ( istat /= 0 ) call endrun (sub//': ERROR: deallocate failed')
         835             :     end if
         836      369408 :   end subroutine diag_deallocate_moist
         837             :
         838      369408 :   subroutine diag_deallocate()
         839             :
         840      369408 :     call diag_deallocate_dry()
         841      369408 :     if (moist_physics) then
         842      369408 :       call diag_deallocate_moist()
         843             :     end if
         844             :
         845      369408 :   end subroutine diag_deallocate
         846             :
         847             : !===============================================================================
         848             :
         849     1495368 :   subroutine diag_conv_tend_ini(state,pbuf)
         850             :
         851             :     ! Initialize convective tendency calcs.
         852             :
         853             :     ! Arguments:
         854             :     type(physics_state), intent(in) :: state
         855             :     type(physics_buffer_desc), pointer :: pbuf(:)
         856             :
         857             :     ! Local variables:
         858             :
         859             :     integer :: i, k, m, lchnk, ncol
         860     1495368 :     real(r8), pointer, dimension(:,:) :: t_ttend
         861     1495368 :     real(r8), pointer, dimension(:,:) :: t_utend
         862     1495368 :     real(r8), pointer, dimension(:,:) :: t_vtend
         863             :
         864     1495368 :     lchnk = state%lchnk
         865     1495368 :     ncol  = state%ncol
         866             :
         867    40374936 :     do k = 1, pver
         868   650693736 :       do i = 1, ncol
         869   649198368 :         dtcond(i,k,lchnk) = state%t(i,k)
         870             :       end do
         871             :     end do
         872             :
         873     2990736 :     do m = 1, dqcond_num
         874    41870304 :       do k = 1, pver
         875   650693736 :         do i = 1, ncol
         876   649198368 :           dqcond(m)%cnst(i,k,lchnk) = state%q(i,k,m)
         877             :         end do
         878             :       end do
         879             :     end do
         880             :
         881             :     !! initialize to pbuf T_TTEND to temperature at first timestep
         882     1495368 :     if (is_first_step()) then
         883        6192 :       do m = 1, dyn_time_lvls
         884       12384 :         call pbuf_get_field(pbuf, t_ttend_idx, t_ttend, start=(/1,1,m/), kount=(/pcols,pver,1/))
         885     1347192 :         t_ttend(:ncol,:) = state%t(:ncol,:)
         886       12384 :         call pbuf_get_field(pbuf, t_utend_idx, t_utend, start=(/1,1,m/), kount=(/pcols,pver,1/))
         887     1347192 :         t_utend(:ncol,:) = state%u(:ncol,:)
         888       12384 :         call pbuf_get_field(pbuf, t_vtend_idx, t_vtend, start=(/1,1,m/), kount=(/pcols,pver,1/))
         889     1350288 :         t_vtend(:ncol,:) = state%v(:ncol,:)
         890             :       end do
         891             :     end if
         892             :
         893     1495368 :   end subroutine diag_conv_tend_ini
         894             :
         895             : !===============================================================================
         896             :
         897     1495368 :   subroutine diag_phys_writeout_dry(state, pbuf, p_surf_t)
         898             :
         899             :     !-----------------------------------------------------------------------
         900             :     !
         901             :     ! Purpose: output dry physics diagnostics
         902             :     !
         903             :     !-----------------------------------------------------------------------
         904             :     use physconst,            only: gravit, rga, rair, cappa
         905             :     use time_manager,         only: get_nstep
         906             :     use interpolate_data,     only: vertinterp
         907             :     use tidal_diag,           only: tidal_diag_write
         908             :     use air_composition,      only: cpairv, rairv
         909             :     use cam_diagnostic_utils, only: cpslec
         910             :     !-----------------------------------------------------------------------
         911             :     !
         912             :     ! Arguments
         913             :     !
         914             :     type(physics_state), intent(inout) :: state
         915             :     type(physics_buffer_desc), pointer :: pbuf(:)
         916             :     real(r8),            intent(out)   :: p_surf_t(pcols, nsurf)  ! data interpolated to a pressure surface
         917             :     !
         918             :     !---------------------------Local workspace-----------------------------
         919             :     !
         920             :     real(r8) :: ftem(pcols,pver)  ! temporary workspace
         921             :     real(r8) :: z3(pcols,pver)    ! geo-potential height
         922             :     real(r8) :: p_surf(pcols)     ! data interpolated to a pressure surface
         923             :     real(r8) :: timestep(pcols)   ! used for outfld call
         924             :
         925     1495368 :     real(r8), pointer :: psl(:)   ! Sea Level Pressure
         926             :
         927             :     integer  :: i, k, m, lchnk, ncol, nstep
         928             :     !
         929             :     !-----------------------------------------------------------------------
         930             :     !
         931     1495368 :     lchnk = state%lchnk
         932     1495368 :     ncol  = state%ncol
         933             :
         934             :     ! Output NSTEP for debugging
         935     2990736 :     nstep = get_nstep()
         936    24969168 :     timestep(:ncol) = nstep
         937     1495368 :     call outfld ('NSTEP   ',timestep, pcols, lchnk)
         938             :
         939     1495368 :     call outfld('T       ',state%t , pcols   ,lchnk   )
         940     1495368 :     call outfld('PS      ',state%ps, pcols   ,lchnk   )
         941     1495368 :     call outfld('U       ',state%u , pcols   ,lchnk   )
         942     1495368 :     call outfld('V       ',state%v , pcols   ,lchnk   )
         943             :
         944     1495368 :     call outfld('PHIS    ',state%phis,    pcols,   lchnk     )
         945             :
         946     1495368 :     if (write_camiop) call outfld('phis    ',state%phis,    pcols,   lchnk     )
         947             :
         948   153698328 :     call outfld( 'CPAIRV', cpairv(:ncol,:,lchnk), ncol, lchnk )
         949   153698328 :     call outfld( 'RAIRV', rairv(:ncol,:,lchnk), ncol, lchnk )
         950             :
         951     5981472 :     do m = 1, pcnst
         952     5981472 :       if (cnst_cam_outfld(m)) then
         953     4486104 :         call outfld(cnst_name(m), state%q(1,1,m), pcols, lchnk)
         954             :       end if
         955             :     end do
         956             :
         957             :     !
         958             :     ! Add height of surface to midpoint height above surface
         959             :     !
         960    40374936 :     do k = 1, pver
         961   650693736 :       z3(:ncol,k) = state%zm(:ncol,k) + state%phis(:ncol)*rga
         962             :     end do
         963     1495368 :     call outfld('Z3      ',z3,pcols,lchnk)
         964             :     !
         965             :     ! Output Z3 on pressure surfaces
         966             :     !
         967     1495368 :     if (hist_fld_active('Z1000')) then
         968             :       call vertinterp(ncol, pcols, pver, state%pmid, 100000._r8, z3, p_surf, &
         969           0 :           extrapolate='Z', ln_interp=.true., ps=state%ps, phis=state%phis, tbot=state%t(:,pver))
         970           0 :       call outfld('Z1000    ', p_surf, pcols, lchnk)
         971             :     end if
         972     1495368 :     if (hist_fld_active('Z700')) then
         973             :       call vertinterp(ncol, pcols, pver, state%pmid, 70000._r8, z3, p_surf, &
         974           0 :           extrapolate='Z', ln_interp=.true., ps=state%ps, phis=state%phis, tbot=state%t(:,pver))
         975           0 :       call outfld('Z700    ', p_surf, pcols, lchnk)
         976             :     end if
         977     1495368 :     if (hist_fld_active('Z500')) then
         978             :       call vertinterp(ncol, pcols, pver, state%pmid, 50000._r8, z3, p_surf, &
         979           0 :           extrapolate='Z', ln_interp=.true., ps=state%ps, phis=state%phis, tbot=state%t(:,pver))
         980           0 :       call outfld('Z500    ', p_surf, pcols, lchnk)
         981             :     end if
         982     1495368 :     if (hist_fld_active('Z300')) then
         983           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 30000._r8, z3, p_surf, ln_interp=.true.)
         984           0 :       call outfld('Z300    ', p_surf, pcols, lchnk)
         985             :     end if
         986     1495368 :     if (hist_fld_active('Z200')) then
         987           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 20000._r8, z3, p_surf, ln_interp=.true.)
         988           0 :       call outfld('Z200    ', p_surf, pcols, lchnk)
         989             :     end if
         990     1495368 :     if (hist_fld_active('Z100')) then
         991           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 10000._r8, z3, p_surf, ln_interp=.true.)
         992           0 :       call outfld('Z100    ', p_surf, pcols, lchnk)
         993             :     end if
         994     1495368 :     if (hist_fld_active('Z050')) then
         995           0 :       call vertinterp(ncol, pcols, pver, state%pmid,  5000._r8, z3, p_surf, ln_interp=.true.)
         996           0 :       call outfld('Z050    ', p_surf, pcols, lchnk)
         997             :     end if
         998             :     !
         999             :     ! Quadratic height fiels Z3*Z3
        1000             :     !
        1001   650693736 :     ftem(:ncol,:) = z3(:ncol,:)*z3(:ncol,:)
        1002     1495368 :     call outfld('ZZ      ',ftem,pcols,lchnk)
        1003             :
        1004   650693736 :     ftem(:ncol,:) = z3(:ncol,:)*state%v(:ncol,:)
        1005     1495368 :     call outfld('VZ      ',ftem,  pcols,lchnk)
        1006             :     !
        1007             :     ! Meridional advection fields
        1008             :     !
        1009   650693736 :     ftem(:ncol,:) = state%v(:ncol,:)*state%t(:ncol,:)
        1010     1495368 :     call outfld ('VT      ',ftem    ,pcols   ,lchnk     )
        1011             :
        1012   650693736 :     ftem(:ncol,:) = state%v(:ncol,:)**2
        1013     1495368 :     call outfld ('VV      ',ftem    ,pcols   ,lchnk     )
        1014             :
        1015   650693736 :     ftem(:ncol,:) = state%v(:ncol,:) * state%u(:ncol,:)
        1016     1495368 :     call outfld ('VU      ',ftem    ,pcols   ,lchnk     )
        1017             :     !
        1018             :     ! zonal advection
        1019             :     !
        1020   650693736 :     ftem(:ncol,:) = state%u(:ncol,:)**2
        1021     1495368 :     call outfld ('UU      ',ftem    ,pcols   ,lchnk     )
        1022             :
        1023             :     ! Wind speed
        1024   650693736 :     ftem(:ncol,:) = sqrt( state%u(:ncol,:)**2 + state%v(:ncol,:)**2)
        1025     1495368 :     call outfld ('WSPEED  ',ftem    ,pcols   ,lchnk     )
        1026     1495368 :     call outfld ('WSPDSRFMX',ftem(:,pver)   ,pcols   ,lchnk     )
        1027     1495368 :     call outfld ('WSPDSRFAV',ftem(:,pver)   ,pcols   ,lchnk     )
        1028             :
        1029             :     ! Vertical velocity and advection
        1030             :
        1031     1495368 :     if (single_column) then
        1032           0 :       call outfld('OMEGA   ',wfld,    pcols,   lchnk     )
        1033             :     else
        1034     1495368 :       call outfld('OMEGA   ',state%omega,    pcols,   lchnk     )
        1035             :     endif
        1036             :
        1037     1495368 :     if (write_camiop) call outfld('omega   ',state%omega,    pcols,   lchnk     )
        1038             :
        1039   650693736 :     ftem(:ncol,:) = state%omega(:ncol,:)*state%t(:ncol,:)
        1040     1495368 :     call outfld('OMEGAT  ',ftem,    pcols,   lchnk     )
        1041   650693736 :     ftem(:ncol,:) = state%omega(:ncol,:)*state%u(:ncol,:)
        1042     1495368 :     call outfld('OMEGAU  ',ftem,    pcols,   lchnk     )
        1043   650693736 :     ftem(:ncol,:) = state%omega(:ncol,:)*state%v(:ncol,:)
        1044     1495368 :     call outfld('OMEGAV  ',ftem,    pcols,   lchnk     )
        1045   650693736 :     ftem(:ncol,:) = state%omega(:ncol,:)*state%omega(:ncol,:)
        1046     1495368 :     call outfld('OMGAOMGA',ftem,    pcols,   lchnk     )
        1047             :     !
        1048             :     ! Output omega at 850 and 500 mb pressure levels
        1049             :     !
        1050     1495368 :     if (hist_fld_active('OMEGA850')) then
        1051           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%omega, p_surf)
        1052           0 :       call outfld('OMEGA850', p_surf, pcols, lchnk)
        1053             :     end if
        1054     1495368 :     if (hist_fld_active('OMEGA500')) then
        1055           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 50000._r8, state%omega, p_surf)
        1056           0 :       call outfld('OMEGA500', p_surf, pcols, lchnk)
        1057             :     end if
        1058             :
        1059             :     ! Sea level pressure
        1060     1495368 :     call pbuf_get_field(pbuf, psl_idx, psl)
        1061     1495368 :     call cpslec(ncol, state%pmid, state%phis, state%ps, state%t, psl, gravit, rair)
        1062     1495368 :     call outfld('PSL', psl, pcols, lchnk)
        1063             :
        1064             :     ! Output T,u,v fields on pressure surfaces
        1065             :     !
        1066     1495368 :     if (hist_fld_active('T850')) then
        1067             :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%t, p_surf, &
        1068           0 :           extrapolate='T', ps=state%ps, phis=state%phis)
        1069           0 :       call outfld('T850    ', p_surf, pcols, lchnk )
        1070             :     end if
        1071     1495368 :     if (hist_fld_active('T500')) then
        1072             :       call vertinterp(ncol, pcols, pver, state%pmid, 50000._r8, state%t, p_surf, &
        1073           0 :           extrapolate='T', ps=state%ps, phis=state%phis)
        1074           0 :       call outfld('T500    ', p_surf, pcols, lchnk )
        1075             :     end if
        1076     1495368 :     if (hist_fld_active('T400')) then
        1077             :       call vertinterp(ncol, pcols, pver, state%pmid, 40000._r8, state%t, p_surf, &
        1078           0 :           extrapolate='T', ps=state%ps, phis=state%phis)
        1079           0 :       call outfld('T400    ', p_surf, pcols, lchnk )
        1080             :     end if
        1081     1495368 :     if (hist_fld_active('T300')) then
        1082           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 30000._r8, state%t, p_surf)
        1083           0 :       call outfld('T300    ', p_surf, pcols, lchnk )
        1084             :     end if
        1085     1495368 :     if (hist_fld_active('T200')) then
        1086           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 20000._r8, state%t, p_surf)
        1087           0 :       call outfld('T200    ', p_surf, pcols, lchnk )
        1088             :     end if
        1089     1495368 :     if (hist_fld_active('U850')) then
        1090           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%u, p_surf)
        1091           0 :       call outfld('U850    ', p_surf, pcols, lchnk )
        1092             :     end if
        1093     1495368 :     if (hist_fld_active('U500')) then
        1094           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 50000._r8, state%u, p_surf)
        1095           0 :       call outfld('U500    ', p_surf, pcols, lchnk )
        1096             :     end if
        1097     1495368 :     if (hist_fld_active('U250')) then
        1098           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 25000._r8, state%u, p_surf)
        1099           0 :       call outfld('U250    ', p_surf, pcols, lchnk )
        1100             :     end if
        1101     1495368 :     if (hist_fld_active('U200')) then
        1102           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 20000._r8, state%u, p_surf)
        1103           0 :       call outfld('U200    ', p_surf, pcols, lchnk )
        1104             :     end if
        1105     1495368 :     if (hist_fld_active('U010')) then
        1106           0 :       call vertinterp(ncol, pcols, pver, state%pmid,  1000._r8, state%u, p_surf)
        1107           0 :       call outfld('U010    ', p_surf, pcols, lchnk )
        1108             :     end if
        1109     1495368 :     if (hist_fld_active('V850')) then
        1110           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%v, p_surf)
        1111           0 :       call outfld('V850    ', p_surf, pcols, lchnk )
        1112             :     end if
        1113     1495368 :     if (hist_fld_active('V500')) then
        1114           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 50000._r8, state%v, p_surf)
        1115           0 :       call outfld('V500    ', p_surf, pcols, lchnk )
        1116             :     end if
        1117     1495368 :     if (hist_fld_active('V250')) then
        1118           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 25000._r8, state%v, p_surf)
        1119           0 :       call outfld('V250    ', p_surf, pcols, lchnk )
        1120             :     end if
        1121     1495368 :     if (hist_fld_active('V200')) then
        1122           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 20000._r8, state%v, p_surf)
        1123           0 :       call outfld('V200    ', p_surf, pcols, lchnk )
        1124             :     end if
        1125             :
        1126   650693736 :     ftem(:ncol,:) = state%t(:ncol,:)*state%t(:ncol,:)
        1127     1495368 :     call outfld('TT      ',ftem    ,pcols   ,lchnk   )
        1128             :     !
        1129             :     ! Output U, V, T, P and Z at bottom level
        1130             :     !
        1131     1495368 :     call outfld ('UBOT    ', state%u(1,pver)  ,  pcols, lchnk)
        1132     1495368 :     call outfld ('VBOT    ', state%v(1,pver)  ,  pcols, lchnk)
        1133     1495368 :     call outfld ('ZBOT    ', state%zm(1,pver) , pcols, lchnk)
        1134             :
        1135             :     !! Boundary layer atmospheric stability, temperature, water vapor diagnostics
        1136             :
        1137   103180392 :     p_surf_t = -99.0_r8 ! Uninitialized to impossible value
        1138             :     if  (hist_fld_active('T1000')     .or. &
        1139             :          hist_fld_active('T9251000')  .or. &
        1140             :          hist_fld_active('TH9251000') .or. &
        1141             :          hist_fld_active('T8501000')  .or. &
        1142             :          hist_fld_active('TH8501000') .or. &
        1143     1495368 :          hist_fld_active('T7001000')  .or. &
        1144             :          hist_fld_active('TH7001000')) then
        1145           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 100000._r8, state%t, p_surf_t(:,surf_100000))
        1146             :     end if
        1147             :
        1148             :     if ( hist_fld_active('T925')       .or. &
        1149     1495368 :          hist_fld_active('T9251000')   .or. &
        1150             :          hist_fld_active('TH9251000')) then
        1151           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 92500._r8, state%t, p_surf_t(:,surf_092500))
        1152             :     end if
        1153             :
        1154             : !!! at 1000 mb and 925 mb
        1155     1495368 :     if (hist_fld_active('T1000')) then
        1156           0 :       call outfld('T1000    ', p_surf_t(:,surf_100000), pcols, lchnk )
        1157             :     end if
        1158             :
        1159     1495368 :     if (hist_fld_active('T925')) then
        1160           0 :       call outfld('T925    ', p_surf_t(:,surf_092500), pcols, lchnk )
        1161             :     end if
        1162             :
        1163     1495368 :     if (hist_fld_active('T9251000')) then
        1164           0 :       p_surf = p_surf_t(:,surf_092500) - p_surf_t(:,surf_100000)
        1165           0 :       call outfld('T9251000    ', p_surf, pcols, lchnk )
        1166             :     end if
        1167             :
        1168     1495368 :     if (hist_fld_active('TH9251000')) then
        1169           0 :       p_surf = (p_surf_t(:,surf_092500)*(1000.0_r8/925.0_r8)**cappa) - (p_surf_t(:,surf_100000)*(1.0_r8)**cappa)
        1170           0 :       call outfld('TH9251000    ', p_surf, pcols, lchnk )
        1171             :     end if
        1172             :
        1173     1495368 :     if (hist_fld_active('T8501000')  .or. &
        1174             :          hist_fld_active('TH8501000')) then
        1175           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%t, p_surf_t(:,surf_085000))
        1176             :     end if
        1177             :
        1178             : !!! at 1000 mb and 850 mb
        1179     1495368 :     if (hist_fld_active('T8501000')) then
        1180           0 :       p_surf = p_surf_t(:,surf_085000)-p_surf_t(:,surf_100000)
        1181           0 :       call outfld('T8501000    ', p_surf, pcols, lchnk )
        1182             :     end if
        1183             :
        1184     1495368 :     if (hist_fld_active('TH8501000')) then
        1185           0 :       p_surf = (p_surf_t(:,surf_085000)*(1000.0_r8/850.0_r8)**cappa)-(p_surf_t(:,surf_100000)*(1.0_r8)**cappa)
        1186           0 :       call outfld('TH8501000    ', p_surf, pcols, lchnk )
        1187             :     end if
        1188             :
        1189             :     if (hist_fld_active('T7001000')  .or. &
        1190     1495368 :          hist_fld_active('TH7001000') .or. &
        1191             :          hist_fld_active('T700')) then
        1192           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 70000._r8, state%t, p_surf_t(:,surf_070000))
        1193             :     end if
        1194             :
        1195             : !!! at 700 mb
        1196     1495368 :     if (hist_fld_active('T700')) then
        1197           0 :       call outfld('T700    ', p_surf_t(:,surf_070000), pcols, lchnk )
        1198             :     end if
        1199             :
        1200             : !!! at 1000 mb and 700 mb
        1201     1495368 :     if (hist_fld_active('T7001000')) then
        1202           0 :       p_surf = p_surf_t(:,surf_070000)-p_surf_t(:,surf_100000)
        1203           0 :       call outfld('T7001000    ', p_surf, pcols, lchnk )
        1204             :     end if
        1205             :
        1206     1495368 :     if (hist_fld_active('TH7001000')) then
        1207           0 :       p_surf = (p_surf_t(:,surf_070000)*(1000.0_r8/700.0_r8)**cappa)-(p_surf_t(:,surf_100000)*(1.0_r8)**cappa)
        1208           0 :       call outfld('TH7001000    ', p_surf, pcols, lchnk )
        1209             :     end if
        1210             :
        1211     1495368 :     if (hist_fld_active('T010')) then
        1212           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 1000._r8, state%t, p_surf)
        1213           0 :       call outfld('T010           ', p_surf, pcols, lchnk )
        1214             :     end if
        1215             :
        1216             :     !---------------------------------------------------------
        1217             :     ! tidal diagnostics
        1218             :     !---------------------------------------------------------
        1219     1495368 :     call tidal_diag_write(state)
        1220             :
        1221     1495368 :     return
        1222     2990736 :   end subroutine diag_phys_writeout_dry
        1223             :
        1224             : !===============================================================================
        1225             :
        1226     1495368 :   subroutine diag_phys_writeout_moist(state, pbuf, p_surf_t)
        1227             :
        1228             :     !-----------------------------------------------------------------------
        1229             :     !
        1230             :     ! Purpose: record dynamics variables on physics grid
        1231             :     !
        1232             :     !-----------------------------------------------------------------------
        1233     1495368 :     use physconst,          only: gravit, rga, rair, cpair, latvap, rearth, cappa
        1234             :     use interpolate_data,   only: vertinterp
        1235             :     use constituent_burden, only: constituent_burden_comp
        1236             :     use co2_cycle,          only: c_i, co2_transport
        1237             :     !-----------------------------------------------------------------------
        1238             :     !
        1239             :     ! Arguments
        1240             :     !
        1241             :     type(physics_state), intent(inout) :: state
        1242             :     type(physics_buffer_desc), pointer :: pbuf(:)
        1243             :     real(r8),            intent(inout) :: p_surf_t(pcols, nsurf)  ! data interpolated to a pressure surface
        1244             :     !
        1245             :     !---------------------------Local workspace-----------------------------
        1246             :     !
        1247             :     real(r8) :: ftem(pcols,pver) ! temporary workspace
        1248             :     real(r8) :: ftem1(pcols,pver) ! another temporary workspace
        1249             :     real(r8) :: ftem2(pcols,pver) ! another temporary workspace
        1250             :     real(r8) :: p_surf(pcols)    ! data interpolated to a pressure surface
        1251             :     real(r8) :: p_surf_q1(pcols)    ! data interpolated to a pressure surface
        1252             :     real(r8) :: p_surf_q2(pcols)    ! data interpolated to a pressure surface
        1253             :     real(r8) :: tem2(pcols,pver) ! temporary workspace
        1254             :     real(r8) :: esl(pcols,pver)   ! saturation vapor pressures
        1255             :     real(r8) :: esi(pcols,pver)   !
        1256             :
        1257     1495368 :     real(r8), pointer :: ftem_ptr(:,:)
        1258             :
        1259             :     integer :: i, k, m, lchnk, ncol
        1260             :     integer :: ixq, ierr
        1261             :     !
        1262             :     !-----------------------------------------------------------------------
        1263             :     !
        1264     1495368 :     lchnk = state%lchnk
        1265     1495368 :     ncol  = state%ncol
        1266             :
        1267     1495368 :     call cnst_get_ind('Q', ixq)
        1268             :
        1269     1495368 :     if (co2_transport()) then
        1270           0 :       do m = 1,4
        1271           0 :         call outfld(trim(cnst_name(c_i(m)))//'_BOT', state%q(1,pver,c_i(m)), pcols, lchnk)
        1272             :       end do
        1273             :     end if
        1274             :
        1275             :     ! column burdens of all constituents except water vapor
        1276     1495368 :     call constituent_burden_comp(state)
        1277             :
        1278     1495368 :     call outfld('PSDRY',   state%psdry,   pcols, lchnk)
        1279     1495368 :     call outfld('PMID',    state%pmid,    pcols, lchnk)
        1280     1495368 :     call outfld('PINT',    state%pint,    pcols, lchnk)
        1281     1495368 :     call outfld('PDELDRY', state%pdeldry, pcols, lchnk)
        1282     1495368 :     call outfld('PDEL',    state%pdel,    pcols, lchnk)
        1283             :
        1284             :     !
        1285             :     ! Meridional advection fields
        1286             :     !
        1287   650693736 :     ftem(:ncol,:) = state%v(:ncol,:)*state%q(:ncol,:,ixq)
        1288     1495368 :     call outfld ('VQ      ',ftem    ,pcols   ,lchnk     )
        1289             :
        1290   650693736 :     ftem(:ncol,:) = state%q(:ncol,:,1)*state%q(:ncol,:,ixq)
        1291     1495368 :     call outfld ('QQ      ',ftem    ,pcols   ,lchnk     )
        1292             :
        1293             :     ! Vertical velocity and advection
        1294   650693736 :     ftem(:ncol,:) = state%omega(:ncol,:)*state%q(:ncol,:,ixq)
        1295     1495368 :     call outfld('OMEGAQ  ',ftem,    pcols,   lchnk     )
        1296             :     !
        1297             :     ! Mass of q, by layer and vertically integrated
        1298             :     !
        1299   650693736 :     ftem(:ncol,:) = state%q(:ncol,:,ixq) * state%pdel(:ncol,:) * rga
        1300     1495368 :     call outfld ('MQ      ',ftem    ,pcols   ,lchnk     )
        1301             :
        1302    38879568 :     do k=2,pver
        1303   625724568 :       ftem(:ncol,1) = ftem(:ncol,1) + ftem(:ncol,k)
        1304             :     end do
        1305     1495368 :     call outfld ('TMQ     ',ftem, pcols   ,lchnk     )
        1306             :     !
        1307             :     ! Integrated vapor transport calculation
        1308             :     !
        1309             :     !compute uq*dp/g and vq*dp/g
        1310   650693736 :     ftem1(:ncol,:) = state%q(:ncol,:,ixq) * state%u(:ncol,:) *state%pdel(:ncol,:) * rga
        1311   650693736 :     ftem2(:ncol,:) = state%q(:ncol,:,ixq) * state%v(:ncol,:) *state%pdel(:ncol,:) * rga
        1312             :
        1313    38879568 :     do k=2,pver
        1314   624229200 :        ftem1(:ncol,1) = ftem1(:ncol,1) + ftem1(:ncol,k)
        1315   625724568 :        ftem2(:ncol,1) = ftem2(:ncol,1) + ftem2(:ncol,k)
        1316             :     end do
        1317             :     ! compute ivt
        1318    24969168 :     ftem(:ncol,1) = sqrt( ftem1(:ncol,1)**2 + ftem2(:ncol,1)**2)
        1319             :
        1320     1495368 :     call outfld ('IVT     ',ftem, pcols   ,lchnk     )
        1321             :
        1322             :     ! output uq*dp/g
        1323     1495368 :     call outfld ('uIVT     ',ftem1, pcols   ,lchnk     )
        1324             :
        1325             :     ! output vq*dp/g
        1326     1495368 :     call outfld ('vIVT     ',ftem2, pcols   ,lchnk     )
        1327             :     !
        1328             :     ! Relative humidity
        1329             :     !
        1330     1495368 :     if (hist_fld_active('RELHUM')) then
        1331     1495368 :        if (relhum_idx > 0) then
        1332           0 :           call pbuf_get_field(pbuf, relhum_idx, ftem_ptr)
        1333           0 :           ftem(:ncol,:) = ftem_ptr(:ncol,:)
        1334             :        else
        1335    40374936 :           do k = 1, pver
        1336    40374936 :              call qsat(state%t(1:ncol,k), state%pmid(1:ncol,k), tem2(1:ncol,k), ftem(1:ncol,k), ncol)
        1337             :           end do
        1338   650693736 :           ftem(:ncol,:) = state%q(:ncol,:,ixq)/ftem(:ncol,:)*100._r8
        1339             :        end if
        1340     1495368 :        call outfld ('RELHUM  ',ftem    ,pcols   ,lchnk     )
        1341             :     end if
        1342             :
        1343     1495368 :     if (hist_fld_active('RHW') .or. hist_fld_active('RHI') .or. hist_fld_active('RHCFMIP') ) then
        1344             :
        1345             :       ! RH w.r.t liquid (water)
        1346           0 :       do k = 1, pver
        1347           0 :          call qsat_water (state%t(1:ncol,k), state%pmid(1:ncol,k), esl(1:ncol,k), ftem(1:ncol,k), ncol)
        1348             :       end do
        1349           0 :       ftem(:ncol,:) = state%q(:ncol,:,ixq)/ftem(:ncol,:)*100._r8
        1350           0 :       call outfld ('RHW  ',ftem    ,pcols   ,lchnk     )
        1351             :
        1352             :       ! Convert to RHI (ice)
        1353           0 :       do k=1,pver
        1354           0 :          call svp_ice_vect(state%t(1:ncol,k), esi(1:ncol,k), ncol)
        1355           0 :          do i=1,ncol
        1356           0 :             ftem1(i,k)=ftem(i,k)*esl(i,k)/esi(i,k)
        1357             :          end do
        1358             :       end do
        1359           0 :       call outfld ('RHI  ',ftem1    ,pcols   ,lchnk     )
        1360             :
        1361             :       ! use temperature to decide if you populate with ftem (liquid, above 0 C) or ftem1 (ice, below 0 C)
        1362             :
        1363           0 :       ftem2(:ncol,:)=ftem(:ncol,:)
        1364             :
        1365           0 :       do i=1,ncol
        1366           0 :         do k=1,pver
        1367           0 :           if (state%t(i,k) .gt. 273) then
        1368           0 :             ftem2(i,k)=ftem(i,k)  !!wrt water
        1369             :           else
        1370           0 :             ftem2(i,k)=ftem1(i,k) !!wrt ice
        1371             :           end if
        1372             :         end do
        1373             :       end do
        1374             :
        1375           0 :       call outfld ('RHCFMIP  ',ftem2    ,pcols   ,lchnk     )
        1376             :
        1377             :     end if
        1378             :     !
        1379             :     ! Output q field on pressure surfaces
        1380             :     !
        1381     1495368 :     if (hist_fld_active('Q850')) then
        1382           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%q(1,1,ixq), p_surf)
        1383           0 :       call outfld('Q850    ', p_surf, pcols, lchnk )
        1384             :     end if
        1385     1495368 :     if (hist_fld_active('Q200')) then
        1386           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 20000._r8, state%q(1,1,ixq), p_surf)
        1387           0 :       call outfld('Q200    ', p_surf, pcols, lchnk )
        1388             :     end if
        1389             :     !
        1390             :     ! Output Q at bottom level
        1391             :     !
        1392     1495368 :     call outfld ('QBOT    ', state%q(1,pver,ixq),  pcols, lchnk)
        1393             :
        1394             :     ! Total energy of the atmospheric column for atmospheric heat storage calculations
        1395             :
        1396             :     !! temporary variable to get surface geopotential in dimensions of (ncol,pver)
        1397    40374936 :     do k=1,pver
        1398   650693736 :       ftem1(:ncol,k)=state%phis(:ncol)  !! surface geopotential in units (m2/s2)
        1399             :     end do
        1400             :
        1401             :     !! calculate sum of sensible, kinetic, latent, and surface geopotential energy
        1402             :     !! E=CpT+PHIS+Lv*q+(0.5)*(u^2+v^2)
        1403     1495368 :     ftem(:ncol,:) = (cpair*state%t(:ncol,:) +  ftem1(:ncol,:) + latvap*state%q(:ncol,:,ixq) + &
        1404   652189104 :          0.5_r8*(state%u(:ncol,:)**2+state%v(:ncol,:)**2))*(state%pdel(:ncol,:)/gravit)
        1405             :     !! vertically integrate
        1406    38879568 :     do k=2,pver
        1407   625724568 :       ftem(:ncol,1) = ftem(:ncol,1) + ftem(:ncol,k)
        1408             :     end do
        1409     1495368 :     call outfld ('ATMEINT   ', ftem(:ncol,1), ncol, lchnk)
        1410             :
        1411             :     !! Boundary layer atmospheric stability, temperature, water vapor diagnostics
        1412             :
        1413             :     if ( hist_fld_active('THE9251000') .or. &
        1414     1495368 :          hist_fld_active('THE8501000') .or. &
        1415             :          hist_fld_active('THE7001000')) then
        1416           0 :       if (p_surf_t(1, surf_100000) < 0.0_r8) then
        1417           0 :         call vertinterp(ncol, pcols, pver, state%pmid, 100000._r8, state%t, p_surf_t(:, surf_100000))
        1418             :       end if
        1419             :     end if
        1420             :
        1421     1495368 :     if ( hist_fld_active('TH9251000')  .or. &
        1422             :          hist_fld_active('THE9251000')) then
        1423           0 :       if (p_surf_t(1, surf_092500) < 0.0_r8) then
        1424           0 :         call vertinterp(ncol, pcols, pver, state%pmid, 92500._r8, state%t, p_surf_t(:, surf_092500))
        1425             :       end if
        1426             :     end if
        1427             :
        1428             :     if ( hist_fld_active('Q1000')      .or. &
        1429             :          hist_fld_active('THE9251000') .or. &
        1430     1495368 :          hist_fld_active('THE8501000') .or. &
        1431             :          hist_fld_active('THE7001000')) then
        1432           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 100000._r8, state%q(1,1,ixq), p_surf_q1)
        1433             :     end if
        1434             :
        1435     1495368 :     if (hist_fld_active('THE9251000') .or. &
        1436             :         hist_fld_active('Q925')) then
        1437           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 92500._r8, state%q(1,1,ixq), p_surf_q2)
        1438             :     end if
        1439             :
        1440             : !!! at 1000 mb and 925 mb
        1441     1495368 :     if (hist_fld_active('Q1000')) then
        1442           0 :       call outfld('Q1000    ', p_surf_q1, pcols, lchnk )
        1443             :     end if
        1444             :
        1445     1495368 :     if (hist_fld_active('Q925')) then
        1446           0 :       call outfld('Q925    ', p_surf_q2, pcols, lchnk )
        1447             :     end if
        1448             :
        1449     1495368 :     if (hist_fld_active('THE9251000')) then
        1450             :       p_surf = ((p_surf_t(:, surf_092500)*(1000.0_r8/925.0_r8)**cappa) *              &
        1451             :                 exp((2500000.0_r8*p_surf_q2)/(1004.0_r8*p_surf_t(:, surf_092500)))) - &
        1452           0 :                 (p_surf_t(:,surf_100000)*(1.0_r8)**cappa)*exp((2500000.0_r8*p_surf_q1)/(1004.0_r8*p_surf_t(:,surf_100000)))
        1453           0 :       call outfld('THE9251000    ', p_surf, pcols, lchnk )
        1454             :     end if
        1455             :
        1456     1495368 :     if (hist_fld_active('THE8501000')) then
        1457           0 :       if (p_surf_t(1, surf_085000) < 0.0_r8) then
        1458           0 :         call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%t, p_surf_t(:, surf_085000))
        1459             :       end if
        1460             :     end if
        1461             :
        1462             : !!! at 1000 mb and 850 mb
        1463     1495368 :     if (hist_fld_active('THE8501000')) then
        1464           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 85000._r8, state%q(1,1,ixq), p_surf_q2)
        1465             :       p_surf = ((p_surf_t(:, surf_085000)*(1000.0_r8/850.0_r8)**cappa) *              &
        1466             :                 exp((2500000.0_r8*p_surf_q2)/(1004.0_r8*p_surf_t(:, surf_085000)))) - &
        1467           0 :                 (p_surf_t(:,surf_100000)*(1.0_r8)**cappa)*exp((2500000.0_r8*p_surf_q1)/(1004.0_r8*p_surf_t(:,surf_100000)))
        1468           0 :       call outfld('THE8501000    ', p_surf, pcols, lchnk )
        1469             :     end if
        1470             :
        1471     1495368 :     if (hist_fld_active('THE7001000')) then
        1472           0 :       if (p_surf_t(1, surf_070000) < 0.0_r8) then
        1473           0 :         call vertinterp(ncol, pcols, pver, state%pmid, 70000._r8, state%t, p_surf_t(:, surf_070000))
        1474             :       end if
        1475             :     end if
        1476             :
        1477             : !!! at 1000 mb and 700 mb
        1478     1495368 :     if (hist_fld_active('THE7001000')) then
        1479           0 :       call vertinterp(ncol, pcols, pver, state%pmid, 70000._r8, state%q(1,1,ixq), p_surf_q2)
        1480             :       p_surf = ((p_surf_t(:, surf_070000)*(1000.0_r8/700.0_r8)**cappa) *              &
        1481             :                 exp((2500000.0_r8*p_surf_q2)/(1004.0_r8*p_surf_t(:, surf_070000)))) - &
        1482           0 :                 (p_surf_t(:,surf_100000)*(1.0_r8)**cappa)*exp((2500000.0_r8*p_surf_q1)/(1004.0_r8*p_surf_t(:,surf_100000)))
        1483           0 :       call outfld('THE7001000    ', p_surf, pcols, lchnk )
        1484             :     end if
        1485             :
        1486     1495368 :     return
        1487     2990736 :   end subroutine diag_phys_writeout_moist
        1488             :
        1489             : !===============================================================================
        1490             :
        1491     1495368 :   subroutine diag_phys_writeout(state, pbuf)
        1492             :
        1493             :     !-----------------------------------------------------------------------
        1494             :     !
        1495             :     ! Arguments
        1496             :     !
        1497             :     type(physics_state), intent(inout) :: state
        1498             :     type(physics_buffer_desc), pointer :: pbuf(:)
        1499             :
        1500             :     ! Local variable
        1501             :     real(r8) :: p_surf_t(pcols, nsurf)  ! data interpolated to a pressure surface
        1502             :
        1503     1495368 :     call diag_phys_writeout_dry(state, pbuf, p_surf_t)
        1504             :
        1505     1495368 :     if (moist_physics) then
        1506     1495368 :       call diag_phys_writeout_moist(state, pbuf, p_surf_t)
        1507             :     end if
        1508             :
        1509     1495368 :   end subroutine diag_phys_writeout
        1510             :
        1511             : !===============================================================================
        1512             :
        1513           0 :   subroutine diag_clip_tend_writeout(state, ptend, ncol, lchnk, ixcldliq, ixcldice, ixq, ztodt, rtdt)
        1514             :
        1515             :     !-----------------------------------------------------------------------
        1516             :     !
        1517             :     ! Arguments
        1518             :     !
        1519             :     type(physics_state), intent(in) :: state
        1520             :     type(physics_ptend), intent(in) :: ptend
        1521             :     integer  :: ncol
        1522             :     integer  :: lchnk
        1523             :     integer  :: ixcldliq
        1524             :     integer  :: ixcldice
        1525             :     integer  :: ixq
        1526             :     real(r8) :: ztodt
        1527             :     real(r8) :: rtdt
        1528             :
        1529             :     ! Local variables
        1530             :
        1531             :     ! Debugging output to look at ice tendencies due to hard clipping negative values
        1532             :     real(r8) :: preclipice(pcols,pver)
        1533             :     real(r8) :: icecliptend(pcols,pver)
        1534             :     real(r8) :: preclipliq(pcols,pver)
        1535             :     real(r8) :: liqcliptend(pcols,pver)
        1536             :     real(r8) :: preclipvap(pcols,pver)
        1537             :     real(r8) :: vapcliptend(pcols,pver)
        1538             :
        1539             :     ! Initialize to zero
        1540           0 :     liqcliptend(:,:) = 0._r8
        1541           0 :     icecliptend(:,:) = 0._r8
        1542           0 :     vapcliptend(:,:) = 0._r8
        1543             :
        1544           0 :     preclipliq(:ncol,:) = state%q(:ncol,:,ixcldliq)+(ptend%q(:ncol,:,ixcldliq)*ztodt)
        1545           0 :     preclipice(:ncol,:) = state%q(:ncol,:,ixcldice)+(ptend%q(:ncol,:,ixcldice)*ztodt)
        1546           0 :     preclipvap(:ncol,:) = state%q(:ncol,:,ixq)+(ptend%q(:ncol,:,ixq)*ztodt)
        1547           0 :     vapcliptend(:ncol,:) = (state%q(:ncol,:,ixq)-preclipvap(:ncol,:))*rtdt
        1548           0 :     icecliptend(:ncol,:) = (state%q(:ncol,:,ixcldice)-preclipice(:ncol,:))*rtdt
        1549           0 :     liqcliptend(:ncol,:) = (state%q(:ncol,:,ixcldliq)-preclipliq(:ncol,:))*rtdt
        1550             :
        1551           0 :     call outfld('INEGCLPTEND', icecliptend, pcols, lchnk   )
        1552           0 :     call outfld('LNEGCLPTEND', liqcliptend, pcols, lchnk   )
        1553           0 :     call outfld('VNEGCLPTEND', vapcliptend, pcols, lchnk   )
        1554             :
        1555           0 :   end subroutine diag_clip_tend_writeout
        1556             :
        1557             : !===============================================================================
        1558             :
        1559     1495368 :   subroutine diag_conv(state, ztodt, pbuf)
        1560             :
        1561             :     !-----------------------------------------------------------------------
        1562             :     !
        1563             :     ! Output diagnostics associated with all convective processes.
        1564             :     !
        1565             :     !-----------------------------------------------------------------------
        1566             :     use tidal_diag,    only: get_tidal_coeffs
        1567             :
        1568             :     ! Arguments:
        1569             :
        1570             :     real(r8),            intent(in) :: ztodt   ! timestep for computing physics tendencies
        1571             :     type(physics_state), intent(in) :: state
        1572             :     type(physics_buffer_desc), pointer :: pbuf(:)
        1573             :
        1574             :     ! convective precipitation variables
        1575     1495368 :     real(r8), pointer :: prec_dp(:)                 ! total precipitation   from ZM convection
        1576     1495368 :     real(r8), pointer :: snow_dp(:)                 ! snow from ZM   convection
        1577     1495368 :     real(r8), pointer :: prec_sh(:)                 ! total precipitation   from Hack convection
        1578     1495368 :     real(r8), pointer :: snow_sh(:)                 ! snow from   Hack   convection
        1579     1495368 :     real(r8), pointer :: prec_sed(:)                ! total precipitation   from ZM convection
        1580     1495368 :     real(r8), pointer :: snow_sed(:)                ! snow from ZM   convection
        1581     1495368 :     real(r8), pointer :: prec_pcw(:)                ! total precipitation   from Hack convection
        1582     1495368 :     real(r8), pointer :: snow_pcw(:)                ! snow from Hack   convection
        1583             :
        1584             :     ! Local variables:
        1585             :
        1586             :     integer :: i, k, m, lchnk, ncol
        1587             :
        1588             :     real(r8) :: rtdt
        1589             :
        1590             :     real(r8):: precc(pcols)                ! convective precip rate
        1591             :     real(r8):: precl(pcols)                ! stratiform precip rate
        1592             :     real(r8):: snowc(pcols)                ! convective snow rate
        1593             :     real(r8):: snowl(pcols)                ! stratiform snow rate
        1594             :     real(r8):: prect(pcols)                ! total (conv+large scale) precip rate
        1595             :     real(r8) :: dcoef(6)                   ! for tidal component of T tend
        1596             :
        1597     1495368 :     lchnk = state%lchnk
        1598     1495368 :     ncol  = state%ncol
        1599             :
        1600     1495368 :     rtdt = 1._r8/ztodt
        1601             :
        1602     1495368 :     if (moist_physics) then
        1603     1495368 :       if (prec_dp_idx > 0) then
        1604     1495368 :         call pbuf_get_field(pbuf, prec_dp_idx, prec_dp)
        1605             :       else
        1606           0 :         nullify(prec_dp)
        1607             :       end if
        1608     1495368 :       if (snow_dp_idx > 0) then
        1609     1495368 :         call pbuf_get_field(pbuf, snow_dp_idx, snow_dp)
        1610             :       else
        1611           0 :         nullify(snow_dp)
        1612             :       end if
        1613     1495368 :       if (prec_sh_idx > 0) then
        1614     1495368 :         call pbuf_get_field(pbuf, prec_sh_idx, prec_sh)
        1615             :       else
        1616           0 :         nullify(prec_sh)
        1617             :       end if
        1618     1495368 :       if (snow_sh_idx > 0) then
        1619     1495368 :         call pbuf_get_field(pbuf, snow_sh_idx, snow_sh)
        1620             :       else
        1621           0 :         nullify(snow_sh)
        1622             :       end if
        1623     1495368 :       if (prec_sed_idx > 0) then
        1624     1495368 :         call pbuf_get_field(pbuf, prec_sed_idx, prec_sed)
        1625             :       else
        1626           0 :         nullify(prec_sed)
        1627             :       end if
        1628     1495368 :       if (snow_sed_idx > 0) then
        1629     1495368 :         call pbuf_get_field(pbuf, snow_sed_idx, snow_sed)
        1630             :       else
        1631           0 :         nullify(snow_sed)
        1632             :       end if
        1633     1495368 :       if (prec_pcw_idx > 0) then
        1634     1495368 :         call pbuf_get_field(pbuf, prec_pcw_idx, prec_pcw)
        1635             :       else
        1636           0 :         nullify(prec_pcw)
        1637             :       end if
        1638     1495368 :       if (snow_pcw_idx > 0) then
        1639     1495368 :         call pbuf_get_field(pbuf, snow_pcw_idx, snow_pcw)
        1640             :       else
        1641           0 :         nullify(snow_pcw)
        1642             :       end if
        1643             :
        1644             :       ! Precipitation rates (multi-process)
        1645     1495368 :       if (associated(prec_dp) .and. associated(prec_sh)) then
        1646    24969168 :         precc(:ncol) = prec_dp(:ncol)  + prec_sh(:ncol)
        1647           0 :       else if (associated(prec_dp)) then
        1648           0 :         precc(:ncol) = prec_dp(:ncol)
        1649           0 :       else if (associated(prec_sh)) then
        1650           0 :         precc(:ncol) = prec_sh(:ncol)
        1651             :       else
        1652           0 :         precc(:ncol) = 0._r8
        1653             :       end if
        1654     1495368 :       if (associated(prec_sed) .and. associated(prec_pcw)) then
        1655    24969168 :         precl(:ncol) = prec_sed(:ncol) + prec_pcw(:ncol)
        1656           0 :       else if (associated(prec_sed)) then
        1657           0 :         precl(:ncol) = prec_sed(:ncol)
        1658           0 :       else if (associated(prec_pcw)) then
        1659           0 :         precl(:ncol) = prec_pcw(:ncol)
        1660             :       else
        1661           0 :         precl(:ncol) = 0._r8
        1662             :       end if
        1663     1495368 :       if (associated(snow_dp) .and. associated(snow_sh)) then
        1664    24969168 :         snowc(:ncol) = snow_dp(:ncol)  + snow_sh(:ncol)
        1665           0 :       else if (associated(snow_dp)) then
        1666           0 :         snowc(:ncol) = snow_dp(:ncol)
        1667           0 :       else if (associated(snow_sh)) then
        1668           0 :         snowc(:ncol) = snow_sh(:ncol)
        1669             :       else
        1670           0 :         snowc(:ncol) = 0._r8
        1671             :       end if
        1672     1495368 :       if (associated(snow_sed) .and. associated(snow_pcw)) then
        1673    24969168 :         snowl(:ncol) = snow_sed(:ncol) + snow_pcw(:ncol)
        1674           0 :       else if (associated(snow_sed)) then
        1675           0 :         snowl(:ncol) = snow_sed(:ncol)
        1676           0 :       else if (associated(snow_pcw)) then
        1677           0 :         snowl(:ncol) = snow_pcw(:ncol)
        1678             :       else
        1679           0 :         snowl(:ncol) = 0._r8
        1680             :       end if
        1681    26464536 :       prect(:ncol) = precc(:ncol)    + precl(:ncol)
        1682             :
        1683     1495368 :       call outfld('PRECC   ', precc, pcols, lchnk )
        1684     1495368 :       call outfld('PRECL   ', precl, pcols, lchnk )
        1685     1495368 :       if (associated(prec_pcw)) then
        1686     1495368 :         call outfld('PREC_PCW', prec_pcw,pcols   ,lchnk )
        1687             :       end if
        1688     1495368 :       if (associated(prec_dp)) then
        1689     1495368 :         call outfld('PREC_zmc', prec_dp ,pcols   ,lchnk )
        1690             :       end if
        1691     1495368 :       call outfld('PRECSC  ', snowc, pcols, lchnk )
        1692     1495368 :       call outfld('PRECSL  ', snowl, pcols, lchnk )
        1693     1495368 :       call outfld('PRECT   ', prect, pcols, lchnk )
        1694     1495368 :       call outfld('PRECTMX ', prect, pcols, lchnk )
        1695             :
        1696     1495368 :       call outfld('PRECLav ', precl, pcols, lchnk )
        1697     1495368 :       call outfld('PRECCav ', precc, pcols, lchnk )
        1698             :
        1699     1495368 :       if (write_camiop) call outfld('Prec   ' , prect, pcols, lchnk )
        1700             :
        1701             :       ! Total convection tendencies.
        1702             :
        1703    40374936 :       do k = 1, pver
        1704   650693736 :         do i = 1, ncol
        1705   649198368 :           dtcond(i,k,lchnk) = (state%t(i,k) - dtcond(i,k,lchnk))*rtdt
        1706             :         end do
        1707             :       end do
        1708     1495368 :       call outfld('DTCOND  ', dtcond(:,:,lchnk), pcols, lchnk)
        1709             :
        1710             :       ! output tidal coefficients
        1711     1495368 :       call get_tidal_coeffs( dcoef )
        1712   650693736 :       call outfld( 'DTCOND_24_SIN', dtcond(:ncol,:,lchnk)*dcoef(1), ncol, lchnk )
        1713   650693736 :       call outfld( 'DTCOND_24_COS', dtcond(:ncol,:,lchnk)*dcoef(2), ncol, lchnk )
        1714   650693736 :       call outfld( 'DTCOND_12_SIN', dtcond(:ncol,:,lchnk)*dcoef(3), ncol, lchnk )
        1715   650693736 :       call outfld( 'DTCOND_12_COS', dtcond(:ncol,:,lchnk)*dcoef(4), ncol, lchnk )
        1716   650693736 :       call outfld( 'DTCOND_08_SIN', dtcond(:ncol,:,lchnk)*dcoef(5), ncol, lchnk )
        1717   650693736 :       call outfld( 'DTCOND_08_COS', dtcond(:ncol,:,lchnk)*dcoef(6), ncol, lchnk )
        1718             :
        1719     2990736 :       do m = 1, dqcond_num
        1720     2990736 :         if ( cnst_cam_outfld(m) ) then
        1721    40374936 :           do k = 1, pver
        1722   650693736 :             do i = 1, ncol
        1723   649198368 :               dqcond(m)%cnst(i,k,lchnk) = (state%q(i,k,m) - dqcond(m)%cnst(i,k,lchnk))*rtdt
        1724             :             end do
        1725             :           end do
        1726     1495368 :           call outfld(dcconnam(m), dqcond(m)%cnst(:,:,lchnk), pcols, lchnk)
        1727             :         end if
        1728             :       end do
        1729             :
        1730             :     end if
        1731     1495368 :   end subroutine diag_conv
        1732             :
        1733             : !===============================================================================
        1734             :
        1735     1489176 :   subroutine diag_surf (cam_in, cam_out, state, pbuf)
        1736             :
        1737             :     !-----------------------------------------------------------------------
        1738             :     !
        1739             :     ! Purpose: record surface diagnostics
        1740             :     !
        1741             :     !-----------------------------------------------------------------------
        1742             :
        1743             :     use time_manager,     only: is_end_curr_day
        1744             :     use co2_cycle,        only: c_i, co2_transport
        1745             :     use constituents,     only: sflxnam
        1746             :
        1747             :     !-----------------------------------------------------------------------
        1748             :     !
        1749             :     ! Input arguments
        1750             :     !
        1751             :     type(cam_in_t),  intent(in) :: cam_in
        1752             :     type(cam_out_t), intent(in) :: cam_out
        1753             :     type(physics_state), intent(in)    :: state
        1754             :     type(physics_buffer_desc), pointer :: pbuf(:)
        1755             :     !
        1756             :     !---------------------------Local workspace-----------------------------
        1757             :     !
        1758             :     integer :: i, k, m      ! indexes
        1759             :     integer :: lchnk        ! chunk identifier
        1760             :     integer :: ncol         ! longitude dimension
        1761             :     real(r8) tem2(pcols)    ! temporary workspace
        1762             :     real(r8) ftem(pcols)    ! temporary workspace
        1763             :
        1764     1489176 :     real(r8), pointer :: trefmnav(:) ! daily minimum tref
        1765     1489176 :     real(r8), pointer :: trefmxav(:) ! daily maximum tref
        1766             :
        1767             :     !
        1768             :     !-----------------------------------------------------------------------
        1769             :     !
        1770     1489176 :     lchnk = cam_in%lchnk
        1771     1489176 :     ncol  = cam_in%ncol
        1772             :
        1773     1489176 :     if (moist_physics) then
        1774     1489176 :       call outfld('SHFLX',    cam_in%shf,       pcols, lchnk)
        1775     1489176 :       call outfld('LHFLX',    cam_in%lhf,       pcols, lchnk)
        1776     1489176 :       call outfld('QFLX',     cam_in%cflx(1,1), pcols, lchnk)
        1777             :
        1778     1489176 :       call outfld('TAUX',     cam_in%wsx,       pcols, lchnk)
        1779     1489176 :       call outfld('TAUY',     cam_in%wsy,       pcols, lchnk)
        1780     1489176 :       call outfld('TREFHT  ', cam_in%tref,      pcols, lchnk)
        1781     1489176 :       call outfld('TREFHTMX', cam_in%tref,      pcols, lchnk)
        1782     1489176 :       call outfld('TREFHTMN', cam_in%tref,      pcols, lchnk)
        1783     1489176 :       call outfld('QREFHT',   cam_in%qref,      pcols, lchnk)
        1784     1489176 :       call outfld('U10',      cam_in%u10,       pcols, lchnk)
        1785     1489176 :       call outfld('UGUST',    cam_in%ugustOut,  pcols, lchnk)
        1786     1489176 :       call outfld('U10WITHGUSTS',cam_in%u10withGusts, pcols, lchnk)
        1787             :
        1788             :       !
        1789             :       ! Calculate and output reference height RH (RHREFHT)
        1790     1489176 :       call qsat(cam_in%tref(1:ncol), state%ps(1:ncol), tem2(1:ncol), ftem(1:ncol), ncol)
        1791    24865776 :       ftem(:ncol) = cam_in%qref(:ncol)/ftem(:ncol)*100._r8
        1792             :
        1793             :
        1794     1489176 :       call outfld('RHREFHT',   ftem,      pcols, lchnk)
        1795             :
        1796             :
        1797     1489176 :       if (write_camiop) then
        1798           0 :          call outfld('shflx   ',cam_in%shf,   pcols,   lchnk)
        1799           0 :          call outfld('lhflx   ',cam_in%lhf,   pcols,   lchnk)
        1800           0 :          call outfld('trefht  ',cam_in%tref,  pcols,   lchnk)
        1801           0 :          call outfld('Tg', cam_in%ts, pcols, lchnk)
        1802           0 :          call outfld('Tsair',cam_in%ts, pcols, lchnk)
        1803             :       end if
        1804             :       !
        1805             :       ! Ouput ocn and ice fractions
        1806             :       !
        1807     1489176 :       call outfld('LANDFRAC', cam_in%landfrac, pcols, lchnk)
        1808     1489176 :       call outfld('ICEFRAC',  cam_in%icefrac,  pcols, lchnk)
        1809     1489176 :       call outfld('OCNFRAC',  cam_in%ocnfrac,  pcols, lchnk)
        1810             :       !
        1811             :       ! Compute daily minimum and maximum of TREF
        1812             :       !
        1813     1489176 :       call pbuf_get_field(pbuf, trefmxav_idx, trefmxav)
        1814     1489176 :       call pbuf_get_field(pbuf, trefmnav_idx, trefmnav)
        1815    24865776 :       do i = 1,ncol
        1816    23376600 :         trefmxav(i) = max(cam_in%tref(i),trefmxav(i))
        1817    24865776 :         trefmnav(i) = min(cam_in%tref(i),trefmnav(i))
        1818             :       end do
        1819     1489176 :       if (is_end_curr_day()) then
        1820       34056 :         call outfld('TREFMXAV', trefmxav,pcols,   lchnk     )
        1821       34056 :         call outfld('TREFMNAV', trefmnav,pcols,   lchnk     )
        1822      568656 :         trefmxav(:ncol) = -1.0e36_r8
        1823      568656 :         trefmnav(:ncol) =  1.0e36_r8
        1824             :       endif
        1825             :
        1826     1489176 :       call outfld('TBOT',     cam_out%tbot,     pcols, lchnk)
        1827     1489176 :       call outfld('TS',       cam_in%ts,        pcols, lchnk)
        1828     1489176 :       call outfld('TSMN',     cam_in%ts,        pcols, lchnk)
        1829     1489176 :       call outfld('TSMX',     cam_in%ts,        pcols, lchnk)
        1830     1489176 :       call outfld('SNOWHLND', cam_in%snowhland, pcols, lchnk)
        1831     1489176 :       call outfld('SNOWHICE', cam_in%snowhice,  pcols, lchnk)
        1832     1489176 :       call outfld('ASDIR',    cam_in%asdir,     pcols, lchnk)
        1833     1489176 :       call outfld('ASDIF',    cam_in%asdif,     pcols, lchnk)
        1834     1489176 :       call outfld('ALDIR',    cam_in%aldir,     pcols, lchnk)
        1835     1489176 :       call outfld('ALDIF',    cam_in%aldif,     pcols, lchnk)
        1836     1489176 :       call outfld('SST',      cam_in%sst,       pcols, lchnk)
        1837             :
        1838     1489176 :       if (co2_transport()) then
        1839           0 :         do m = 1,4
        1840           0 :           call outfld(sflxnam(c_i(m)), cam_in%cflx(:,c_i(m)), pcols, lchnk)
        1841             :         end do
        1842             :       end if
        1843             :     end if
        1844             :
        1845     2978352 :   end subroutine diag_surf
        1846             :
        1847             : !===============================================================================
        1848             :
        1849     1495368 :   subroutine diag_export(cam_out)
        1850             :
        1851             :     !-----------------------------------------------------------------------
        1852             :     !
        1853             :     ! Purpose: Write export state to history file
        1854             :     !
        1855             :     !-----------------------------------------------------------------------
        1856             :
        1857             :     ! arguments
        1858             :     type(cam_out_t), intent(inout) :: cam_out
        1859             :
        1860             :     ! Local variables:
        1861             :     integer :: lchnk        ! chunk identifier
        1862             :     logical :: atm_dep_flux ! true ==> sending deposition fluxes to coupler.
        1863             :     ! Otherwise, set them to zero.
        1864             :     !-----------------------------------------------------------------------
        1865             :
        1866     1495368 :     lchnk = cam_out%lchnk
        1867             :
        1868     1495368 :     call phys_getopts(atm_dep_flux_out=atm_dep_flux)
        1869             :
        1870     1495368 :     if (.not. atm_dep_flux) then
        1871             :       ! set the fluxes to zero before outfld and sending them to the
        1872             :       ! coupler
        1873    25421256 :       cam_out%bcphiwet = 0.0_r8
        1874    25421256 :       cam_out%bcphidry = 0.0_r8
        1875    25421256 :       cam_out%bcphodry = 0.0_r8
        1876    25421256 :       cam_out%ocphiwet = 0.0_r8
        1877    25421256 :       cam_out%ocphidry = 0.0_r8
        1878    25421256 :       cam_out%ocphodry = 0.0_r8
        1879    25421256 :       cam_out%dstwet1  = 0.0_r8
        1880    25421256 :       cam_out%dstdry1  = 0.0_r8
        1881    25421256 :       cam_out%dstwet2  = 0.0_r8
        1882    25421256 :       cam_out%dstdry2  = 0.0_r8
        1883    25421256 :       cam_out%dstwet3  = 0.0_r8
        1884    25421256 :       cam_out%dstdry3  = 0.0_r8
        1885    25421256 :       cam_out%dstwet4  = 0.0_r8
        1886    25421256 :       cam_out%dstdry4  = 0.0_r8
        1887             :     end if
        1888             :
        1889     1495368 :     if (moist_physics) then
        1890     1495368 :       call outfld('a2x_BCPHIWET', cam_out%bcphiwet, pcols, lchnk)
        1891     1495368 :       call outfld('a2x_BCPHIDRY', cam_out%bcphidry, pcols, lchnk)
        1892     1495368 :       call outfld('a2x_BCPHODRY', cam_out%bcphodry, pcols, lchnk)
        1893     1495368 :       call outfld('a2x_OCPHIWET', cam_out%ocphiwet, pcols, lchnk)
        1894     1495368 :       call outfld('a2x_OCPHIDRY', cam_out%ocphidry, pcols, lchnk)
        1895     1495368 :       call outfld('a2x_OCPHODRY', cam_out%ocphodry, pcols, lchnk)
        1896     1495368 :       call outfld('a2x_DSTWET1',  cam_out%dstwet1,  pcols, lchnk)
        1897     1495368 :       call outfld('a2x_DSTDRY1',  cam_out%dstdry1,  pcols, lchnk)
        1898     1495368 :       call outfld('a2x_DSTWET2',  cam_out%dstwet2,  pcols, lchnk)
        1899     1495368 :       call outfld('a2x_DSTDRY2',  cam_out%dstdry2,  pcols, lchnk)
        1900     1495368 :       call outfld('a2x_DSTWET3',  cam_out%dstwet3,  pcols, lchnk)
        1901     1495368 :       call outfld('a2x_DSTDRY3',  cam_out%dstdry3,  pcols, lchnk)
        1902     1495368 :       call outfld('a2x_DSTWET4',  cam_out%dstwet4,  pcols, lchnk)
        1903     1495368 :       call outfld('a2x_DSTDRY4',  cam_out%dstdry4,  pcols, lchnk)
        1904             :     end if
        1905             :
        1906     1489176 :   end subroutine diag_export
        1907             :
        1908             : !#######################################################################
        1909             :
        1910     1495368 :   subroutine diag_physvar_ic (lchnk,  pbuf, cam_out, cam_in)
        1911             :     !
        1912             :     !---------------------------------------------
        1913             :     !
        1914             :     ! Purpose: record physics variables on IC file
        1915             :     !
        1916             :     !---------------------------------------------
        1917             :     !
        1918             :
        1919             :     !
        1920             :     ! Arguments
        1921             :     !
        1922             :     integer       , intent(in) :: lchnk  ! chunk identifier
        1923             :     type(physics_buffer_desc), pointer :: pbuf(:)
        1924             :
        1925             :     type(cam_out_t), intent(inout) :: cam_out
        1926             :     type(cam_in_t),  intent(inout) :: cam_in
        1927             :     !
        1928             :     !---------------------------Local workspace-----------------------------
        1929             :     !
        1930             :     integer  :: itim_old          ! indices
        1931             :
        1932     1495368 :     real(r8), pointer, dimension(:,:) :: cwat_var
        1933     1495368 :     real(r8), pointer, dimension(:,:) :: conv_var_3d
        1934     1495368 :     real(r8), pointer, dimension(:  ) :: conv_var_2d
        1935     1495368 :     real(r8), pointer :: tpert(:), pblh(:), qpert(:)
        1936             :     !
        1937             :     !-----------------------------------------------------------------------
        1938             :     !
        1939     1495368 :     if( write_inithist() .and. moist_physics ) then
        1940             :
        1941             :       !
        1942             :       ! Associate pointers with physics buffer fields
        1943             :       !
        1944           0 :       itim_old = pbuf_old_tim_idx()
        1945             :
        1946           0 :       if (qcwat_idx > 0) then
        1947           0 :         call pbuf_get_field(pbuf, qcwat_idx, cwat_var, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
        1948           0 :         call outfld('QCWAT&IC   ',cwat_var, pcols,lchnk)
        1949             :       end if
        1950             :
        1951           0 :       if (tcwat_idx > 0) then
        1952           0 :         call pbuf_get_field(pbuf, tcwat_idx,  cwat_var, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
        1953           0 :         call outfld('TCWAT&IC   ',cwat_var, pcols,lchnk)
        1954             :       end if
        1955             :
        1956           0 :       if (lcwat_idx > 0) then
        1957           0 :         call pbuf_get_field(pbuf, lcwat_idx,  cwat_var, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
        1958           0 :         call outfld('LCWAT&IC   ',cwat_var, pcols,lchnk)
        1959             :       end if
        1960             :
        1961           0 :       if (cld_idx > 0) then
        1962           0 :         call pbuf_get_field(pbuf, cld_idx,    cwat_var, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
        1963           0 :         call outfld('CLOUD&IC   ',cwat_var, pcols,lchnk)
        1964             :       end if
        1965             :
        1966           0 :       if (concld_idx > 0) then
        1967           0 :         call pbuf_get_field(pbuf, concld_idx, cwat_var, start=(/1,1,itim_old/), kount=(/pcols,pver,1/) )
        1968           0 :         call outfld('CONCLD&IC   ',cwat_var, pcols,lchnk)
        1969             :       end if
        1970             :
        1971           0 :       if (cush_idx > 0) then
        1972           0 :         call pbuf_get_field(pbuf, cush_idx, conv_var_2d ,(/1,itim_old/),  (/pcols,1/))
        1973           0 :         call outfld('CUSH&IC   ',conv_var_2d, pcols,lchnk)
        1974             :
        1975             :       end if
        1976             :
        1977           0 :       if (tke_idx > 0) then
        1978           0 :         call pbuf_get_field(pbuf, tke_idx, conv_var_3d)
        1979           0 :         call outfld('TKE&IC    ',conv_var_3d, pcols,lchnk)
        1980             :       end if
        1981             :
        1982           0 :       if (kvm_idx > 0) then
        1983           0 :         call pbuf_get_field(pbuf, kvm_idx,  conv_var_3d)
        1984           0 :         call outfld('KVM&IC    ',conv_var_3d, pcols,lchnk)
        1985             :       end if
        1986             :
        1987           0 :       if (kvh_idx > 0) then
        1988           0 :         call pbuf_get_field(pbuf, kvh_idx,  conv_var_3d)
        1989           0 :         call outfld('KVH&IC    ',conv_var_3d, pcols,lchnk)
        1990             :       end if
        1991             :
        1992           0 :       if (qpert_idx > 0) then
        1993           0 :         call pbuf_get_field(pbuf, qpert_idx, qpert)
        1994           0 :         call outfld('QPERT&IC   ', qpert, pcols, lchnk)
        1995             :       end if
        1996             :
        1997           0 :       if (pblh_idx > 0) then
        1998           0 :         call pbuf_get_field(pbuf, pblh_idx,  pblh)
        1999           0 :         call outfld('PBLH&IC    ', pblh,  pcols, lchnk)
        2000             :       end if
        2001             :
        2002           0 :       if (tpert_idx > 0) then
        2003           0 :         call pbuf_get_field(pbuf, tpert_idx, tpert)
        2004           0 :         call outfld('TPERT&IC   ', tpert, pcols, lchnk)
        2005             :       end if
        2006             :
        2007             :     end if
        2008             :
        2009     1495368 :   end subroutine diag_physvar_ic
        2010             :
        2011             :
        2012             : !#######################################################################
        2013             :
        2014     1489176 :   subroutine diag_phys_tend_writeout_dry(state, pbuf,  tend, ztodt)
        2015             :
        2016             :     !---------------------------------------------------------------
        2017             :     !
        2018             :     ! Purpose:  Dump physics tendencies for temperature
        2019             :     !
        2020             :     !---------------------------------------------------------------
        2021             :
        2022             :     use check_energy,    only: check_energy_get_integrals
        2023             :     use physconst,       only: cpair
        2024             :
        2025             :     ! Arguments
        2026             :
        2027             :     type(physics_state), intent(in)    :: state
        2028             :
        2029             :     type(physics_buffer_desc), pointer :: pbuf(:)
        2030             :     type(physics_tend ), intent(in)    :: tend
        2031             :     real(r8),            intent(in)    :: ztodt             ! physics timestep
        2032             :
        2033             :     !---------------------------Local workspace-----------------------------
        2034             :
        2035             :     integer  :: lchnk             ! chunk index
        2036             :     integer  :: ncol              ! number of columns in chunk
        2037             :     real(r8) :: ftem2(pcols)      ! Temporary workspace for outfld variables
        2038             :     real(r8) :: ftem3(pcols,pver) ! Temporary workspace for outfld variables
        2039             :     real(r8) :: heat_glob         ! global energy integral (FV only)
        2040             :     ! CAM pointers to get variables from the physics buffer
        2041     1489176 :     real(r8), pointer, dimension(:,:) :: t_ttend
        2042     1489176 :     real(r8), pointer, dimension(:,:) :: t_utend
        2043     1489176 :     real(r8), pointer, dimension(:,:) :: t_vtend
        2044             :     integer  :: itim_old,m
        2045             :
        2046             :     !-----------------------------------------------------------------------
        2047             :
        2048     1489176 :     lchnk = state%lchnk
        2049     1489176 :     ncol  = state%ncol
        2050             :
        2051             :     ! Dump out post-physics state (FV only)
        2052             :
        2053     1489176 :     call outfld('TAP', state%t, pcols, lchnk   )
        2054     1489176 :     call outfld('UAP', state%u, pcols, lchnk   )
        2055     1489176 :     call outfld('VAP', state%v, pcols, lchnk   )
        2056             :
        2057             :     ! Total physics tendency for Temperature
        2058             :     ! (remove global fixer tendency from total for FV and SE dycores)
        2059             :
        2060     1489176 :     if (.not.dycore_is('EUL')) then
        2061     1489176 :       call check_energy_get_integrals( heat_glob_out=heat_glob )
        2062    24865776 :       ftem2(:ncol)  = heat_glob/cpair
        2063     1489176 :       call outfld('TFIX', ftem2, pcols, lchnk   )
        2064   647999352 :       ftem3(:ncol,:pver)  = tend%dtdt(:ncol,:pver) - heat_glob/cpair
        2065             :     else
        2066           0 :       ftem3(:ncol,:pver)  = tend%dtdt(:ncol,:pver)
        2067             :     end if
        2068     1489176 :     call outfld('PTTEND',ftem3, pcols, lchnk )
        2069   647999352 :     ftem3(:ncol,:pver)  = tend%dudt(:ncol,:pver)
        2070     1489176 :     call outfld('UTEND_PHYSTOT',ftem3, pcols, lchnk )
        2071   647999352 :     ftem3(:ncol,:pver)  = tend%dvdt(:ncol,:pver)
        2072     1489176 :     call outfld('VTEND_PHYSTOT',ftem3, pcols, lchnk )
        2073             :
        2074             :     ! Total (physics+dynamics, everything!) tendency for Temperature
        2075             :
        2076             :     !! get temperature, U, and V stored in physics buffer
        2077     1489176 :     itim_old = pbuf_old_tim_idx()
        2078     5956704 :     call pbuf_get_field(pbuf, t_ttend_idx, t_ttend, start=(/1,1,itim_old/), kount=(/pcols,pver,1/))
        2079     5956704 :     call pbuf_get_field(pbuf, t_utend_idx, t_utend, start=(/1,1,itim_old/), kount=(/pcols,pver,1/))
        2080     5956704 :     call pbuf_get_field(pbuf, t_vtend_idx, t_vtend, start=(/1,1,itim_old/), kount=(/pcols,pver,1/))
        2081             :
        2082             :     !! calculate and outfld the total temperature, U, and V tendencies
        2083   647999352 :     ftem3(:ncol,:) = (state%t(:ncol,:) - t_ttend(:ncol,:))/ztodt
        2084     1489176 :     call outfld('TTEND_TOT', ftem3, pcols, lchnk)
        2085   647999352 :     ftem3(:ncol,:) = (state%u(:ncol,:) - t_utend(:ncol,:))/ztodt
        2086     1489176 :     call outfld('UTEND_TOT', ftem3, pcols, lchnk)
        2087   647999352 :     ftem3(:ncol,:) = (state%v(:ncol,:) - t_vtend(:ncol,:))/ztodt
        2088     1489176 :     call outfld('VTEND_TOT', ftem3, pcols, lchnk)
        2089             :
        2090             :     !! update physics buffer with this time-step's temperature, U, and V
        2091   647999352 :     t_ttend(:ncol,:) = state%t(:ncol,:)
        2092   647999352 :     t_utend(:ncol,:) = state%u(:ncol,:)
        2093   647999352 :     t_vtend(:ncol,:) = state%v(:ncol,:)
        2094             :
        2095     2978352 :   end subroutine diag_phys_tend_writeout_dry
        2096             :
        2097             : !#######################################################################
        2098             :
        2099     1489176 :   subroutine diag_phys_tend_writeout_moist(state, pbuf,  tend, ztodt,         &
        2100             :        qini, cldliqini, cldiceini)
        2101             :
        2102             :     !---------------------------------------------------------------
        2103             :     !
        2104             :     ! Purpose:  Dump physics tendencies for moisture
        2105             :     !
        2106             :     !---------------------------------------------------------------
        2107             :
        2108             :     ! Arguments
        2109             :
        2110             :     type(physics_state), intent(in)    :: state
        2111             :
        2112             :     type(physics_buffer_desc), pointer :: pbuf(:)
        2113             :     type(physics_tend ), intent(in)    :: tend
        2114             :     real(r8),            intent(in)    :: ztodt                  ! physics timestep
        2115             :     real(r8),            intent(in)    :: qini      (pcols,pver) ! tracer fields at beginning of physics
        2116             :     real(r8),            intent(in)    :: cldliqini (pcols,pver) ! tracer fields at beginning of physics
        2117             :     real(r8),            intent(in)    :: cldiceini (pcols,pver) ! tracer fields at beginning of physics
        2118             :
        2119             :     !---------------------------Local workspace-----------------------------
        2120             :
        2121             :     integer  :: lchnk  ! chunk index
        2122             :     integer  :: ncol   ! number of columns in chunk
        2123             :     real(r8) :: ftem3(pcols,pver) ! Temporary workspace for outfld variables
        2124             :     real(r8) :: rtdt
        2125             :     integer  :: ixcldice, ixcldliq! constituent indices for cloud liquid and ice water.
        2126             :
        2127     1489176 :     lchnk = state%lchnk
        2128     1489176 :     ncol  = state%ncol
        2129     1489176 :     rtdt  = 1._r8/ztodt
        2130     1489176 :     call cnst_get_ind('CLDLIQ', ixcldliq, abort=.false.)
        2131     1489176 :     call cnst_get_ind('CLDICE', ixcldice, abort=.false.)
        2132             :
        2133     1489176 :     if ( cnst_cam_outfld(       1) ) then
        2134     1489176 :       call outfld (apcnst(       1), state%q(1,1,       1), pcols, lchnk)
        2135             :     end if
        2136     1489176 :     if (ixcldliq > 0) then
        2137     1489176 :       if (cnst_cam_outfld(ixcldliq)) then
        2138     1489176 :         call outfld (apcnst(ixcldliq), state%q(1,1,ixcldliq), pcols, lchnk)
        2139             :       end if
        2140             :     end if
        2141     1489176 :     if (ixcldice > 0) then
        2142     1489176 :       if ( cnst_cam_outfld(ixcldice) ) then
        2143     1489176 :         call outfld (apcnst(ixcldice), state%q(1,1,ixcldice), pcols, lchnk)
        2144             :       end if
        2145             :     end if
        2146             :
        2147             :     ! Total physics tendency for moisture and other tracers
        2148             :
        2149     1489176 :     if ( cnst_cam_outfld(       1) ) then
        2150   647999352 :       ftem3(:ncol,:pver) = (state%q(:ncol,:pver,       1) - qini     (:ncol,:pver) )*rtdt
        2151     1489176 :       call outfld (ptendnam(       1), ftem3, pcols, lchnk)
        2152             :     end if
        2153     1489176 :     if (ixcldliq > 0) then
        2154     1489176 :       if (cnst_cam_outfld(ixcldliq) ) then
        2155   647999352 :         ftem3(:ncol,:pver) = (state%q(:ncol,:pver,ixcldliq) - cldliqini(:ncol,:pver) )*rtdt
        2156     1489176 :         call outfld (ptendnam(ixcldliq), ftem3, pcols, lchnk)
        2157             :       end if
        2158             :     end if
        2159     1489176 :     if (ixcldice > 0) then
        2160     1489176 :       if ( cnst_cam_outfld(ixcldice) ) then
        2161   647999352 :         ftem3(:ncol,:pver) = (state%q(:ncol,:pver,ixcldice) - cldiceini(:ncol,:pver) )*rtdt
        2162     1489176 :         call outfld (ptendnam(ixcldice), ftem3, pcols, lchnk)
        2163             :       end if
        2164             :     end if
        2165             :
        2166     1489176 :   end subroutine diag_phys_tend_writeout_moist
        2167             :
        2168             : !#######################################################################
        2169             :
        2170     1489176 :   subroutine diag_phys_tend_writeout(state, pbuf,  tend, ztodt,               &
        2171             :        qini, cldliqini, cldiceini)
        2172             :
        2173             :     !---------------------------------------------------------------
        2174             :     !
        2175             :     ! Purpose:  Dump physics tendencies for moisture and temperature
        2176             :     !
        2177             :     !---------------------------------------------------------------
        2178             :
        2179             :     ! Arguments
        2180             :
        2181             :     type(physics_state), intent(in)    :: state
        2182             :
        2183             :     type(physics_buffer_desc), pointer :: pbuf(:)
        2184             :     type(physics_tend ), intent(in)    :: tend
        2185             :     real(r8),            intent(in)    :: ztodt                  ! physics timestep
        2186             :     real(r8),            intent(in)    :: qini      (pcols,pver) ! tracer fields at beginning of physics
        2187             :     real(r8),            intent(in)    :: cldliqini (pcols,pver) ! tracer fields at beginning of physics
        2188             :     real(r8),            intent(in)    :: cldiceini (pcols,pver) ! tracer fields at beginning of physics
        2189             :
        2190             :     !-----------------------------------------------------------------------
        2191             :
        2192     1489176 :     call diag_phys_tend_writeout_dry(state, pbuf, tend, ztodt)
        2193     1489176 :     if (moist_physics) then
        2194             :       call diag_phys_tend_writeout_moist(state, pbuf,  tend, ztodt,           &
        2195     1489176 :            qini, cldliqini, cldiceini)
        2196             :     end if
        2197             :
        2198     1489176 :   end subroutine diag_phys_tend_writeout
        2199             :
        2200             : !#######################################################################
        2201             :
        2202     1495368 :   subroutine diag_state_b4_phys_write_dry (state)
        2203             :     !
        2204             :     !---------------------------------------------------------------
        2205             :     !
        2206             :     ! Purpose:  Dump dry state just prior to executing physics
        2207             :     !
        2208             :     !---------------------------------------------------------------
        2209             :     !
        2210             :     ! Arguments
        2211             :     !
        2212             :     type(physics_state), intent(in) :: state
        2213             :     !
        2214             :     !---------------------------Local workspace-----------------------------
        2215             :     !
        2216             :     integer :: lchnk              ! chunk index
        2217             :     !
        2218             :     !-----------------------------------------------------------------------
        2219             :     !
        2220     1495368 :     lchnk = state%lchnk
        2221             :
        2222     1495368 :     call outfld('TBP', state%t, pcols, lchnk   )
        2223     1495368 :     call outfld('UBP', state%u, pcols, lchnk   )
        2224     1495368 :     call outfld('VBP', state%v, pcols, lchnk   )
        2225             :
        2226     1495368 :   end subroutine diag_state_b4_phys_write_dry
        2227             :
        2228     1495368 :   subroutine diag_state_b4_phys_write_moist (state)
        2229             :     !
        2230             :     !---------------------------------------------------------------
        2231             :     !
        2232             :     ! Purpose:  Dump moist state just prior to executing physics
        2233             :     !
        2234             :     !---------------------------------------------------------------
        2235             :     !
        2236             :     ! Arguments
        2237             :     !
        2238             :     type(physics_state), intent(in) :: state
        2239             :     !
        2240             :     !---------------------------Local workspace-----------------------------
        2241             :     !
        2242             :     integer :: ixcldice, ixcldliq ! constituent indices for cloud liquid and ice water.
        2243             :     integer :: lchnk              ! chunk index
        2244             :     !
        2245             :     !-----------------------------------------------------------------------
        2246             :     !
        2247     1495368 :     lchnk = state%lchnk
        2248             :
        2249     1495368 :     call cnst_get_ind('CLDLIQ', ixcldliq, abort=.false.)
        2250     1495368 :     call cnst_get_ind('CLDICE', ixcldice, abort=.false.)
        2251             :
        2252     1495368 :     if ( cnst_cam_outfld(       1) ) then
        2253     1495368 :       call outfld (bpcnst(       1), state%q(1,1,       1), pcols, lchnk)
        2254             :     end if
        2255     1495368 :     if (ixcldliq > 0) then
        2256     1495368 :       if (cnst_cam_outfld(ixcldliq)) then
        2257     1495368 :         call outfld (bpcnst(ixcldliq), state%q(1,1,ixcldliq), pcols, lchnk)
        2258             :       end if
        2259             :     end if
        2260     1495368 :     if (ixcldice > 0) then
        2261     1495368 :       if (cnst_cam_outfld(ixcldice)) then
        2262     1495368 :         call outfld (bpcnst(ixcldice), state%q(1,1,ixcldice), pcols, lchnk)
        2263             :       end if
        2264             :     end if
        2265             :
        2266     1495368 :   end subroutine diag_state_b4_phys_write_moist
        2267             :
        2268     1495368 :   subroutine diag_state_b4_phys_write (state)
        2269             :     !
        2270             :     !---------------------------------------------------------------
        2271             :     !
        2272             :     ! Purpose:  Dump state just prior to executing physics
        2273             :     !
        2274             :     !---------------------------------------------------------------
        2275             :     !
        2276             :     ! Arguments
        2277             :     !
        2278             :     type(physics_state), intent(in) :: state
        2279             :     !
        2280             :
        2281     1495368 :     call diag_state_b4_phys_write_dry(state)
        2282     1495368 :     if (moist_physics) then
        2283     1495368 :       call diag_state_b4_phys_write_moist(state)
        2284             :     end if
        2285     1495368 :   end subroutine diag_state_b4_phys_write
        2286             :
        2287           0 : end module cam_diagnostics

Generated by: LCOV version 1.14