LCOV - code coverage report
Current view: | top level - chemistry/aerosol - soil_erod_mod.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 0 | 45 | 0.0 %
Date: | 2025-01-13 21:54:50 |  | Functions: | 0 | 1 | 0.0 %

              Line data    Source code
           1             : !===============================================================================
           2             : !===============================================================================
           3             : module soil_erod_mod
           4             :   use shr_kind_mod,     only: r8 => shr_kind_r8, cl => shr_kind_cl
           5             :   use cam_logfile,      only: iulog
           6             :   use spmd_utils,       only: masterproc
           7             :   use cam_abortutils,   only: endrun
           8             :
           9             :   implicit none
          10             :   private
          11             :
          12             :   public :: soil_erod_init
          13             :   public :: soil_erodibility
          14             :   public :: soil_erod_fact
          15             :
          16             :   real(r8), allocatable ::  soil_erodibility(:,:)  ! soil erodibility factor
          17             :   real(r8) :: soil_erod_fact                       ! tuning parameter for dust emissions
          18             :
          19             : contains
          20             :
          21             :   !=============================================================================
          22             :   !=============================================================================
          23           0 :   subroutine soil_erod_init( dust_emis_fact, soil_erod_file )
          24             :     use interpolate_data, only: lininterp_init, lininterp, lininterp_finish, interp_type
          25             :     use ppgrid,           only: begchunk, endchunk, pcols
          26             :     use mo_constants,     only: pi, d2r
          27             :     use pio,              only: file_desc_t,pio_inq_dimid,pio_inq_dimlen,pio_get_var,pio_inq_varid, PIO_NOWRITE
          28             :     use phys_grid,        only: get_ncols_p, get_rlat_all_p, get_rlon_all_p
          29             :     use cam_pio_utils,    only: cam_pio_openfile
          30             :     use ioFileMod,        only: getfil
          31             :
          32             :     real(r8),         intent(in) :: dust_emis_fact
          33             :     character(len=*), intent(in) :: soil_erod_file
          34             :
          35           0 :     real(r8), allocatable ::  soil_erodibility_in(:,:)  ! temporary input array
          36           0 :     real(r8), allocatable :: dst_lons(:)
          37           0 :     real(r8), allocatable :: dst_lats(:)
          38             :     character(len=cl)     :: infile
          39             :     integer :: did, vid, nlat, nlon
          40             :     type(file_desc_t) :: ncid
          41             :
          42             :     type(interp_type) :: lon_wgts, lat_wgts
          43             :     real(r8) :: to_lats(pcols), to_lons(pcols)
          44             :     integer :: c, ncols, ierr
          45             :     real(r8), parameter :: zero=0._r8, twopi=2._r8*pi
          46             :
          47           0 :     soil_erod_fact = dust_emis_fact
          48             :
          49             :     ! Summary to log file
          50           0 :     if (masterproc) then
          51           0 :        write(iulog,*) 'soil_erod_mod: soil erodibility dataset: ', trim(soil_erod_file)
          52           0 :        write(iulog,*) 'soil_erod_mod: soil_erod_fact = ', soil_erod_fact
          53             :     end if
          54             :
          55             :     ! for soil erodibility in mobilization, apply inside CAM instead of lsm.
          56             :     ! read in soil erodibility factors, similar to Zender's boundary conditions
          57             :
          58             :     ! Get file name.
          59           0 :     call getfil(soil_erod_file, infile, 0)
          60           0 :     call cam_pio_openfile (ncid, trim(infile), PIO_NOWRITE)
          61             :
          62             :     ! Get input data resolution.
          63           0 :     ierr = pio_inq_dimid( ncid, 'lon', did )
          64           0 :     ierr = pio_inq_dimlen( ncid, did, nlon )
          65             :
          66           0 :     ierr = pio_inq_dimid( ncid, 'lat', did )
          67           0 :     ierr = pio_inq_dimlen( ncid, did, nlat )
          68             :
          69           0 :     allocate(dst_lons(nlon))
          70           0 :     allocate(dst_lats(nlat))
          71           0 :     allocate(soil_erodibility_in(nlon,nlat))
          72             :
          73           0 :     ierr = pio_inq_varid( ncid, 'lon', vid )
          74           0 :     ierr = pio_get_var( ncid, vid, dst_lons  )
          75             :
          76           0 :     ierr = pio_inq_varid( ncid, 'lat', vid )
          77           0 :     ierr = pio_get_var( ncid, vid, dst_lats  )
          78             :
          79           0 :     ierr = pio_inq_varid( ncid, 'mbl_bsn_fct_geo', vid )
          80           0 :     ierr = pio_get_var( ncid, vid, soil_erodibility_in )
          81             :
          82             :     !-----------------------------------------------------------------------
          83             :     !           ... convert to radians and setup regridding
          84             :     !-----------------------------------------------------------------------
          85           0 :     dst_lats(:) = d2r * dst_lats(:)
          86           0 :     dst_lons(:) = d2r * dst_lons(:)
          87             :
          88           0 :     allocate( soil_erodibility(pcols,begchunk:endchunk), stat=ierr )
          89           0 :     if( ierr /= 0 ) then
          90           0 :        write(iulog,*) 'soil_erod_init: failed to allocate soil_erodibility_in, ierr = ',ierr
          91           0 :        call endrun('soil_erod_init: failed to allocate soil_erodibility_in')
          92             :     end if
          93             :
          94             :     !-----------------------------------------------------------------------
          95             :     !           ... regrid ..
          96             :     !-----------------------------------------------------------------------
          97           0 :     do c=begchunk,endchunk
          98           0 :        ncols = get_ncols_p(c)
          99           0 :        call get_rlat_all_p(c, pcols, to_lats)
         100           0 :        call get_rlon_all_p(c, pcols, to_lons)
         101             :
         102           0 :        call lininterp_init(dst_lons, nlon, to_lons, ncols, 2, lon_wgts, zero, twopi)
         103           0 :        call lininterp_init(dst_lats, nlat, to_lats, ncols, 1, lat_wgts)
         104             :
         105           0 :        call lininterp(soil_erodibility_in(:,:), nlon,nlat , soil_erodibility(:,c), ncols, lon_wgts,lat_wgts)
         106             :
         107           0 :        call lininterp_finish(lat_wgts)
         108           0 :        call lininterp_finish(lon_wgts)
         109             :     end do
         110           0 :     deallocate( soil_erodibility_in, stat=ierr )
         111           0 :     if( ierr /= 0 ) then
         112           0 :        write(iulog,*) 'soil_erod_init: failed to deallocate soil_erodibility_in, ierr = ',ierr
         113           0 :        call endrun('soil_erod_init: failed to deallocate soil_erodibility_in')
         114             :     end if
         115             :
         116           0 :     deallocate( dst_lats )
         117           0 :     deallocate( dst_lons )
         118             :
         119           0 :   end  subroutine soil_erod_init
         120             :
         121             : end module soil_erod_mod

Generated by: LCOV version 1.14