LCOV - code coverage report
Current view: | top level - hemco/HEMCO/src/Core - hco_filedata_mod.F90 (source / functions) |  |  | Hit | Total | Coverage
Test: | coverage.info |  | Lines: | 0 | 99 | 0.0 %
Date: | 2025-01-13 21:54:50 |  | Functions: | 0 | 8 | 0.0 %

              Line data    Source code
           1             : !------------------------------------------------------------------------------
           2             : !                   Harmonized Emissions Component (HEMCO)                    !
           3             : !------------------------------------------------------------------------------
           4             : !BOP
           5             : !
           6             : ! !MODULE: hco_filedata_mod.F90
           7             : !
           8             : ! !DESCRIPTION: Module HCO\_Filedata\_Mod contains routines and
           9             : ! variables to handle the HEMCO file data object FileData.
          10             : ! FileData holds all information of source file data, such as file
          11             : ! name, update frequency, temporal resolution, the data array itself,
          12             : ! etc. These values are specified in the HEMCO configuration file. Many
          13             : ! of these attributes are primarily used for reading/updating the data
          14             : ! from file using the HEMCO generic file reading routines. Within an
          15             : ! ESMF environment, these attributes may be obsolete.
          16             : !\\
          17             : !\\
          18             : ! FileData consists of the following elements:
          19             : !
          20             : ! \begin{itemize}
          21             : ! \item ncFile: path and filename to the source file, as specified in
          22             : !       the configuration file.
          23             : ! \item ncPara: file parameter (variable) of interest, as specified in
          24             : !       the configuration file.
          25             : ! \item ncYrs: range of years in the source file, as specified in the
          26             : !       configuration file through the timestamp attribute.
          27             : ! \item ncMts: range of months in the source file, as specified in the
          28             : !       configuration file through the timestamp attribute.
          29             : ! \item ncDys: range of days in the source file, as specified in the
          30             : !       configuration file through the timestamp attribute.
          31             : ! \item ncHrs: range of hours in the source file, as specified in the
          32             : !       configuration file through the timestamp attribute.
          33             : ! \item CycleFlag: determines how to deal with time stamps that do not
          34             : !       correspond to one of the source file time slices. If set to 1,
          35             : !       the closest available time slice (in the past) is used (or the
          36             : !       first available time slice if model time is before first
          37             : !       available time slice). If set to 2, the file data is ignored if
          38             : !       model time is outside of the source file range. If CycleFlag is
          39             : !       set to 3, an error is returned if none of the file time slices
          40             : !       matches the model time.
          41             : ! \item MustFind: if yes, the code returns with an error if no field
          42             : !       can be found for the given simulation time (and according to
          43             : !       the cycle flag and time attribute settings). Only of relevance
          44             : !       for cycle flags range and exact.
          45             : ! \item UpdtFlag: determines the update frequency of the data. This is
          46             : !       currently only used to distinguish containers that are updated
          47             : !       on every time step (always) or according to the frequency
          48             : !       provided in the HEMCO configuration file via attribute 'srcTime'.
          49             : ! \item ncRead: logical denoting whether or not we need to read this
          50             : !       data container. ncRead is set to false for containers whose
          51             : !       data is directly specified in the configuration file. For
          52             : !       internal use only.
          53             : ! \item OrigUnit: original unit of data.
          54             : ! \item ArbDimName: name of additional (arbitrary) file dimension.
          55             : ! \item ArbDimVal : desired value of arbitrary dimension.
          56             : ! \item IsConc: Set to true if data is concentration. Concentration
          57             : !       data will be added to the concentration array instead of the
          58             : !       emission array.
          59             : ! \item IsLocTime: Set to true if data is in local time. Defaults to
          60             : !       false and becomes only true if data is scalar (e.g. uniform
          61             : !       diurnal scale factors), country-specific data (read from
          62             : !       ASCII), or weekdaily data.
          63             : ! \item V3: vector of 3D fields. For 3D-data, this vector will hold
          64             : !       the 3D arrays of all time slices kept in memory (e.g. 24
          65             : !       elements for hourly data).
          66             : ! \item V2: vector of 2D fields. For 2D-data, this vector will hold
          67             : !       the 2D arrays of all time slices kept in memory (e.g. 24
          68             : !       elements for hourly data).
          69             : ! \item tIDx: derived type used for proper indexing of the time slices
          70             : !       in memory. Internal use only.
          71             : ! \item Cover: data coverage on this CPU: 0=no overlap; 1=full overlap;
          72             : !       -1=partial overlap. As determined from the mask regions
          73             : !       specified in the configuration file.
          74             : ! \item SpaceDim: spatial dimension of data array: 1 = spatially uniform
          75             : !       (x=y=z=1); 2 = 2D data (x,y); 3 = 3D data (x,y,z).
          76             : ! \item Levels: handling of vertical levels (3D data only). For internal
          77             : !       use only.
          78             : ! \item nt: time dimension. length of vector V3 or V2. For internal use
          79             : !       only.
          80             : ! \item DeltaT: time interval between time slices. For internal use only.
          81             : !       ID i (e.g. cIDList(3) points to data-container w/ cID = 3).
          82             : ! \item DoShare: will be set to True if this file data object is shared
          83             : !       by multiple data containers. For internal use only.
          84             : ! \item IsInList: will be set to True if this file data object is part
          85             : !       of the emissions list EmisList. For internal use only.
          86             : ! \item IsTouched: will be set to True as soon as the container becomes
          87             : !       touched for the first time. For internal use only.
          88             : ! \end{itemize}
          89             : !
          90             : ! !INTERFACE:
          91             : !
          92             : MODULE HCO_FileData_Mod
          93             : !
          94             : ! !USES:
          95             : !
          96             :   USE HCO_TYPES_MOD
          97             :   USE HCO_ERROR_MOD
          98             :   USE HCO_ARR_MOD
          99             :
         100             :   IMPLICIT NONE
         101             :   PRIVATE
         102             : !
         103             : ! !PUBLIC MEMBER FUNCTIONS:
         104             : !
         105             :   PUBLIC  :: FileData_Init
         106             :   PUBLIC  :: FileData_Cleanup
         107             :   PUBLIC  :: FileData_ArrCheck
         108             :   PUBLIC  :: FileData_ArrIsDefined
         109             :   PUBLIC  :: FileData_ArrIsTouched
         110             :   PUBLIC  :: FileData_ArrInit
         111             : !
         112             : ! !PRIVATE MEMBER FUNCTIONS:
         113             : !
         114             :   PRIVATE :: FileData_ArrCheck2D
         115             :   PRIVATE :: FileData_ArrCheck3D
         116             : !
         117             : ! !REVISION HISTORY:
         118             : !  19 Dec 2013 - C. Keller   - Initialization
         119             : !  See https://github.com/geoschem/hemco for complete history
         120             : !EOP
         121             : !------------------------------------------------------------------------------
         122             : !BOC
         123             : !
         124             : ! !PRIVATE TYPES:
         125             : !
         126             : !
         127             : ! !INTERFACES:
         128             : !
         129             :   INTERFACE FileData_ArrCheck
         130             :      MODULE PROCEDURE FileData_ArrCheck2D
         131             :      MODULE PROCEDURE FileData_ArrCheck3D
         132             :   END INTERFACE FileData_ArrCheck
         133             :
         134             :   INTERFACE FileData_ArrInit
         135             :      MODULE PROCEDURE FileData_ArrInit2D
         136             :      MODULE PROCEDURE FileData_ArrInit3D
         137             :   END INTERFACE FileData_ArrInit
         138             :
         139             : CONTAINS
         140             : !EOC
         141             : !------------------------------------------------------------------------------
         142             : !                   Harmonized Emissions Component (HEMCO)                    !
         143             : !------------------------------------------------------------------------------
         144             : !BOP
         145             : !
         146             : ! !IROUTINE: FileData_Init
         147             : !
         148             : ! !DESCRIPTION: Subroutine FileData\_Init initializes a new (blank) file
         149             : ! data object.
         150             : !\\
         151             : !\\
         152             : ! !INTERFACE:
         153             : !
         154           0 :   SUBROUTINE FileData_Init( FileDta )
         155             : !
         156             : ! !INPUT PARAMETERS:
         157             : !
         158             :     TYPE(FileData), POINTER    :: FileDta
         159             : !
         160             : ! !REVISION HISTORY:
         161             : !  19 Dec 2013 - C. Keller   - Initialization
         162             : !  See https://github.com/geoschem/hemco for complete history
         163             : !EOP
         164             : !------------------------------------------------------------------------------
         165             : !BOC
         166             : !
         167             : ! !LOCAL VARIABLES:
         168             : !
         169             :     !======================================================================
         170             :     ! FileData_Init begins here!
         171             :     !======================================================================
         172             :
         173             :     ! Allocate memory to the FileData object
         174           0 :     ALLOCATE( FileDta )
         175             :
         176             :     ! Nullify all pointers and initialize variables
         177           0 :     FileDta%V3          => NULL()
         178           0 :     FileDta%V2          => NULL()
         179           0 :     FileDta%tIDx        => NULL()
         180           0 :     FileDta%ncFile       = ''
         181           0 :     FileDta%ncPara       = ''
         182           0 :     FileDta%ncYrs(:)     = -999
         183           0 :     FileDta%ncMts(:)     = -999
         184           0 :     FileDta%ncDys(:)     = -999
         185           0 :     FileDta%ncHrs(:)     = -999
         186           0 :     FileDta%tShift(:)    = 0
         187           0 :     FileDta%CycleFlag    = HCO_CFLAG_CYCLE
         188           0 :     FileDta%UpdtFlag     = HCO_UFLAG_FROMFILE
         189           0 :     FileDta%MustFind     = .FALSE.
         190           0 :     FileDta%ncRead       = .TRUE.
         191           0 :     FileDta%Cover        = -999
         192           0 :     FileDta%DeltaT       = 0
         193           0 :     FileDta%nt           = 0
         194           0 :     FileDta%SpaceDim     = -1
         195           0 :     FileDta%Levels       = 0
         196           0 :     FileDta%EmisL1       = 1.0_hp
         197           0 :     FileDta%EmisL2       = 1.0_hp
         198           0 :     FileDta%EmisL1Unit   = HCO_EMISL_LEV
         199           0 :     FileDta%EmisL2Unit   = HCO_EMISL_LEV
         200           0 :     FileDta%OrigUnit     = ''
         201           0 :     FileDta%ArbDimName   = 'none'
         202           0 :     FileDta%ArbDimVal    = ''
         203           0 :     FileDta%IsLocTime    = .FALSE.
         204           0 :     FileDta%IsConc       = .FALSE.
         205           0 :     FileDta%DoShare      = .FALSE.
         206           0 :     FileDta%IsInList     = .FALSE.
         207           0 :     FileDta%IsTouched    = .FALSE.
         208             :
         209           0 :   END SUBROUTINE FileData_Init
         210             : !EOC
         211             : !------------------------------------------------------------------------------
         212             : !                   Harmonized Emissions Component (HEMCO)                    !
         213             : !------------------------------------------------------------------------------
         214             : !BOP
         215             : !
         216             : ! !IROUTINE: FileData_Cleanup
         217             : !
         218             : ! !DESCRIPTION: Subroutine FileData\_Cleanup cleans up the file data object
         219             : ! FileDta. If DeepClean is set to False, only the data arrays will be removed.
         220             : !\\
         221             : !\\
         222             : ! !INTERFACE:
         223             : !
         224           0 :   SUBROUTINE FileData_Cleanup( FileDta, DeepClean )
         225             : !
         226             : ! !INPUT PARAMETERS:
         227             : !
         228             :     TYPE(FileData), POINTER    :: FileDta
         229             :     LOGICAL,        INTENT(IN) :: DeepClean
         230             : !
         231             : ! !REVISION HISTORY:
         232             : !  19 Dec 2013 - C. Keller: Initialization
         233             : !  See https://github.com/geoschem/hemco for complete history
         234             : !EOP
         235             : !------------------------------------------------------------------------------
         236             : !BOC
         237             : !
         238             : ! !LOCAL VARIABLES:
         239             : !
         240             :     INTEGER :: I
         241             :
         242             :     !======================================================================
         243             :     ! FileData_Cleanup begins here!
         244             :     !======================================================================
         245           0 :     IF ( ASSOCIATED( FileDta ) ) THEN
         246             :
         247             :        ! Deallocate data arrays
         248           0 :        CALL HCO_ArrCleanup( FileDta%V3, DeepClean )
         249           0 :        CALL HCO_ArrCleanup( FileDta%V2, DeepClean )
         250           0 :        FileDta%nt = 0
         251             :
         252           0 :        IF ( DeepClean ) THEN
         253           0 :           FileDta%tIDx => NULL()
         254           0 :           DEALLOCATE ( FileDta )
         255             :           FileDta => NULL()
         256             :        ENDIF
         257             :     ENDIF
         258             :
         259           0 :   END SUBROUTINE FileData_Cleanup
         260             : !EOC
         261             : !------------------------------------------------------------------------------
         262             : !                   Harmonized Emissions Component (HEMCO)                    !
         263             : !------------------------------------------------------------------------------
         264             : !BOP
         265             : !
         266             : ! !IROUTINE: FileData_ArrCheck2D
         267             : !
         268             : ! !DESCRIPTION: Subroutine FileData\_ArrCheck2D allocates the 2D data array
         269             : ! vector of the given file data object if it is not yet allocated. If already
         270             : ! allocated, it compares the array dimensions against the passed dimensions.
         271             : !\\
         272             : !\\
         273             : ! !INTERFACE:
         274             : !
         275           0 :   SUBROUTINE FileData_ArrCheck2D( HcoConfig, FileDta, nx, ny, nt, RC )
         276             : !
         277             : ! !INPUT PARAMETERS:
         278             : !
         279             :     TYPE(ConfigObj),POINTER       :: HcoConfig ! HEMCO config object
         280             :     TYPE(FileData), POINTER       :: FileDta   ! file data object
         281             :     INTEGER,        INTENT(IN)    :: nx        ! x-dim
         282             :     INTEGER,        INTENT(IN)    :: ny        ! y-dim
         283             :     INTEGER,        INTENT(IN)    :: nt        ! time dim => vector length
         284             : !
         285             : ! !INPUT/OUTPUT PARAMETERS:
         286             : !
         287             :     INTEGER,        INTENT(INOUT) :: RC        ! Return code
         288             : !
         289             : ! !REVISION HISTORY:
         290             : !  20 Apr 2013 - C. Keller - Initial version
         291             : !  See https://github.com/geoschem/hemco for complete history
         292             : !EOP
         293             : !------------------------------------------------------------------------------
         294             : !BOC
         295             : !
         296             : ! !LOCAL VARIABLES:
         297             : !
         298             :     INTEGER            :: I, AS
         299             :     CHARACTER(LEN=255) :: MSG, LOC
         300             :
         301             :     ! ================================================================
         302             :     ! FileData_ArrCheck2D begins here
         303             :     ! ================================================================
         304           0 :     LOC = 'FileData_ArrCheck2D (HCO_FILEDATA_MOD.F90)'
         305             :
         306             :     ! Assume success until otherwise
         307           0 :     RC = HCO_SUCCESS
         308             :
         309             :     ! Compare dimensions if array already allocated
         310           0 :     IF ( ASSOCIATED(FileDta%V2) ) THEN
         311             :        IF ( (               FileDta%nt  /= nt ) .OR. &
         312           0 :             ( SIZE(FileDta%V2(1)%Val,1) /= nx ) .OR. &
         313             :             ( SIZE(FileDta%V2(1)%Val,2) /= ny )       ) THEN
         314           0 :           MSG = 'Wrong dimensions: ' // TRIM(FileDta%ncFile)
         315           0 :           CALL HCO_ERROR ( MSG, RC )
         316             :        ENDIF
         317           0 :        RETURN
         318             :     ENDIF
         319             :
         320             :     ! If not associated yet:
         321             :     ! Initialize vector and corresponding arrays.
         322           0 :     CALL FileData_ArrInit ( FileDta, nt, nx, ny, RC )
         323           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         324           0 :         CALL HCO_ERROR( 'ERROR 0', RC, THISLOC=LOC )
         325           0 :         RETURN
         326             :     ENDIF
         327             :
         328             :   END SUBROUTINE FileData_ArrCheck2D
         329             : !EOC
         330             : !------------------------------------------------------------------------------
         331             : !                   Harmonized Emissions Component (HEMCO)                    !
         332             : !------------------------------------------------------------------------------
         333             : !BOP
         334             : !
         335             : ! !IROUTINE: FileData_ArrCheck3D
         336             : !
         337             : ! !DESCRIPTION: Subroutine FileData\_ArrCheck3D allocates the 3D data array
         338             : ! vector of the given file data object if it is not yet allocated. If already
         339             : ! allocated, it compares the array dimensions against the passed dimensions.
         340             : !\\
         341             : !\\
         342             : ! !INTERFACE:
         343             : !
         344           0 :   SUBROUTINE FileData_ArrCheck3D( HcoConfig, FileDta, nx, ny, nz, nt, RC )
         345             : !
         346             : ! !USES:
         347             : !
         348             : !
         349             : ! !INPUT PARAMETERS:
         350             : !
         351             :     TYPE(ConfigObj),POINTER       :: HcoConfig ! HEMCO config object
         352             :     TYPE(FileData), POINTER       :: FileDta  ! Container
         353             :     INTEGER,        INTENT(IN)    :: nx        ! x-dim
         354             :     INTEGER,        INTENT(IN)    :: ny        ! y-dim
         355             :     INTEGER,        INTENT(IN)    :: nz        ! z-dim
         356             :     INTEGER,        INTENT(IN)    :: nt        ! Time dim => vector length
         357             : !
         358             : ! !INPUT/OUTPUT PARAMETERS:
         359             : !
         360             :     INTEGER,        INTENT(INOUT) :: RC        ! Return code
         361             : !
         362             : ! !REVISION HISTORY:
         363             : !  20 Apr 2013 - C. Keller - Initial version
         364             : !  See https://github.com/geoschem/hemco for complete history
         365             : !EOP
         366             : !------------------------------------------------------------------------------
         367             : !BOC
         368             : !
         369             : ! !LOCAL VARIABLES:
         370             : !
         371             :     INTEGER            :: I, AS
         372             :     CHARACTER(LEN=255) :: MSG, LOC
         373             :
         374             :     ! ================================================================
         375             :     ! FileData_ArrCheck3D begins here
         376             :     ! ================================================================
         377           0 :     LOC = 'FileData_ArrCheck3D (HCO_FILEDATA_MOD.F90)'
         378             :
         379             :     ! Assume success until otherwise
         380           0 :     RC = HCO_SUCCESS
         381             :
         382             :     ! Compare dimensions if array already allocated
         383           0 :     IF ( Associated(FileDta%V3) ) THEN
         384             :        IF ( (                FileDta%nt /= nt ) .OR. &
         385           0 :             ( SIZE(FileDta%V3(1)%Val,1) /= nx ) .OR. &
         386           0 :             ( SIZE(FileDta%V3(1)%Val,2) /= ny ) .OR. &
         387             :             ( SIZE(FileDta%V3(1)%Val,3) /= nz )       ) THEN
         388           0 :           MSG = 'Wrong dimensions: ' // TRIM(FileDta%ncFile)
         389           0 :           CALL HCO_ERROR ( MSG, RC )
         390             :        ENDIF
         391           0 :        RETURN
         392             :     ENDIF
         393             :
         394             :     ! If not associated yet:
         395             :     ! Initialize vector and corresponding arrays.
         396           0 :     CALL FileData_ArrInit( FileDta, nt, nx, ny, nz, RC )
         397           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         398           0 :         CALL HCO_ERROR( 'ERROR 1', RC, THISLOC=LOC )
         399           0 :         RETURN
         400             :     ENDIF
         401             :
         402             :   END SUBROUTINE FileData_ArrCheck3D
         403             : !EOC
         404             : !------------------------------------------------------------------------------
         405             : !                   Harmonized Emissions Component (HEMCO)                    !
         406             : !------------------------------------------------------------------------------
         407             : !BOP
         408             : !
         409             : ! !IROUTINE: FileData_ArrIsDefined
         410             : !
         411             : ! !DESCRIPTION: Function FileData\_ArrIsDefined returns true if the data
         412             : ! array of the given file data object is defined.
         413             : !\\
         414             : !\\
         415             : ! !INTERFACE:
         416             : !
         417           0 :   FUNCTION FileData_ArrIsDefined( FileDta ) RESULT( IsDefined )
         418             : !
         419             : ! !INPUT PARAMETERS:
         420             : !
         421             :     TYPE(FileData), POINTER :: FileDta  ! Container
         422             : !
         423             : ! !RETURN VALUE:
         424             : !
         425             :     LOGICAL                 :: IsDefined
         426             : !
         427             : ! !REVISION HISTORY:
         428             : !  20 Apr 2013 - C. Keller - Initial version
         429             : !  See https://github.com/geoschem/hemco for complete history
         430             : !EOP
         431             : !------------------------------------------------------------------------------
         432             : !BOC
         433             :
         434             :     ! ================================================================
         435             :     ! FileData_ArrIsDefined begins here
         436             :     ! ================================================================
         437             :
         438             :     ! Init
         439           0 :     IsDefined = .FALSE.
         440             :
         441             :     ! Return here if passed FileDta object is not defined
         442           0 :     IF ( .NOT. ASSOCIATED( FileDta ) ) RETURN
         443             :
         444             :     ! nt must be larger than zero!
         445           0 :     IF ( FileDta%nt <= 0 ) Return
         446             :
         447             :     ! 2D array
         448           0 :     IF ( (FileDta%SpaceDim<=2) .AND. ASSOCIATED(FileDta%V2) ) THEN
         449           0 :        IsDefined = .TRUE.
         450             :     ENDIF
         451             :
         452             :     ! 3D array
         453           0 :     IF ( (FileDta%SpaceDim==3) .AND. ASSOCIATED(FileDta%V3) ) THEN
         454           0 :        IsDefined = .TRUE.
         455             :     ENDIF
         456             :
         457             :   END FUNCTION FileData_ArrIsDefined
         458             : !EOC
         459             : !------------------------------------------------------------------------------
         460             : !                   Harmonized Emissions Component (HEMCO)                    !
         461             : !------------------------------------------------------------------------------
         462             : !BOP
         463             : !
         464             : ! !IROUTINE: FileData_ArrIsTouched
         465             : !
         466             : ! !DESCRIPTION: Function FileData\_ArrIsTouched returns true if the data
         467             : ! array of the given file data object has already been touched, e.g. if
         468             : ! the data has already been read (or at least attempted to being read).
         469             : ! This information is mostly important for file data objects that are shared
         470             : ! by multiple data containers. See ReadList\_Fill in hco\_readlist\_mod.F90
         471             : ! for more details.
         472             : !\\
         473             : !\\
         474             : ! !INTERFACE:
         475             : !
         476           0 :   FUNCTION FileData_ArrIsTouched( FileDta ) RESULT( IsTouched )
         477             : !
         478             : ! !INPUT PARAMETERS:
         479             : !
         480             :     TYPE(FileData), POINTER :: FileDta  ! Container
         481             : !
         482             : ! !RETURN VALUE:
         483             : !
         484             :     LOGICAL                 :: IsTouched
         485             : !
         486             : ! !REVISION HISTORY:
         487             : !  17 Mar 2015 - C. Keller - Initial version
         488             : !  See https://github.com/geoschem/hemco for complete history
         489             : !EOP
         490             : !------------------------------------------------------------------------------
         491             : !BOC
         492             :
         493             :     ! ================================================================
         494             :     ! FileData_ArrIsTouched begins here
         495             :     ! ================================================================
         496             :
         497             :     ! Init
         498           0 :     IsTouched = .FALSE.
         499             :
         500             :     ! Return touched flag
         501           0 :     IF ( ASSOCIATED( FileDta ) ) THEN
         502           0 :        IsTouched = FileDta%IsTouched
         503             :     ENDIF
         504             :
         505             :
         506           0 :   END FUNCTION FileData_ArrIsTouched
         507             : !EOC
         508             : !------------------------------------------------------------------------------
         509             : !                   Harmonized Emissions Component (HEMCO)                    !
         510             : !------------------------------------------------------------------------------
         511             : !BOP
         512             : !
         513             : ! !IROUTINE: FileData_ArrInit2D
         514             : !
         515             : ! !DESCRIPTION: Subroutine FileData\_ArrInit2D is a wrapper routine
         516             : ! to initialize 2D data arrays of a file data object. To ensure proper
         517             : ! functioning of the file data object and related routines, this routine
         518             : ! should always be used to initialize file data arrays (and NOT HCO\_ArrInit
         519             : ! directly!).
         520             : !\\
         521             : !\\
         522             : ! !INTERFACE:
         523             : !
         524           0 :   SUBROUTINE FileData_ArrInit2D( FileDta, nt, nx, ny, RC )
         525             : !
         526             : ! !USES:
         527             : !
         528             : !
         529             : ! !INPUT PARAMETERS:
         530             : !
         531             :     TYPE(FileData), POINTER       :: FileDta  ! Container
         532             :     INTEGER,        INTENT(IN)    :: nt        ! Time dim => vector length
         533             :     INTEGER,        INTENT(IN)    :: nx        ! x-dim
         534             :     INTEGER,        INTENT(IN)    :: ny        ! y-dim
         535             : !
         536             : ! !INPUT/OUTPUT PARAMETERS:
         537             : !
         538             :     INTEGER,        INTENT(INOUT) :: RC        ! Return code
         539             : !
         540             : ! !REVISION HISTORY:
         541             : !  01 Oct 2014 - C. Keller - Initial version
         542             : !  See https://github.com/geoschem/hemco for complete history
         543             : !EOP
         544             : !------------------------------------------------------------------------------
         545             : !BOC
         546             : !
         547             : ! !LOCAL VARIABLES:
         548             : !
         549             :     CHARACTER(LEN=255)  :: LOC
         550             :     ! ================================================================
         551             :     ! FileData_ArrInit2D begins here
         552             :     ! ================================================================
         553           0 :     LOC = 'FileData_ArrInit2D (HCO_FILEDATA_MOD.F90)'
         554             :
         555             :     ! Assume success until otherwise
         556           0 :     RC = HCO_SUCCESS
         557             :
         558             :     ! Initialize vector and corresponding arrays.
         559           0 :     CALL HCO_ArrInit( FileDta%V2, nt, nx, ny, RC )
         560           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         561           0 :         CALL HCO_ERROR( 'ERROR 2', RC, THISLOC=LOC )
         562           0 :         RETURN
         563             :     ENDIF
         564             :
         565             :     ! Update nt
         566           0 :     FileDta%nt = nt
         567             :
         568             :     ! Return w/ success
         569           0 :     RC = HCO_SUCCESS
         570             :
         571             :   END SUBROUTINE FileData_ArrInit2D
         572             : !EOC
         573             : !------------------------------------------------------------------------------
         574             : !                   Harmonized Emissions Component (HEMCO)                    !
         575             : !------------------------------------------------------------------------------
         576             : !BOP
         577             : !
         578             : ! !IROUTINE: FileData_ArrInit3D
         579             : !
         580             : ! !DESCRIPTION: Subroutine FileData\_ArrInit3D is a wrapper routine
         581             : ! to initialize 3D data arrays of a file data object. To ensure proper
         582             : ! functioning of the file data object and related routines, this routine
         583             : ! should always be used to initialize file data arrays (and NOT HCO\_ArrInit
         584             : ! directly!).
         585             : !\\
         586             : !\\
         587             : ! !INTERFACE:
         588             : !
         589           0 :   SUBROUTINE FileData_ArrInit3D( FileDta, nt, nx, ny, nz, RC )
         590             : !
         591             : ! !USES:
         592             : !
         593             : !
         594             : ! !INPUT PARAMETERS:
         595             : !
         596             :     TYPE(FileData), POINTER       :: FileDta  ! Container
         597             :     INTEGER,        INTENT(IN)    :: nt        ! Time dim => vector length
         598             :     INTEGER,        INTENT(IN)    :: nx        ! x-dim
         599             :     INTEGER,        INTENT(IN)    :: ny        ! y-dim
         600             :     INTEGER,        INTENT(IN)    :: nz        ! z-dim
         601             : !
         602             : ! !INPUT/OUTPUT PARAMETERS:
         603             : !
         604             :     INTEGER,        INTENT(INOUT) :: RC        ! Return code
         605             : !
         606             : ! !REVISION HISTORY:
         607             : !  20 Apr 2013 - C. Keller - Initial version
         608             : !  See https://github.com/geoschem/hemco for complete history
         609             : !EOP
         610             : !------------------------------------------------------------------------------
         611             : !BOC
         612             : !
         613             : ! !LOCAL VARIABLES:
         614             : !
         615             :     CHARACTER(LEN=255)  :: LOC
         616             :     ! ================================================================
         617             :     ! FileData_ArrInit3D begins here
         618             :     ! ================================================================
         619           0 :     LOC = 'FileData_ArrInit3D (HCO_FILEDATA_MOD.F90)'
         620             :
         621             :     ! Assume success until otherwise
         622           0 :     RC = HCO_SUCCESS
         623             :
         624             :     ! Initialize vector and corresponding arrays.
         625           0 :     CALL HCO_ArrInit( FileDta%V3, nt, nx, ny, nz, RC )
         626           0 :     IF ( RC /= HCO_SUCCESS ) THEN
         627           0 :         CALL HCO_ERROR( 'ERROR 3', RC, THISLOC=LOC )
         628           0 :         RETURN
         629             :     ENDIF
         630             :
         631             :     ! Update nt
         632           0 :     FileDta%nt = nt
         633             :
         634             :     ! Return w/ success
         635           0 :     RC = HCO_SUCCESS
         636             :
         637             :   END SUBROUTINE FileData_ArrInit3D
         638             : !EOC
         639             : END MODULE HCO_FileData_Mod

Generated by: LCOV version 1.14